contrail performance guide

2020-05-29

March 04th, 2020 - v3.2

|  |  |
| --- | --- |
| v1 | First version |
| v2 | Updates: Page 14 (X710 NIC) and 52 (Problem with re assigning kernel driver back to interface when DPDK vRouter is stopped). |
| v2.1 | Add description of vif command counters (July 2018) |
| v2.2 | various changes: coremask for dpdk changed. vrouter logical cores numbering description. |
| v2.3 | New appendix section with DPDK fine tuning for Intel NIC cards (Niantic and Fortville family). |
| v2.4 | More details on DPDK |
| v2.5 | Document rearrangement. Some updates on vrouter fine tuning options. |
| v2.6 | Document rearrangement. More details about virtio. |
| v3.0 | Performance tuning which will be available in 20.03 release. |
| v3.0.2 | Added details of DPDK packet flow and polling core assignment as of R1910. |
| v3.0,3 | Performance tuning parameters which will be available in 20.03 update |
| v3.1 | Details about vNIC and MultiQueues - Control Thread new parameter (20.03 release). |
| 3.1.1 | Compute nodes and CPU capacity planning |
| 3.2 | Configurations description and deployment considerations sections rearrangement |

# **DPDK fundamentals**

## Performance requirements for packet processing

Ethernet minimum frame size is 64 Bytes. When Ethernet frames are sent onto the wire, Inter Frame Gap and Preamble bits are added. Minimum size of Ethernet frames on the physical layer is 84 Bytes (672 bits).

![image](data:image/png;base64;base64,)

For a 10 Gbit/s interface, the number of frames per seconds can reach up to 14.88 Mpps for traffic using the smallest Ethernet frame size. It means a new frame will have to be forwarded each 67 ns.

A CPU running at 2Ghz has a 0.5 ns cycle. Such a CPU has a budget of only 134 cycles per packet to be able to process a flow of 10 Gb/s.

Generic Linux Ethernet drivers are not performant enough to be able to process such a 10Gb/s packet flow.

Indeed lots of times are required to :

* perform packet processing in Linux Kernel using interrupt mechanism,
* transfer application data from host memory to Network Interface card

A SDN solution like Contrail needs to use specific setup and mechanisms in order to be able to process network flows onto a generic x86 platform at a high rate.

## kvm, QEMU and Virtio

*Kernel-based Virtual Machine (KVM) is an open source virtualization technology built into Linux. It provides hardware assist to the virtualization software, using built-in CPU virtualization technology to reduce virtualization overheads (cache, I/O, memory) and improving security.*

*QEMU is a hosted virtual machine emulator that provides a set of different hardware and device models for the guest machine. For the host, qemu appears as a regular process scheduled by the standard Linux scheduler, with its own process memory. In the process, QEMU allocates a memory region that the guest see as physical, and executes the virtual machine’s CPU instructions.*

*With KVM, QEMU can just create a virtual machine with virtual CPUs (vCPUs) that the processor is aware of, that runs native-speed instructions. When a special instruction is reached by KVM, like the ones that interacts with the devices or to special memory regions, vCPU pauses and informs QEMU of the cause of pause, allowing hypervisor to react to that event.*

*Virtio is an open specification for virtual machines' data I/O communication, offering a straightforward, efficient, standard and extensible mechanism for virtual devices, rather than boutique per-environment or per-OS mechanisms. It uses the fact that the guest can share memory with the host for I/O to implement that.*

Virtio was developed as a standardized open interface for virtual machines (VMs) to access simplified devices such as block devices and network adaptors.

There are two parts to networking within VirtIO:

* the virtual network device that is provided to the guest (e.g. a PCI network card).
* the network backend that interacts with the emulated NIC (e.g. puts packets onto the host’s network, to the vrouter).

In Contrail Networking, VirtIO is used to connect with guest VM vNIC onto the vrouter vif interface.

When we talk about the virtio interface we have a backend component and a frontend component:

* The backend component is the host side of the virtio interface
* The frontend component is the guest side of the virtio interface

In the vhost-net/virtio-net architecture the components are as follows:

* vhost-net is the backend running in the host kernel space
* virtio-net is the frontend running in the guest kernel space

The following diagram shows how virtio backend and frontend are mapped to the big picture:

![2019 09 10 virtio intro fig2](data:image/jpg;base64;base64,)

In the diagram below you have a detailed view of a Virtual instance connectivity with a Kernel mode vrouter :

![image](data:image/png;base64;base64,)

For more information on VirtIO :

* <https://www.redhat.com/en/blog/introduction-virtio-networking-and-vhost-net>
* <https://www.redhat.com/en/blog/deep-dive-virtio-networking-and-vhost-net>

## Non-Uniform Memory Access (NUMA) systems

A traditional server has a single CPU, a single RAM and a single RAM controller.

A RAM can be made of several DIMM banks in several sockets, all being associated to the CPU. When the CPU needs access to data in RAM, it requests it to its RAM controller.

Recent servers can have multiple CPUs, each one having its own RAM and its own RAM controller. Such systems are called NUMA systems, or Non-Uniform Memory Access. For example, in a server with 2 CPUs, each one can be a separate NUMA: NUMA0 and NUMA1.

![NUMA nodes architecture.](data:image/jpg;base64;base64,)

NUMA nodes architecture.

* **In green**: CPU core accessing a memory item located in its own NUMA’s RAM controller, showing minimum latency.
* **In red**: CPU core accessing a memory item located in the other NUMA through the QPI (Quick Path Interconnect) path and the remote RAM controller, showing a higher latency.

When CPU0 needs to access data located in RAM0, it will go through its local RAM controller 0. Same thing happens for CPU1.

When CPU0 needs to access data located in the other RAM1, the first (local) controller 0 has to go through the second (or remote) RAM controller 1 which will access the (remote) data in RAM 1. Data will use an internal connection between the 2 CPUs called QPI, or Quick Path Interconnect, which is typically of a high enough capacity to avoid being a bottleneck, typically 1 or 2 times 25GBps (400 Gbps). For example the Intel Xeon E5 has 2 CPUs with 2 QPI links between them; Intel Xeon E7 has 4 CPUs, with a single QPI between pairs of CPUs.

The fastest RAM that the CPU has access to is the register, which is inside the CPU and reserved to it.

Beyond the register, the CPU has access to cached memory, which is a special memory based on higher performance hardware.

Cached memory are shared between the cores of a single CPU. Typical characteristics of memory cache are:

* Accessing a Level 1 cache takes 7 CPU cycles (with a size of 64KB or 128KB).
* Accessing a Level 2 cache takes 11 CPU cycles (with a size of 1MB).
* Accessing a Level 3 cache takes 30 CPU cycles (with a larger size).

If the CPU needs to access data that is in the main RAM, it has to use its RAM controller.

Access to RAM takes then typically 170 CPU cycles (the green line in the diagram). Access to the remote RAM through the remote RAM controller typically adds 200 cycles (the red line in the diagram), meaning RAM latency is roughly doubled.

When data needed by the CPU is located both in the local and in the remote RAM with no particular structure, latency to access data can be unpredictable and unstable.

## Hyper-threading (HT)

A single physical CPU core with hyper-threading appears as two logical CPUs to an operating system.

While the operating system sees two CPUs for each core, the actual CPU hardware only has a single set of execution resources for each core.

Hyper-threading allows the two logical CPU cores to share physical execution resources.

The sharing of resources allows two logical processors to work with each other more efficiently, and allows a logical processor to borrow resources from a stalled logical core (assuming both logical cores are associated with the same physical core). Hyper-threading can help speed processing up, but it’s nowhere near as good as having actual additional cores.

The performance of vRouter with ***sibling*** HT cores can increase by 10% to 20% (result is based on performance tests described hereinafter).

## Huge pages

Memory is managed in blocks known as pages. On most systems, a page is 4Ki. 1Mi of memory is equal to 256 pages; 1Gi of memory is 256,000 pages, etc. CPUs have a built-in memory management unit that manages a list of these pages in hardware.

The Translation Lookaside Buffer (TLB) is a small hardware cache of virtual-to-physical page mappings. If the virtual address passed in a hardware instruction can be found in the TLB, the mapping can be determined quickly. If not, a TLB miss occurs, and the system falls back to slower, software based address translation. This results in performance issues. Since the size of the TLB is fixed, the only way to reduce the chance of a TLB miss is to increase the page size.

Virtual memory address lookup slows down when the number of entries increases.

A huge page is a memory page that is larger than 4Ki. In x86\_64 architecture, in addition to **standard 4KB memory** page size, two larger page sizes are available: **2MB** and **1GB**.

Contrail DPDK vrouter can use both or only one huge page size.

## what is DPDK

Data Plane Development Kit (DPDK) is a set of data plane libraries and network interface controller drivers for fast packet processing, currently managed as an open-source project under the Linux Foundation.

![image](data:image/png;base64;base64,)

The main goal of the DPDK is to provide a simple, complete framework for fast packet processing in data plane applications.

The framework creates a set of libraries for specific environments through the creation of an Environment Abstraction Layer (EAL), which may be specific to a mode of the Intel® architecture (32-bit or 64-bit), Linux\* user space compilers or a specific platform.

These environments are created through the use of make files and configuration files. Once the EAL library is created, the user may link with the library to create their own applications.

The DPDK implements a "run to completion model" for packet processing, where all resources must be allocated prior to calling Data Plane applications, running as execution units on logical processing cores.

The model does not support a scheduler and all devices are accessed by polling. The primary reason for not using interrupts is the performance overhead imposed by interrupt processing.

For more information please refer to dpdk.org documents <http://dpdk.org/doc/guides/prog_guide/index.html>

## DPDK memory management

With DPDK there is a direct link between application data stored in host memory and the NIC memory used to transfer data onto the wire :

![image](data:image/png;base64;base64,)

DPDK uses message buffers known as mbufs to store packet data into the host memory. These mbufs are stored in memory pools known as mempools. Mempools are set up as a ring, which creates a pool with a configuration similar to a first-in, first-out (FIFO) system.

![image](data:image/png;base64;base64,)

Rings descriptors are managing data storage into mempools. The more descriptors RX/TX rings are containing, the more memory size will be required in each mempool to store data.

![image](data:image/png;base64;base64,)

The Host OS exchanges packets with the NIC through the so called rings. A ring is a circular array of descriptors allocated by the OS in the system memory (RAM). Each descriptor contains information about a packet that has been received or that is going to be transmitted.

"ring" = "descriptor", seems like located on both cores or NIC? also see [vrouter DPDK fine tuning parameters](#X30e96fc6b25b2ee4f8f5f5a389f298b4226cb1a)

answer: Ring is a set of memory pointers (descriptors). These pointers are pointing the real memory area in which the data to be processed (packets) are stored.

There are 2 rings per “queues” (1 per direction:. 1 RX ring, 1 TX ring).

Data are stored in compute central memory (in huge page area). Packets are not moved from one queue to another, but these are descriptors (pointers) that are moving from one queue to another.

**RX ring**

RX ring is managing Data transfer from NIC memory to host memory :

![image](data:image/png;base64;base64,)

Synchronization between the OS and the NIC happens through two registers, whose content is interpreted as an index in the RX ring:

* Receive Descriptor Head (RDH): indicates the first descriptor prepared by the OS that can be used by the NIC to store the next incoming packet.
* Receive Descriptor Tail (RDT): indicates the position to stop reception, i.e. the first descriptor that is not ready to be used by the NIC.

**TX ring**

TX ring is managing data transfer from host memory to NIC memory :

![image](data:image/png;base64;base64,)

Synchronization between the host OS and the NIC happens through two registers, whose content is interpreted as an index in the TX ring:

* Transmit Descriptor Head (TDH): indicates the first descriptor that has been prepared by the OS and has to be transmitted on the wire.
* Transmit Descriptor Tail (TDT): indicates the position to stop transmission, i.e. the first descriptor that is not ready to be transmitted, and that will be the next to be prepared.


**DMA**

Direct Memory Access (DMA) allows PCI devices to read (write) data from (to) memory without CPU intervention. This is a fundamental requirement for high performance devices.

## DPDK and Poll Mode Drivers (PMD)

When DPDK is used, Network interfaces are no more managed in Kernel space. Legacy NIC driver which is usually used to manage the NIC has to be replaced by a new driver which is able to run into user space. This new drive, called **Poll Mode Driver (PMD)** will be used to manage the network interface into user space with the DPDK library.

A Poll Mode Driver consists of APIs, provided through the BSD driver running in user space, to configure the devices and their respective queues. In addition, a PMD accesses the RX and TX descriptors directly without any interrupts (with the exception of Link Status Change interrupts) to quickly receive, process and deliver packets in the user’s application.



NIC access path: dpdk vs kernel

* PMD used to manage physical interfaces :
  + I40e PMD for Intel X710/XL710/X722 10/40 Gbps family of adapters <http://dpdk.org/doc/guides/nics/i40e.html>
  + IXGBE PMD <http://dpdk.org/doc/guides/nics/ixgbe.html>
  + Linux bonding PMD <http://dpdk.org/doc/guides/prog_guide/link_bonding_poll_mode_drv_lib.html>
* PMD used to manage virtual interfaces :
  + Virtio PMD <http://dpdk.org/doc/guides/nics/virtio.html>

ping? "PMD user space process" vs. "pmd kernel drivers" <https://github.com/pinggit/dpdk-contrail-book/issues/1#issue-625774372>

## Linux drivers for PMD

In Linux user space environment, the DPDK application runs as a user-space application using the pthread library.

PCI information about devices and address space is discovered through the /sys kernel interface and through kernel modules such as:

* uio\_pci\_generic,
* igb\_uio or
* vfio-pci

Different PMDs may require different kernel drivers in order to work properly. Depending on the PMD being used, a corresponding kernel driver should be loaded and bound to the network ports. Before loading, make sure that each NIC has been flashed with the latest version of NVM/firmware.

### UIO

Supported NICs

* Intel [igb](http://dpdk.org/browse/dpdk/tree/drivers/net/e1000) (82575, 82576, 82580, I210, I211, I350, I354, DH89xx)
* Intel [ixgbe](http://dpdk.org/doc/guides/nics/ixgbe.html) (82598, 82599, X520, X540, X550)
* Intel [i40e](http://dpdk.org/doc/guides/nics/i40e.html) (X710, XL710, X722)

RHEL does not support "**uio\_pci\_generic**" driver

To enable igb\_uio driver change physical\_uio\_driver in /etc/contrail/contrail-vrouter-agent.conf file and restart supervisor-vrouter.

/etc/contrail/contrail-vrouter-agent.conf  
[DEFAULT]  
physical\_uio\_driver=igb\_uio

### VFIO

Supported NICs

* Intel [i40e](http://dpdk.org/doc/guides/nics/i40e.html) (X710, XL710, X722)

### VFIO and IOMMU

Input–Output Memory Management Unit (IOMMU) is a memory management unit (MMU) that connects a Direct Memory Access (DMA) capable I/O bus to the main memory.

In Virtualization, an IOMMU is re-mapping the addresses accessed by the hardware into a similar translation table that is used to map guest-physical address to host-physical addresses.

![image](data:image/png;base64;base64,)

IOMMU provides a short path for the guest to get access to the physical device memory. Intel has published a specification for IOMMU technology as **Virtualization Technology for Directed I/O**, abbreviated as **VT-d**.

VFIO need to get IOMMU enabled :

* both kernel and BIOS must support and be configured to use IO virtualization (such as Intel® VT-d).
* IOMMU must be enabled into Linux Kernel parameters in /etc/default/grub and run update-grub command.

GRUB configuration example :

|  |
| --- |
| GRUB\_CMDLINE\_LINUX\_DEFAULT="**iommu=pt intel\_iommu=on**" |

**VFIO can be also be used without IOMMU.**

While this is just as unsafe as using UIO, it does make it possible for the user to keep the degree of device access and programming that VFIO has, in situations where IOMMU is not available.

To enable vfio-pci driver change physical\_uio\_driver in /etc/contrail/contrail-vrouter-agent.conf file and restart supervisor-vrouter.

[DEFAULT]  
physical\_uio\_driver=\*\*vfio-pci\*\*

**Drivers features compatibility list.**

[cols=",,,,",options="header",] |==== | |\*RHEL DPDK\* |\*Ubuntu DPDK\*|\*RHEL SRIOV (VF)\*\*|\*Ubuntu SRIOV (VF)\*\* |\*igb\_uio\* |No (no dkms support) |Yes (dkms) |No |Yes |\*uio\_pci\_generic\*|No (not supported by RHEL)|Yes |No |No |\*vfio\_pci\* |Yes |Yes |Yes |Yes |====

\*vRouter in parallel with SRIOV (VF support on VM)

## Discover hardware architecture topology

Use lstopo (hwloc-nox package)and numactl commands to check cores numbering and numa nodes architecture

(Ubuntu) # apt-get install hwloc  
(RedHat) # yum install hwloc  
  
# lstopo  
Machine (252GB)  
 NUMANode L#0 (P#0 126GB)  
 Socket L#0 + L3 L#0 (30MB)  
 L2 L#0 (256KB) + L1d L#0 (32KB) + L1i L#0 (32KB) + Core L#0  
 PU L#0 (P#0)  
 PU L#1 (P#24)  
 L2 L#1 (256KB) + L1d L#1 (32KB) + L1i L#1 (32KB) + Core L#1  
 PU L#2 (P#1)  
 PU L#3 (P#25)  
 L2 L#2 (256KB) + L1d L#2 (32KB) + L1i L#2 (32KB) + Core L#2  
 PU L#4 (P#2)  
 PU L#5 (P#26)  
 L2 L#3 (256KB) + L1d L#3 (32KB) + L1i L#3 (32KB) + Core L#3  
 PU L#6 (P#3)  
 PU L#7 (P#27)  
 L2 L#4 (256KB) + L1d L#4 (32KB) + L1i L#4 (32KB) + Core L#4  
 PU L#8 (P#4)  
 PU L#9 (P#28)  
 L2 L#5 (256KB) + L1d L#5 (32KB) + L1i L#5 (32KB) + Core L#5  
 PU L#10 (P#5)  
 PU L#11 (P#29)  
 L2 L#6 (256KB) + L1d L#6 (32KB) + L1i L#6 (32KB) + Core L#6  
 PU L#12 (P#6)  
 PU L#13 (P#30)  
 L2 L#7 (256KB) + L1d L#7 (32KB) + L1i L#7 (32KB) + Core L#7  
 PU L#14 (P#7)  
 PU L#15 (P#31)  
 L2 L#8 (256KB) + L1d L#8 (32KB) + L1i L#8 (32KB) + Core L#8  
 PU L#16 (P#8)  
 PU L#17 (P#32)  
 L2 L#9 (256KB) + L1d L#9 (32KB) + L1i L#9 (32KB) + Core L#9  
 PU L#18 (P#9)  
 PU L#19 (P#33)  
 L2 L#10 (256KB) + L1d L#10 (32KB) + L1i L#10 (32KB) + Core L#10  
 PU L#20 (P#10)  
 PU L#21 (P#34)  
 L2 L#11 (256KB) + L1d L#11 (32KB) + L1i L#11 (32KB) + Core L#11  
 PU L#22 (P#11)  
 PU L#23 (P#35)  
 HostBridge L#0  
 PCIBridge  
 PCI 103c:3239  
 Block L#0 "sda"  
 Block L#1 "sdb"  
 PCIBridge  
 PCI 8086:1572  
 Net L#2 "t1a"  
 PCI 8086:1572  
 Net L#3 "t1b"  
 PCIBridge  
 PCI 8086:1572  
 Net L#4 "t2a"  
 PCI 8086:1572  
 Net L#5 "t2b"  
 PCIBridge  
 PCI 102b:0533  
 PCIBridge  
 PCI 14e4:1657  
 Net L#6 "meth0"  
 PCI 14e4:1657  
 Net L#7 "meth1"  
 PCI 14e4:1657  
 Net L#8 "eth4"  
 PCI 14e4:1657  
 Net L#9 "eth6"  
 NUMANode L#1 (P#1 126GB) + Socket L#1 + L3 L#1 (30MB)  
 L2 L#12 (256KB) + L1d L#12 (32KB) + L1i L#12 (32KB) + Core L#12  
 PU L#24 (P#12)  
 PU L#25 (P#36)  
 L2 L#13 (256KB) + L1d L#13 (32KB) + L1i L#13 (32KB) + Core L#13  
 PU L#26 (P#13)  
 PU L#27 (P#37)  
 L2 L#14 (256KB) + L1d L#14 (32KB) + L1i L#14 (32KB) + Core L#14  
 PU L#28 (P#14)  
 PU L#29 (P#38)  
 L2 L#15 (256KB) + L1d L#15 (32KB) + L1i L#15 (32KB) + Core L#15  
 PU L#30 (P#15)  
 PU L#31 (P#39)  
 L2 L#16 (256KB) + L1d L#16 (32KB) + L1i L#16 (32KB) + Core L#16  
 PU L#32 (P#16)  
 PU L#33 (P#40)  
 L2 L#17 (256KB) + L1d L#17 (32KB) + L1i L#17 (32KB) + Core L#17  
 PU L#34 (P#17)  
 PU L#35 (P#41)  
 L2 L#18 (256KB) + L1d L#18 (32KB) + L1i L#18 (32KB) + Core L#18  
 PU L#36 (P#18)  
 PU L#37 (P#42)  
 L2 L#19 (256KB) + L1d L#19 (32KB) + L1i L#19 (32KB) + Core L#19  
 PU L#38 (P#19)  
 PU L#39 (P#43)  
 L2 L#20 (256KB) + L1d L#20 (32KB) + L1i L#20 (32KB) + Core L#20  
 PU L#40 (P#20)  
 PU L#41 (P#44)  
 L2 L#21 (256KB) + L1d L#21 (32KB) + L1i L#21 (32KB) + Core L#21  
 PU L#42 (P#21)  
 PU L#43 (P#45)  
 L2 L#22 (256KB) + L1d L#22 (32KB) + L1i L#22 (32KB) + Core L#22  
 PU L#44 (P#22)  
 PU L#45 (P#46)  
 L2 L#23 (256KB) + L1d L#23 (32KB) + L1i L#23 (32KB) + Core L#23  
 PU L#46 (P#23)  
 PU L#47 (P#47)

(Ubuntu) # apt-get install numactl  
(RedHat) # yum install numactl  
  
# numactl --hardware  
available: 2 nodes (0-1)  
node 0 cpus: 0 1 2 3 4 5 6 7 8 9 10 11 24 25 26 27 28 29 30 31 32 33 34 35  
node 0 size: 128811 MB  
node 0 free: 89428 MB  
node 1 cpus: 12 13 14 15 16 17 18 19 20 21 22 23 36 37 38 39 40 41 42 43 44 45 46 47  
node 1 size: 129019 MB  
node 1 free: 92592 MB  
node distances:  
node 0 1  
 0: 10 21  
 1: 21 10  
  
# lscpu | grep NUMA  
NUMA node(s): 2  
NUMA node0 CPU(s): 0-11,24-35  
NUMA node1 CPU(s): 12-23,36-47

To check NIC assignment to NUMA node.

# cat /sys/class/net/eth0/device/numa\_node  
0

We recommend assigning the Cores (real and sibling/hyperthreaded) to the same NUMA as the NIC(s).

Use lspci command to find PCI addresses of NICs that will be bound to DPDK process

# lspci | grep Ethernet  
02:00.0 Ethernet controller: Broadcom Corporation NetXtreme BCM5719 Gigabit Ethernet PCIe (rev 01)  
02:00.1 Ethernet controller: Broadcom Corporation NetXtreme BCM5719 Gigabit Ethernet PCIe (rev 01)  
02:00.2 Ethernet controller: Broadcom Corporation NetXtreme BCM5719 Gigabit Ethernet PCIe (rev 01)  
02:00.3 Ethernet controller: Broadcom Corporation NetXtreme BCM5719 Gigabit Ethernet PCIe (rev 01)  
05:00.0 Ethernet controller: Intel Corporation Ethernet Controller X710 for 10GbE SFP+ (rev 01)  
05:00.1 Ethernet controller: Intel Corporation Ethernet Controller X710 for 10GbE SFP+ (rev 01)  
0b:00.0 Ethernet controller: Intel Corporation Ethernet Controller X710 for 10GbE SFP+ (rev 01)  
0b:00.1 Ethernet controller: Intel Corporation Ethernet Controller X710 for 10GbE SFP+ (rev 01)

Use dpdk\_nic\_bind.py command to verify proper binding of NICs to DPDK

sudo /opt/contrail/bin/dpdk\_nic\_bind.py -s

![hwloc-ls GUI from 3.2 lab](data:image/png;base64;base64,)

hwloc-ls GUI from 3.2 lab

**3.2 lab.**

$ lstopo  
Machine (189GB)  
 NUMANode L#0 (P#0 94GB)  
 Socket L#0 + L3 L#0 (30MB)  
 L2 L#0 (256KB) + L1d L#0 (32KB) + L1i L#0 (32KB) + Core L#0  
 PU L#0 (P#0)  
 PU L#1 (P#24)  
 L2 L#1 (256KB) + L1d L#1 (32KB) + L1i L#1 (32KB) + Core L#1  
 PU L#2 (P#1)  
 PU L#3 (P#25)  
 L2 L#2 (256KB) + L1d L#2 (32KB) + L1i L#2 (32KB) + Core L#2  
 PU L#4 (P#2)  
 PU L#5 (P#26)  
 L2 L#3 (256KB) + L1d L#3 (32KB) + L1i L#3 (32KB) + Core L#3  
 PU L#6 (P#3)  
 PU L#7 (P#27)  
 L2 L#4 (256KB) + L1d L#4 (32KB) + L1i L#4 (32KB) + Core L#4  
 PU L#8 (P#4)  
 PU L#9 (P#28)  
 L2 L#5 (256KB) + L1d L#5 (32KB) + L1i L#5 (32KB) + Core L#5  
 PU L#10 (P#5)  
 PU L#11 (P#29)  
 L2 L#6 (256KB) + L1d L#6 (32KB) + L1i L#6 (32KB) + Core L#6  
 PU L#12 (P#6)  
 PU L#13 (P#30)  
 L2 L#7 (256KB) + L1d L#7 (32KB) + L1i L#7 (32KB) + Core L#7  
 PU L#14 (P#7)  
 PU L#15 (P#31)  
 L2 L#8 (256KB) + L1d L#8 (32KB) + L1i L#8 (32KB) + Core L#8  
 PU L#16 (P#8)  
 PU L#17 (P#32)  
 L2 L#9 (256KB) + L1d L#9 (32KB) + L1i L#9 (32KB) + Core L#9  
 PU L#18 (P#9)  
 PU L#19 (P#33)  
 L2 L#10 (256KB) + L1d L#10 (32KB) + L1i L#10 (32KB) + Core L#10  
 PU L#20 (P#10)  
 PU L#21 (P#34)  
 L2 L#11 (256KB) + L1d L#11 (32KB) + L1i L#11 (32KB) + Core L#11  
 PU L#22 (P#11)  
 PU L#23 (P#35)  
 HostBridge L#0  
 PCIBridge  
 PCI 8086:10f8  
 Net L#0 "em49"  
 PCI 8086:10f8  
 Net L#1 "em50"  
 PCIBridge  
 PCI 103c:3239  
 Block L#2 "sda"  
 PCIBridge  
 PCI 8086:10f8  
 Net L#3 "p1p1"  
 PCI 8086:10f8  
 PCIBridge  
 PCI 102b:0533  
 NUMANode L#1 (P#1 94GB)  
 Socket L#1 + L3 L#1 (30MB)  
 L2 L#12 (256KB) + L1d L#12 (32KB) + L1i L#12 (32KB) + Core L#12  
 PU L#24 (P#12)  
 PU L#25 (P#36)  
 L2 L#13 (256KB) + L1d L#13 (32KB) + L1i L#13 (32KB) + Core L#13  
 PU L#26 (P#13)  
 PU L#27 (P#37)  
 L2 L#14 (256KB) + L1d L#14 (32KB) + L1i L#14 (32KB) + Core L#14  
 PU L#28 (P#14)  
 PU L#29 (P#38)  
 L2 L#15 (256KB) + L1d L#15 (32KB) + L1i L#15 (32KB) + Core L#15  
 PU L#30 (P#15)  
 PU L#31 (P#39)  
 L2 L#16 (256KB) + L1d L#16 (32KB) + L1i L#16 (32KB) + Core L#16  
 PU L#32 (P#16)  
 PU L#33 (P#40)  
 L2 L#17 (256KB) + L1d L#17 (32KB) + L1i L#17 (32KB) + Core L#17  
 PU L#34 (P#17)  
 PU L#35 (P#41)  
 L2 L#18 (256KB) + L1d L#18 (32KB) + L1i L#18 (32KB) + Core L#18  
 PU L#36 (P#18)  
 PU L#37 (P#42)  
 L2 L#19 (256KB) + L1d L#19 (32KB) + L1i L#19 (32KB) + Core L#19  
 PU L#38 (P#19)  
 PU L#39 (P#43)  
 L2 L#20 (256KB) + L1d L#20 (32KB) + L1i L#20 (32KB) + Core L#20  
 PU L#40 (P#20)  
 PU L#41 (P#44)  
 L2 L#21 (256KB) + L1d L#21 (32KB) + L1i L#21 (32KB) + Core L#21  
 PU L#42 (P#21)  
 PU L#43 (P#45)  
 L2 L#22 (256KB) + L1d L#22 (32KB) + L1i L#22 (32KB) + Core L#22  
 PU L#44 (P#22)  
 PU L#45 (P#46)  
 L2 L#23 (256KB) + L1d L#23 (32KB) + L1i L#23 (32KB) + Core L#23  
 PU L#46 (P#23)  
 PU L#47 (P#47)  
 HostBridge L#5  
 PCIBridge  
 PCI 8086:10f8  
 PCI 8086:10f8  
 Net L#4 "p2p2"

**2003 lab.**

[root@overcloudjcx-compdpdk1hw0-0 heat-admin]# lspci | grep Ether  
19:00.0 Ethernet controller: Intel Corporation Ethernet Controller X710 for 10GbE SFP+ (rev 02)  
19:00.1 Ethernet controller: Intel Corporation Ethernet Controller X710 for 10GbE SFP+ (rev 02)  
19:00.2 Ethernet controller: Intel Corporation Ethernet Controller X710 for 10GbE SFP+ (rev 02)  
19:00.3 Ethernet controller: Intel Corporation Ethernet Controller X710 for 10GbE SFP+ (rev 02)  
3b:00.0 Ethernet controller: Intel Corporation I350 Gigabit Network Connection (rev 01)  
3b:00.1 Ethernet controller: Intel Corporation I350 Gigabit Network Connection (rev 01)  
  
  
[root@overcloudjcx-compdpdk1hw0-0 heat-admin]# docker exec -it contrail-vrouter-agent-dpdk /opt/contrail/bin/dpdk\_nic\_bind.py -s  
  
Network devices using DPDK-compatible driver  
============================================  
0000:19:00.0 'Ethernet Controller X710 for 10GbE SFP+' drv=vfio-pci unused=i40e  
0000:19:00.1 'Ethernet Controller X710 for 10GbE SFP+' drv=vfio-pci unused=i40e  
  
Network devices using kernel driver  
===================================  
0000:19:00.2 'Ethernet Controller X710 for 10GbE SFP+' if=em3 drv=i40e unused=vfio-pci  
0000:19:00.3 'Ethernet Controller X710 for 10GbE SFP+' if=em4 drv=i40e unused=vfio-pci  
0000:3b:00.0 'I350 Gigabit Network Connection' if=p1p1 drv=igb unused=vfio-pci \*Active\*  
0000:3b:00.1 'I350 Gigabit Network Connection' if=p1p2 drv=igb unused=vfio-pci  
  
Other network devices  
=====================  
<none>

## NICs supporing DPDK

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **NICs** | **Ubuntu - KVM** | **Ubuntu - DPDK** | **Redhat - KVM** | **Redhat - DPDK** | **vCenter - ESX** |
| Intel 82599/X520 "Niantic" - 10G | Yes | Yes | Yes | Yes | Yes |
| Intel X710 "Fortville" - 10G/25G/40G | Yes | Yes | Yes | Yes | Not tested |
| Broadcom bnxt 2x25G | Yes | Yes | Not tested | Not tested | Not tested |
| Mellanox 2x25G | Yes | Yes | Not tested | Not tested | Not tested |
| Netronome | 3.1.x only | No | No | No | No |

These are the guidelines from Intel with regard to Intel NIC X710 (in order not to bump into a known issue that impacts data plane)

* Do not use a single PCI NIC for non-DPDK and DPDK interfaces (having i40e kernel driver used together with i40e PMD driver for interfaces on the same PCI NIC cause problems)
* Upgrade NIC FW to 6.01 and i40e kernel driver to 2.4.6 (all necessary information you find in that document, table 9. <https://www.intel.com/content/dam/www/public/us/en/documents/release-notes/xl710-ethernet-controller-feature-matrix.pdf>
* LLDP is supported from 6.01 NIC FW but Intel also suggested to disable (ethtool -set-priv-flags <interface name> disable-fw-lldp on)

If your server manufacturer has no support for the latest firmware please contact him asap (i.e. The latest Lenovo server firmware includes 5.05 for X710 NICs)

* Redhat supports 1.6.27 i40 kernel driver version.
* Canonical supports 1.4.25 i40e kernel version.

# **Contrail vrouter and DPDK**

## Contrail vrouter architecture

vRouter is made of 2 parts :

* **vRouter agent** : vrouter control and configuration plane
* **vRouter dataplane** : vrouter userplane (user packet processing)

**agent (control plane).**

vRouter agent is used to manage the communication between Contrail SDN Controller and vRouter.

vRouter agent has 2 interfaces :

* vhost0 (north controller)
* pkt0 (south dataplane)

vRouter agent is always running in compute node user mode.

**vrouter (dataplane).**

vRouter dataplane has 2 kinds of interfaces

* Physical NIC : connected to underlay network in order to send traffic out of the compute node
* vNIC tap : connected to guest virtual instances

![vrouter interfaces](data:image/png;base64;base64,)

vrouter interfaces

vRouter dataplane is running either in Linux Kernel space or in Linux User space when DPDK is used. Better performances are expected when vRouter dataplane is running into Linux User space.

## vrouter and dpdk

Contrail vRouter is using DPDK library to improve packet processing performance.

When using contrail vrouter without DPDK, vRouter dataplane process is running into Linux Kernel.

![vRouter in kernel with VM application not DPDK aware](data:image/png;base64;base64,)

vRouter in kernel with VM application not DPDK aware

When using contrail vrouter with DPDK, vRouter dataplane is running into Linux user space.

![vRouter DPDK with VM application DPDK aware.](data:image/png;base64;base64,)

vRouter DPDK with VM application DPDK aware.

![vRouter DPDK with VM application not DPDK aware.](data:image/png;base64;base64,)

vRouter DPDK with VM application not DPDK aware.

In order to get good network performances, virtual instances (especially VNF - Virtual Network Function) are implementing DPDK. 4 topologies are possible:

* vrouter in Kernel mode collecting VNF with a network in Kernel Mode
* vrouter in Kernel mode collecting VNF running DPDK
* vrouter in DPDK mode collecting VNF with a network in Kernel Mode
* vrouter in DPDK mode collecting VNF running DPDK

An all DPDK stack, used both at vrouter level and at VNF level, is providing the best performance.

**vrouter 4 topologies.**

![image](data:image/png;base64;base64,)

When DPDK is used into the virtual instance, vNIC driver (virtio-net) used for packet processing in Kernel space is replaced by a virtio Poll Mode Driver (virtio-net PMD) in order to perform packet processing in Virtual Instance user space.

## DPDK threads and Contrail lcore numbering

DPDK vrouter is a multi-threads application. DPDK vrouter forwarding plane process is made up of several kinds of threads.

control and service threads are used for DPDK vrouter configuration (add/remove vif interfaces onto the vrouter, manage the communication with the vrouter agent for instance)

The term lcore refers to an EAL (Environment Abstraction Layer) thread, which is really a Linux/FreeBSD pthread (physical Thread). A numbering into the dpdk vrouter is used for lcores.

There are 3 set of threads into a DPDK vrouter, Each set of threads is made up of several single threads:

* **control threads** : used for DPDK internal processing. eal-intr-thread, rte\_mp\_handle, rte\_mp\_async (they are generated by the DPDK library itself - DPDK setup management) **DPDK control threads will be allocated onto Operating System assigned CPUs**
* **service threads** : used for connectivity between vrouter agent and vrouter forwarding plane (DPDK vrouter). Thread names are lcore 0 to 9 thread names are lcore 0 to 9. They each one has a specific role:
  + lcore 0: vhost0
  + lcore 1: timers
  + lcore 2: Interrupts
  + lcore 8: pkt0 (can be busy)
  + lcore 9: Netlink (can be busy)
* **processing threads** : used for packet polling and processing (forwarding plane), thread names are lcore 10 and above

### control threads

DPDK control threads can be pinned on any CPU. These CPUs are only used during Contrail vRouter startup for DPDK initialization. As they did not require high CPU capacity, a good strategy is to use the CPU allocated to the Operating System for these threads.

### Service and Processing threads

Besides forwarding threads Contrail DPDK vRouter runs service threads :

* **pkt0 thread** for a communication with Contrail vRouter Agent (flow setup)
  + this is vRouter lcore ID 8 thread (cf appendix section for lcore/pthread numbering).
  + This is used to send and receive packets to/from the agent.
  + eg: 1st packet of flow, arp, dhcp etc.
* **netlink thread** to give vRouter Agent possibility to get statistics from Contrail DPDK vRouter
  + this is vRouter lcore ID 9 thread (cf appendix section for lcore/pthread numbering)
  + The Netlink socket family is a Linux kernel interface used for inter-process communication (IPC)
* Before contrail 20.03 release, Service threads were pinned to the whole range of cores available on the host system.
* Since the 20.03 release it is possible to pin these threads on some specific CPUs.

Service and Processing threads are named lcore-slave-<ID>. Contrail vRouter cores ID have a specific meaning defined in the following C enum data structure, An enumeration is defining this numbering :

enum {  
 VR\_DPDK\_KNITAP\_LCORE\_ID = 0,  
 VR\_DPDK\_TIMER\_LCORE\_ID,  
 VR\_DPDK\_UVHOST\_LCORE\_ID,  
 VR\_DPDK\_IO\_LCORE\_ID, # 3  
 VR\_DPDK\_IO\_LCORE\_ID2,  
 VR\_DPDK\_IO\_LCORE\_ID3,  
 VR\_DPDK\_IO\_LCORE\_ID4,  
 VR\_DPDK\_LAST\_IO\_LCORE\_ID, # 7  
 VR\_DPDK\_PACKET\_LCORE\_ID, # 8  
 VR\_DPDK\_NETLINK\_LCORE\_ID,  
 VR\_DPDK\_FWD\_LCORE\_ID, # 10  
};

This **lcore numbering** used in vrouter can be seen into source file (vr\_dpdk.h). Lots of other details concerning DPDK vrouter can also be seen into following files :

include/vr\_dpdk.h  
dpdk/dpdk\_vrouter.c  
dpdk/vr\_dpdk\_lcore.c

**ping: from** [**https://github.com/Juniper/contrail-vrouter/blob/master/include/vr\_dpdk.h**](https://github.com/Juniper/contrail-vrouter/blob/master/include/vr_dpdk.h)**.**

/\*  
 \* DPDK LCore IDs  
 \*/  
enum {  
 VR\_DPDK\_KNITAP\_LCORE\_ID = 0,  
 VR\_DPDK\_TIMER\_LCORE\_ID,  
 VR\_DPDK\_UVHOST\_LCORE\_ID,  
 /\*  
 \* The actual number of IO lcores depends on the number of  
 \* forwarding lcores.  
 \*/  
 VR\_DPDK\_IO\_LCORE\_ID,  
 VR\_DPDK\_IO\_LCORE\_ID2,  
 VR\_DPDK\_IO\_LCORE\_ID3,  
 VR\_DPDK\_IO\_LCORE\_ID4,  
 VR\_DPDK\_LAST\_IO\_LCORE\_ID,  
 /\* [PACKET\_ID..FWD\_ID) lcores have TX queues, but no RX queues \*/  
 VR\_DPDK\_PACKET\_LCORE\_ID,  
 VR\_DPDK\_NETLINK\_LCORE\_ID,  
 /\* The actual number of forwarding lcores depends on affinity mask. \*/  
 VR\_DPDK\_FWD\_LCORE\_ID,  
};

0 to 9 lcore numbers are statically defined into the source code and can’t be configured by user.

* The 3 first logical numbers (0 to 2) are used for "service lcores".
* The 5 next ones (3 to 7) are booked for IO lcores.
* The 2 next ones (8 to 9) are "lcores with TX queues".
* Logical cores with number 10 and above are forwarding logical cores.

contrail and service cores should be pinned to dedicated core(s) if flow mode is heavly used, in packet mode can be use the CPU allocated to the Operating System. This value is set into /etc/sysconfig/network-scripts/ifcfg-vhost0 configuration file.

DPDK\_CTRL\_THREAD\_MASK=0,1,28,29  
SERVICE\_CORE\_MASK=0,1,28,29

The value can be provided as list (in the example) or hex mask (0x540000054).

### forwarding threads

* Contrail DPDK vRouter runs forwarding threads to poll NIC queues
* Forwarding threads are lcore ID 10 and above (cf appendix section for lcore/pthread numbering)
* 1 to 1 mapping between thread and queue
* Forwarding threads in their infinity loops poll its queues on the NIC to check if there is packet or burst of packets to receive.
* It is providing descriptors where packets have to be copied to host memory (memory allocated by hugepage).
* That packet movement to memory is done using NIC DMA (Direct Memory Access processor).
* Each forwarding thread is pinned to its dedicated CPU core (named DPDK lcore).
* The number of NIC queues is dependent on the number of CPU cores which are specified by coremask in Contrail DPDK vRouter configuration (contrail-vrouter-dpdk.ini file).
* Contrail DPDK vRouter uses DPDK ethdev function to program the NIC.

lcore numbers 10 and above are used for forwarding purpose and defined with CPU affinity value.

This value is set into /etc/sysconfig/network-scripts/ifcfg-vhost0 configuration file.

CPU\_LIST=2,4,6,30,32,34

For instance 2,4,6,30,32,34 CPU list is giving following mapping :

34 33 32 31 30 29 28 27 26 25 24 23 22 21 20 19 18 17 16 15 14 13 12 11 10 09 08 07 06 05 04 03 02 01 00  
 1 0 1 0 1 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 1 0 1 0 1 0 0

it means Host CPU numbers 2, 4, 6, 30, 32 and 34 are used for vrouter forwarding logical cores.

$ cat /etc/contrail/supervisord\_vrouter\_files/contrail-vrouter-dpdk.ini  
[program:contrail-vrouter-dpdk]  
command=taskset 0xf /usr/bin/contrail-vrouter-dpdk --no-daemon --vdev "eth\_bond\_bond0,mode=4,xmit\_policy=l34,socket\_id=0,mac=5c:b9:01:8b:6f:3c,slave=0000:08:00.0,slave=0000:08:00.1" --vlan\_tci "2004" --vlan\_fwd\_intf\_name "bond0" --socket-mem 1024,1024

0xf ⇒ cpu# 0~3 are pinned for forwarding.

***how to check in logs*.**

When the router boots up, it displays a message about its logical cores numbering. For instance, we can get into contrail-vrouter-dpdk-stdout.log file, such a message :

VROUTER: --lcores "(0-2)@(0-47),(8-9)@(0-47),\*10@2,11@4,12@6,13@8,14@26,15@28,16@30,17@32\*"  
EAL: Detected 48 lcore(s)  
\*VROUTER: Using 8 forwarding lcore(s)\*  
VROUTER: Using 0 IO lcore(s)  
VROUTER: Using 5 service lcores

* First part of the message - (0-2)@(0-N),(8-9)@(0-N) - is always the same, as this internal CPU logical numbering is statically defined in vrouter source code.
* N is the total number of CPU available in the compute onto which the vrouter is running.
* Last part of the message - 10@2,11@4,12@6,13@8,14@26,15@28,16@30,17@32 - is depending on the CPU affinity.
* Here 8 logical cores are used for forwarding purpose, they are numbered from 10 to 17. They are mapped one by one onto the host CPUs 2, 4, 6, 8, 26, 28, 30 and 32.

**3.2 lab.**

$ cat /var/log/contrail/contrail-vrouter-dpdk-stdout.log  
2019-09-27 11:09:58,126 VROUTER: EAL arguments:  
2019-09-27 11:09:58,126 VROUTER: -n "4"  
2019-09-27 11:09:58,126 VROUTER: --socket-mem "1024,1024"  
2019-09-27 11:09:58,126 VROUTER: --vdev "eth\_bond\_bond0,mode=4,xmit\_policy=l34,socket\_id=0,mac=5c:b9:01:8b:6f:3c,slave=0000:08:00.0,slave=0000:08:00.1"  
2019-09-27 11:09:58,126 VROUTER: --lcores "(0-2)@(0-47),(8-9)@(0-47),10@0,11@1,12@2,13@3"  
2019-09-27 11:09:58,126 EAL: Detected 48 lcore(s)

**19.08 lab.**

$ cat /var/log/containers/contrail/contrail-vrouter-dpdk.log  
2020-03-09 08:20:55,137 VROUTER: EAL arguments:  
2020-03-09 08:20:55,137 VROUTER: -n "4"  
2020-03-09 08:20:55,137 VROUTER: --socket-mem "1024,1024"  
2020-03-09 08:20:55,137 VROUTER: --vdev "eth\_bond\_bond0,mode=4,xmit\_policy=l23,socket\_id=0,mac=0c:c4:7a:b7:2c:f8,lacp\_rate=1,slave=0000:02:00.0,slave=0000:02:00.1"  
2020-03-09 08:20:55,137 VROUTER: --lcores "(0-2)@(0-39),(8-9)@(0-39),10@1,11@2,12@3,13@21,14@22,15@23"  
2020-03-09 08:20:55,144 EAL: Detected 40 lcore(s)  
2020-03-09 08:20:55,144 EAL: Detected 2 NUMA nodes

**2003 lab.**

2020-05-25 09:31:19,640 VROUTER: EAL arguments:  
2020-05-25 09:31:19,640 VROUTER: -n "4"  
2020-05-25 09:31:19,640 VROUTER: --socket-mem "1024,1024"  
2020-05-25 09:31:19,640 VROUTER: --vdev "eth\_bond\_bond1,mode=4,xmit\_policy=l34,socket\_id=0,mac=e4:43:4b:6e:70:70,lacp\_rate=1,slave=0000:19:00.0,slave=0000:19:00.1"  
2020-05-25 09:31:19,640 VROUTER: -t "(0,1,28,29)"  
2020-05-25 09:31:19,640 VROUTER: --lcores "(0-2)@(0,1,28,29),(8-9)@(0,1,28,29),10@2,11@4,12@6,13@30,14@32,15@34"  
2020-05-25 09:31:19,646 EAL: Detected 56 lcore(s)  
2020-05-25 09:31:19,646 EAL: Detected 2 NUMA nodes

This is this vrouter logical core numbering that has to be in dropstats command (not the real host CPU numbering)

$ dropstats –core 10

A maximum of 16 polling cores is currently supported by Contrail as the maximum RX queue is currently 16:

#define VR\_DPDK\_MAX\_NB\_RX\_QUEUES 16

We can find those names by running using the "ps" command with some additional arguments (this is from a compute node where vrouter is using 8 logical forwarding cores, 4 phy cores using HT siblings):

# ps -Tp `pidof contrail-vrouter-dpdk`  
PID SPID TTY TIME CMD  
\*54490 54490 ? 02:46:12 contrail-vroute\*  
\*54490 54611 ? 00:02:33 eal-intr-thread\*  
\*54490 54612 ? 01:35:26 lcore-slave-1\*  
\*54490 54613 ? 00:00:00 lcore-slave-2\*  
\*54490 54614 ? 00:00:17 lcore-slave-8\*  
\*54490 54615 ? 00:02:14 lcore-slave-9\*  
\*54490 54616 ? 2-21:44:06 lcore-slave-10\*  
\*54490 54617 ? 2-21:44:06 lcore-slave-11\*  
\*54490 54618 ? 2-21:44:06 lcore-slave-12\*  
\*54490 54619 ? 2-21:44:06 lcore-slave-13\*  
\*54490 54620 ? 2-21:44:06 lcore-slave-14\*  
\*54490 54621 ? 2-21:44:06 lcore-slave-15\*  
\*54490 54622 ? 2-21:44:06 lcore-slave-16\*  
\*54490 54623 ? 2-21:44:06 lcore-slave-17\*  
\*54490 54990 ? 00:00:00 lcore-slave-9\*

**ping: lab.**

[heat-admin@jnprctdpdk01 ~]$ ps -Tp `pidof contrail-vrouter-dpdk`  
 PID SPID TTY TIME CMD  
 46058 46058 ? 1-18:54:41 contrail-vroute  
 46058 46070 ? 00:00:00 rte\_mp\_handle  
 46058 46071 ? 00:00:00 rte\_mp\_async  
 46058 46073 ? 01:24:03 eal-intr-thread  
 46058 46074 ? 2-12:27:21 lcore-slave-1  
 46058 46075 ? 00:00:00 lcore-slave-2  
 46058 46076 ? 00:04:59 lcore-slave-8  
 46058 46077 ? 00:33:48 lcore-slave-9  
 46058 46078 ? 24-13:55:14 lcore-slave-10  
 46058 46079 ? 24-13:55:58 lcore-slave-11  
 46058 46080 ? 24-13:56:00 lcore-slave-12  
 46058 46536 ? 00:00:00 lcore-slave-9

Here we have :

* **contrail-vrouter is main thread**
* **lcore-slave-1 is timer thread**
* **lcore-slave-2 is uvhost (for qemu) thread**
* l**core-slave-8 is pkt0 thread**
* lcore-slave-9 is netlink thread (for nh/rt programming)
* **lcore-slave-10 onwards are forwarding threads, the ones running at 100% as they are constantly polling the interfaces**

To list all lightweight processes created by contrail-vrouter-dpdk run following command:

# pstree -p $(ps -ef | awk '$8=="/usr/bin/contrail-vrouter-dpdk" {print $2}')  
contrail-vroute(6665)─┬─{contrail-vroute}(7800)  
├─{contrail-vroute}(7801)  
├─{contrail-vroute}(7802)  
├─{contrail-vroute}(7803)  
├─{contrail-vroute}(7804)  
├─{contrail-vroute}(7805)  
├─{contrail-vroute}(7806)  
├─{contrail-vroute}(7807)  
├─{contrail-vroute}(7808)  
└─{contrail-vroute}(8200)

The following command can be used. It provides in the last column the CPU load generated by each thread:

# ps -mo pid,tid,comm,psr,pcpu -p $(ps -ef | awk '$8=="/usr/bin/contrail-vrouter-dpdk" {print $2}')  
 PID TID COMMAND PSR %CPU  
 58324 - contrail-vroute - 602  
 - 58324 - 28 3.7  
 - 58337 - 0 0.0  
 - 58338 - 0 0.0  
 - 58341 - 1 0.0  
 - 58342 - 28 5.0  
 - 58343 - 0 0.0  
 - 58344 - 29 0.2  
 - 58345 - 1 0.4  
 - 58346 - 2 99.2  
 - 58347 - 4 99.2  
 - 58348 - 6 99.2  
 - 58349 - 30 99.2  
 - 58350 - 32 99.2  
 - 58351 - 34 99.2  
 - 58774 - 1 0.0

Using ***pidstat*** command we can see that some vrouter threads are running at 100% CPU. Those are the forwarding threads, the ones pinned based on the configured coremask :

#pidstat -t -p `pidof contrail-vrouter-dpdk`  
Linux 3.10.0-1062.12.1.el7.x86\_64 (overcloudjcx-compdpdk1hw0-0.prod1.bw.juniper.net) 05/25/2020 \_x86\_64\_ (56 CPU)  
  
09:39:05 AM UID TGID TID %usr %system %guest %CPU CPU Command  
09:39:05 AM 0 58324 - 0.06 0.00 0.00 0.06 1 contrail-vroute  
09:39:05 AM 0 - 58324 0.00 0.00 0.00 0.00 1 |\_\_contrail-vroute  
09:39:05 AM 0 - 58337 0.00 0.00 0.00 0.00 0 |\_\_rte\_mp\_handle  
09:39:05 AM 0 - 58338 0.00 0.00 0.00 0.00 0 |\_\_rte\_mp\_async  
09:39:05 AM 0 - 58341 0.00 0.00 0.00 0.00 0 |\_\_eal-intr-thread  
09:39:05 AM 0 - 58342 0.00 0.00 0.00 0.00 29 |\_\_lcore-slave-1  
09:39:05 AM 0 - 58343 0.00 0.00 0.00 0.00 0 |\_\_lcore-slave-2  
09:39:05 AM 0 - 58344 0.00 0.00 0.00 0.00 29 |\_\_lcore-slave-8  
09:39:05 AM 0 - 58345 0.00 0.00 0.00 0.00 29 |\_\_lcore-slave-9  
09:39:05 AM 0 - 58346 0.01 0.00 0.00 0.01 2 |\_\_lcore-slave-10  
09:39:05 AM 0 - 58347 0.01 0.00 0.00 0.01 4 |\_\_lcore-slave-11  
09:39:05 AM 0 - 58348 0.01 0.00 0.00 0.01 6 |\_\_lcore-slave-12  
09:39:05 AM 0 - 58349 0.01 0.00 0.00 0.01 30 |\_\_lcore-slave-13  
09:39:05 AM 0 - 58350 0.01 0.00 0.00 0.01 32 |\_\_lcore-slave-14  
09:39:05 AM 0 - 58351 0.01 0.00 0.00 0.01 34 |\_\_lcore-slave-15  
09:39:05 AM 0 - 58774 0.00 0.00 0.00 0.00 29 |\_\_lcore-slave-9

In the example above, we can notice:

* **processing/forwarding threads:** lcore-slave-10 - lcore-slave-15, ~100% CPU load.
* **service threads:** lcore-slave-1 - lcore-slave-9.
* **control threads:** rte\_mp\_handle,rte\_mp\_async, eal-intr-thread.

pidstat command is not provided in default OS installation. It has to be installed with following command on RedHat system:

# yum install -y sysstat

In order to list CPU cores assigned to contrail-vrouter-dpdk, we have to run taskset command for each lightweight process.

# taskset -cp -a $(pidof contrail-vrouter-dpdk)  
pid 58324's current affinity list: 0,1,28,29  
pid 58337's current affinity list: 0,1,28,29  
pid 58338's current affinity list: 0,1,28,29  
pid 58341's current affinity list: 0,1,28,29  
pid 58342's current affinity list: 0,1,28,29  
pid 58343's current affinity list: 0,1,28,29  
pid 58344's current affinity list: 0,1,28,29  
pid 58345's current affinity list: 0,1,28,29  
pid 58346's current affinity list: 2  
pid 58347's current affinity list: 4  
pid 58348's current affinity list: 6  
pid 58349's current affinity list: 30  
pid 58350's current affinity list: 32  
pid 58351's current affinity list: 34  
pid 58774's current affinity list: 0,1,28,29

[heat-admin@jnprctdpdk01 ~]$ pstree -p $(ps -ef | awk '$8=="/usr/bin/contrail-vrouter-dpdk" {print $2}')  
contrail-vroute(46058)─┬─{contrail-vroute}(46070)  
 ├─{contrail-vroute}(46071)  
 ├─{contrail-vroute}(46073)  
 ├─{contrail-vroute}(46074)  
 ├─{contrail-vroute}(46075)  
 ├─{contrail-vroute}(46076)  
 ├─{contrail-vroute}(46077)  
 ├─{contrail-vroute}(46078)  
 ├─{contrail-vroute}(46079)  
 ├─{contrail-vroute}(46080)  
 └─{contrail-vroute}(46536)

**2003 lab.**

# pstree -p $(ps -ef | awk '$8=="/usr/bin/contrail-vrouter-dpdk" {print $2}')  
contrail-vroute(58324)─┬─{contrail-vroute}(58337)  
 ├─{contrail-vroute}(58338)  
 ├─{contrail-vroute}(58341)  
 ├─{contrail-vroute}(58342)  
 ├─{contrail-vroute}(58343)  
 ├─{contrail-vroute}(58344)  
 ├─{contrail-vroute}(58345)  
 ├─{contrail-vroute}(58346)  
 ├─{contrail-vroute}(58347)  
 ├─{contrail-vroute}(58348)  
 ├─{contrail-vroute}(58349)  
 ├─{contrail-vroute}(58350)  
 ├─{contrail-vroute}(58351)  
 └─{contrail-vroute}(58774)

ps -mo pid,tid,comm,psr,pcpu -p $(ps -ef | awk '$8=="/usr/bin/contrail-vrouter-dpdk" {print $2}')  
PID TID COMMAND PSR %CPU  
161791 - contrail-vroute - 618  
- 161791 - 22 1.6  
- 161867 - 3 0.0  
- 161868 - 27 1.1  
- 161869 - 18 0.0  
- 161870 - 27 0.3  
- 161871 - 21 0.0  
- 161872 - 2 64.3  
- 161873 - 3 64.3  
- 161874 - 4 64.3  
- 161875 - 5 64.3  
- 161876 - 6 64.3  
- 161877 - 7 98.3  
- 161878 - 8 98.1  
- 161879 - 9 97.7  
- 162134 - 11 0.0

[root@overcloudmz5-compdpdk-1 ~]# pidstat -t -p `pidof contrail-vrouter-dpdk`  
Linux 3.10.0-957.27.2.el7.x86\_64 (overcloudmz5-compdpdk-1.srelab1.englab.juniper.net) 05/06/2020 \_x86\_64\_ (40 CPU)  
  
07:53:19 AM UID TGID TID %usr %system %guest %CPU CPU Command  
07:53:19 AM 0 15745 - 100.00 100.00 0.00 100.00 6 contrail-vroute  
07:53:19 AM 0 - 15745 0.68 0.62 0.00 1.29 6 |\_\_contrail-vroute  
07:53:19 AM 0 - 15777 0.00 0.00 0.00 0.00 3 |\_\_rte\_mp\_handle  
07:53:19 AM 0 - 15778 0.00 0.00 0.00 0.00 3 |\_\_rte\_mp\_async  
07:53:19 AM 0 - 15780 0.01 0.01 0.00 0.02 6 |\_\_eal-intr-thread  
07:53:19 AM 0 - 15781 1.21 1.00 0.00 2.21 6 |\_\_lcore-slave-1  
07:53:19 AM 0 - 15782 0.00 0.00 0.00 0.00 6 |\_\_lcore-slave-2  
07:53:19 AM 0 - 15783 0.00 0.00 0.00 0.00 6 |\_\_lcore-slave-8  
07:53:19 AM 0 - 15784 0.03 0.00 0.00 0.03 6 |\_\_lcore-slave-9  
07:53:19 AM 0 - 15785 55.21 44.79 0.00 100.00 1 |\_\_lcore-slave-10  
07:53:19 AM 0 - 15786 56.77 42.18 0.00 98.95 6 |\_\_lcore-slave-11  
07:53:19 AM 0 - 15787 54.10 45.89 0.00 99.99 3 |\_\_lcore-slave-12  
07:53:19 AM 0 - 15788 55.25 44.75 0.00 100.00 21 |\_\_lcore-slave-13  
07:53:19 AM 0 - 15789 57.25 42.75 0.00 100.00 22 |\_\_lcore-slave-14  
07:53:19 AM 0 - 15790 54.27 45.73 0.00 100.00 23 |\_\_lcore-slave-15  
07:53:19 AM 0 - 17452 0.00 0.00 0.00 0.00 6 |\_\_lcore-slave-9

[heat-admin@jnprctdpdk01 ~]$ taskset -cp 46075  
pid 46075's current affinity list: 4  
[heat-admin@jnprctdpdk01 ~]$ taskset -cp 46076  
pid 46076's current affinity list: 4  
[heat-admin@jnprctdpdk01 ~]$ taskset -cp 46074  
pid 46074's current affinity list: 4  
[heat-admin@jnprctdpdk01 ~]$ taskset -cp 46078  
pid 46078's current affinity list: 1  
[heat-admin@jnprctdpdk01 ~]$ taskset -cp 46079  
pid 46079's current affinity list: 2

## contrail dpdk version

Starting from Contrail 3.2.5 DPDK library 17.02 is used. Earlier Contrail versions were based on DPDK library version 2.1 <https://www.juniper.net/documentation/en_US/contrail3.2/information-products/topic-collections/release-notes/jd0e36.html#jd0e185>

Contrail DPDK library fork

<https://github.com/Juniper/contrail-dpdk>

DPDK release notes

<http://dpdk.org/doc/guides-17.02/rel_notes/index.html>

DPDK version used by the vrouter can be checked into dpdk vrouter log files :

$ vi /var/log/containers/contrail/contrail-vrouter-dpdk.log  
...  
2019-04-19 16:30:41,411 VROUTER: vRouter version: \{"build-info": [\{"build-time": "2019-04-11 23:47:32.407280", "build-hostname": "rhel-7-builder-juniper-contrail-ci-c-0000225573.novalocal", "build-user": "zuul", "build-version": "5.1.0"}]}  
2019-04-19 16:30:41,411 VROUTER: DPDK version: \*DPDK 18.05.1\*  
...

$ less /var/log/contrail/contrail-vrouter-dpdk-stdout.log | grep -i version | tail -2  
2019-09-27 11:09:58,103 VROUTER: vRouter version: {"build-info": [{"build-time": "2018-10-18 07:00:47.106457", "build-hostname": "ubuntu", "build-user": "contrail-builder", "build-version": "3.2.13.0"}]}  
2019-09-27 11:09:58,103 VROUTER: DPDK version: DPDK 17.02.0

## Contrail related linux packages

Ubuntu

|  |  |
| --- | --- |
| **Package name** | **Description** |
| contrail-dpdk-kernel-modules-dkms | Contrail DPDK 17.02 library in DKMS format |
| contrail-vrouter-dpdk | Core vRouter DPDK binary |
| contrail-vrouter-dpdk-init a | DPDK compute-node startup and monitoring scripts like: contrail-vrouter-dpdk.ini dpdk\_nic\_bind.py if-vhost0 |

Redhat

|  |  |
| --- | --- |
| **Package name** | **Description** |
| dpdk | RHEL DPDK package |
| contrail-vrouter-dpdk | Core vRouter DPDK binary |
| contrail-vrouter-dpdk-init | DPDK compute-node startup and monitoring scripts like: contrail-vrouter-dpdk.ini dpdk\_nic\_bind.py if-vhost0 |

* info how to deploy with Director with Openstack Newton <https://github.com/Juniper/contrail-tripleo-heat-templates/tree/stable/newton>

**Nova / Qemu / Libvirt.**

It is required to have Contrail qemu / libvirt / nova packages installed on DPDK nodes in order to:

* Support multiqueue (Multiqueue support is available from Mitaka release)
* Not lose connectivity to VMs when restarting DPDK vrouter

This limitation is removed. It is possible to use qemu and nova upstream packages with contrail-nova-vif-driver. Starting from OpenStack Pike release, no patch is required. **libvirt is the only package needed if we want multiqueue**.

# **DPDK vrouter packet forwarding**

## interfaces and queues

Contrail DPDK vrouter as any DPDK application is based on queue management.

Queue packets processing consists in :

* queues: in a network interface
* pthreads (lcore): for packet enqueue or dequeue (packet polling)
* descriptor rings (TX/RX): for packet transfer between interface queue and host memory (mbuf)
* memory spaces (mempool)

![muf, queue, ring, lcore](data:image/png;base64;base64,)

muf, queue, ring, lcore

3 kinds of interfaces are connected onto the vrouter :

* Physical interface card (usually a bond) : vif 0/0
* Internal processing interfaces (pkt0) : vif 0/2
* Virtual Machine Interfaces : vif 0/n

For each vrouter interface one or several queues are managed. Two kinds of interfaces have to be taken in consideration :

* vrouter physical interface card: one TX queue and one RX queue are created for each CPU pinned to vrouter. Onto vrouter virtual machine.
* vrouter virtual machine interface: one or several queues could be implemented for each virtual NIC. It depends if the given virtual machine is supporting multi-queue or not.

**about vhost0(vif 0/1):.**

here is a drawing which is describing how are plugged each internal nic onto vrouter dataplane. Vhost0 is belonging to vrouter agent, not to vrouter dataplane. This is vif0/1 which is connected onto the vrouter dapaplane.

![image](data:image/png;base64;base64,)

**regarding "one Q per cpu": is Q a concept in NIC or in CPU?.**

DPDK application principle is simple.

We are allocating as many as needed CPUs as required to process incoming packets. You have to consider the application we are building with DPDK. For Juniper/Contrail this is a vrouter processing packets coming from a single physical Interface (to be sent to VM). This single interface can be a bond. But at vrouter level there is always a unique physical interface. All the dimensioning consist in “how many CPU do I need to process packet coming from this interface (vif0) ?”

The answer is N CPU. For each CPU we are allocating 1 processing bidirectional Q (2 in reality because there are 2 directions = 1 for RX and one for RX) which are the buffers in which we store the packets coming from the physical NIC (RX Q) or to sent to the physical NIC (TX Q).

So N CPU, means N bidirectional Q (in fact this is 2 x N single direction Q N x RX + N x TX).

In the diagram below we have a first overview of vrouter packet processing for an external packet to be sent to virtual machine instances.

![vrouter packet processing (first overview)](data:image/png;base64;base64,)

vrouter packet processing (first overview)

There are 4 main steps in packet processing :

* **step one**: incoming packets are put into RX queues by the network interface card.
* **step two:** each CPU (c1 to c4) is polling its allocated queue in order to put each packet into host memory in order to be processed.
* **step three:** packet processing is achieved by a forwarding thread. This forwarding thread could be performed onto any CPU allocated to vrouter.
* **step four:** after being processed, packet is copied onto virtual machine TX interface queues.

ping? here term "copy" needs to be double quoted, as we understand it is not a real copy, or copied only once - from NIC to main memory. later "copy" is just sharing the pointer/addresses/descriptors…​

these 4 steps are performed for VxLAN and MPLSoUDP. For MPLSoGRE, it’s different. this will be further explained later.

## DPDK VM incoming traffic (from underlay network)

When the traffic is coming from the underlay network, encapsulated packets are received DPDK compute Physical interface which is bound to vrouter vif 0/0:

![ingress forwarding process](data:image/png;base64;base64,)

ingress forwarding process

**ingress fowarding process.**

Incoming packets are processed in 3 steps :

* packets are polled by a vrouter polling core and decapsulated.
* decapsulated packet are sent by polling core to a processing core
* processing core is delivering packet to a destination vif interface

Two main situations have to be considered for processing core selection :

* incoming underlay packets are encapsulated with MPLS over GRE
* incoming underlay packets are encapsulated with MPLS over UDP or VxLAN

### step 1: NIC spreading (RSS)

![Contrail DPDK vRouter architecture](data:image/png;base64;base64,)

Contrail DPDK vRouter architecture

The packet arrives at a physical NIC (pNIC) The pNIC computes a hash on the packet outer header

* this hash is called "RSS hash" (Receive Side Scaling)
* this hash is computed onto the encapsulated packet and does not take into account the header of the tenant packet (inner header)

Physical NIC (usually an interface bond) itself spread packets across its queues using 5-tuple hashing function (source IP, destination IP, source port, destination port and protocol).

Depending on overlay encapsulation protocol used, the incoming traffic is well balanced or not onto NIC card RX queues :

* **MPLSoUDP, VxLAN encapsulation protocols** : provide a good entropy.
  + A good hashing will be achieved with their UDP datagrams (several source port values are used for the same tunnel IP source and destination pair).
* **MPLSoGRE encapsulation protocol** : not provide a good entropy.
  + Packets from one SDN gateway will be placed only in a single queue, which is not an optimal host resource utilization.
  + With a second gateway it is likely to have two NIC queues utilized.

That is the reason Juniper recommends implementing MPLSoUDP on Juniper MXes (supported in Junos >=16.2).

Based on the "RSS hash", the pNIC selects a queue and writes the packet to the queue (RX QUEUE into the previous diagram).

![RSS hash](data:image/png;base64;base64,)

RSS hash

### step 2: Polling core

Then incoming packet is dequeued by the polling logical core (step 1) :

* there is one queue per vRouter logical core
* vRouter polling logical core in charge of that queue manages packet transfer from NIC queue to a free mbuf into the mempool.
* when incoming packets are encapsulated with MPLS over GRE, vRouter polling logical core in charge of that queue reads the packet header, computes a hash, and selects a vRouter processing logical core based on the hash.

Hashing algorithm is in vr\_dpdk\_ethdev.c module (<https://github.com/Juniper/contrail-vrouter/blob/R5.0/dpdk/vr_dpdk_ethdev.c#L873>)

### step 3: Forwarding core (MPLSoGRE)

In previous stage polling CPU bound to the queue on which a packet has been received, is triggering packet transfer from given NIC RX queue to mbuf.

This CPU (here CPU 0) will also choose which CPU (forwarding CPU) will have to process the packet (decapsulation, routing, switching, etc).

So a hash will be calculated onto polling CPU on decapsulated packet in order to select a forwarding CPU (decapsulated packet should have a better entropy than encapsulated one with MPLS over GRE).

Then the forwarding logical core is processing the packet (step 2). Forwarding CPU is in charge to do :

* flow lookup,
* flow enforcement (switching, routing, NAT, packet transformation)
* decapsulation,
* packet delivery to VM RX queue (vRouter vif TX-QUEUE)

In the diagram below it is shown a situation where the polling CPU core is selecting another CPU for packet processing.

This would be the case for MPLSoGRE traffic, since the hash performed by the NIC is likely not efficient :

![DPDK Contrail vRouter packet walk-through from NIC to DPDK guest](data:image/png;base64;base64,)

DPDK Contrail vRouter packet walk-through from NIC to DPDK guest

### step 3: Forwarding core (MPLSoUDP/VxLAN)

In previous stage polling CPU bound to the queue on which a packet has been received, is triggering packet transfer from given NIC RX queue to mbuf.

This CPU (here CPU 0) will also choose which CPU (forwarding CPU) will have to process the packet (decapsulation, routing, switching, etc).

But as incoming encapsulated packets are using UDP protocol, a good entropy is expected for incoming encapsulated traffic. **No hash is recalculated on the polling core, and each incoming packet will be processed on the same forwarding core than the polling one.**

In the diagram below, it is shown a situation where the polling CPU core is the same as the forwarding CPU, which will be the case for MPLSoUDP and VXLAN packets from the NIC:

![DPDK Contrail vRouter packet walk-through from NIC to DPDK guest](data:image/png;base64;base64,)

DPDK Contrail vRouter packet walk-through from NIC to DPDK guest

When MPLS over UDP is used, there is internal traffic load balancing onto vrouter CPU. Incoming packets are processed with the same forwarding core as polling core :

![ingress MPLS over UDP traffic forwarding](data:image/png;base64;base64,)

ingress MPLS over UDP traffic forwarding

It can be easily shown using a traffic generator to send a "single UDP" flow onto a virtual instance.

When single UDP flow is reaching the vrouter, RX port packets and RX packets counters on vif 0/0 have the same values for a same lcore: Here the VM incoming traffic is polled and processed by core 12:

![UDP flow: polling CPU is same as forwarding CPU](data:image/png;base64;base64,)

UDP flow: polling CPU is same as forwarding CPU

Table above has been made using real single flow traffic seen on each vif 0/0 and vif 0/3 interface (vNIC) with vif --get command (cf appendixes)

how is this neat output captured?

* <https://github.com/PrzemekGrygiel/DPDKstats>
* <https://drive.google.com/open?id=1mhxzRlulBqo3SfbGOywy2smG-NdC5dVN>

## DPDK VM outgoing traffic

vRouter forwarding threads are also responsible for polling virtio interface queues. The decision which thread will poll which virtio queue is made by Contrail DPDK vRouter.

If VM uses multiqueue then more vRouter forwarding threads (CPU cores) will be engaged in receiving packets from a single VM.

![DPDK Contrail vRouter packet walk-through from DPDK guest to NIC](data:image/png;base64;base64,)

DPDK Contrail vRouter packet walk-through from DPDK guest to NIC

* The packet is placed on a vNIC TX queue (vRouter vif RX queue) by the Virtual machine.
* A given vNIC TX queue is always polled by the same vRouter logical core.
* A round robin algorithm (described in next section) is used to assign vNIC queues to logical cores.
* vNIC sub-interfaces are sharing TX/RX queues with their parent interface. Hence the same logical core is polling these queues.

Then, the incoming packet is dequeued by the polling logical core (step 1) :

* vRouter polling logical core in charge of that queue reads the packet header,
* computes a hash, and selects a vRouter processing logical core based on the hash.

ping? confusing: #2 and #3 statements are conflicting

A (LD):

Not very well described indeed.

Step 2 is done during vnic life (how each packet is processed)

Step 3 is done once … at vnic plugin on vrouter

no 1x1 mapping between vNIC queue and forwarding threads? as with pNIC?

Yes, there is. But you have 2 cases to consider. SingleQ and MultiQ NIC. Also, there is a balancing mechanism in order to attach queue0 of each NIC not on a same CPU ( Cf: vNIC queues - Polling Core Assignment (R1910) )

Here, multiQ case:

Each CPU is bound to a Q : ![image](data:image/png;base64;base64,)

But it is only part of the full view. You have to consider each direction … and type of traffic.

See my drawings.

### step 1: polling core

**polling core assignment for vNIC queues (R1910).**

**ping: very confused**

vNIC queues are assigned to logical cores in the following way:

* The forwarding core that is currently polling the least number of queues is selected, with a tie won by the core with the lowest number (the first forwarding core is lcore 10)
* A queue is created for each forwarding core, starting with the least used core and wrapping around to the start of the forwarding cores after the maximum is reached. However, only the first queue is actually enabled. All of the other queues will only be used if the VM supports multiqueue and enables them.
* If the VM supports multiqueue, then it enables the additional queues, at which point they are mapped to the forwarding core they were assigned when they were created.

Log messages showing this process can be seen in the /var/log/containers/contrail/contrail-vrouter-dpdk.log file.

2020-01-22 13:53:28,385 VROUTER: lcore 11 RX from HW queue 0  
2020-01-22 13:53:28,385 VROUTER: lcore 12 RX from HW queue 1  
2020-01-22 13:53:28,385 VROUTER: lcore 13 RX from HW queue 2  
2020-01-22 13:53:28,385 VROUTER: lcore 14 RX from HW queue 3  
2020-01-22 13:53:28,385 VROUTER: lcore 15 RX from HW queue 4  
2020-01-22 13:53:28,385 VROUTER: lcore 10 RX from HW queue 5

**When interface is added and the queue to forwarding core mappings are made.** There are six forwarding cores in this setup. Only the first queue is actually enabled at this point.

The remaining queues will use the mentioned forwarding cores if the VM chooses to enable them (i.e. it supports multiqueue).

2020-01-22 14:02:44,060 UVHOST: Client \_tap4966ea8d-49: setting vring 0 ready state 1  
2020-01-22 14:02:44,060 UVHOST: Client \_tap4966ea8d-49: setting vring 1 ready state 1  
2020-01-22 14:02:44,060 UVHOST: Client \_tap4966ea8d-49: setting vring 2 ready state 1  
2020-01-22 14:02:44,060 UVHOST: Client \_tap4966ea8d-49: setting vring 3 ready state 1  
2020-01-22 14:02:44,060 UVHOST: Client \_tap4966ea8d-49: setting vring 4 ready state 1  
2020-01-22 14:02:44,060 UVHOST: Client \_tap4966ea8d-49: setting vring 5 ready state 1  
2020-01-22 14:02:44,060 UVHOST: Client \_tap4966ea8d-49: setting vring 6 ready state 1  
2020-01-22 14:02:44,060 UVHOST: Client \_tap4966ea8d-49: setting vring 7 ready state 1  
2020-01-22 14:02:44,061 UVHOST: Client \_tap4966ea8d-49: setting vring 8 ready state 0  
2020-01-22 14:02:44,061 UVHOST: Client \_tap4966ea8d-49: setting vring 9 ready state 0

**When a VM (in this case a vSRX) requests to enable some of its available queues.** The vrings here correspond to both transmit and receive queues.

The receive queues are the odd numbers. Divide them by 2 (discard the remainder) to get the queue number. i.e. vring 1 is queue 0. ready state 1 = enabled. ready state 0 = disabled. In this example, the vSRX is only enabling 4 queues:

### step 2: RSS

Hashing algorithm is in vr\_dpdk\_ethdev.c module <https://github.com/Juniper/contrail-vrouter/blob/R5.0/dpdk/vr_dpdk_ethdev.c#L873>

RSS hashing depends on the packet type:

* for non-UDP/TCP IP packets (except GRE), a 2-tuple is used for the hash: source IP address, destination IP address
* for GRE, a hash is done using the source IP address and destination IP address, followed by a hash for the GRE key if present
* for TCP or UDP IP packets (IPv4 or IPv6), a hash is done for the source IP address and destination IP address followed by a hash for the source port and destination port
* Ethernet information is not taken into consideration for hash computation:
  + VLAN tag (eg if a sub-interface is used), are **not** used for the hash
  + source and destination MAC addresses are **not** used for the hash
* Non-IPv4/IPv6 packets (i.e. L2 packets) will **not** have a hash performed and will be processed by their polling core.

### step 3: forwarding core

When polling CPU core (in the above example CPU core 3) polls the packet from VM virtio interface queue it selects which forwarding CPU core will process the incoming packet. This forwarding CPU core does flow lookup, flow enforcement, encapsulation and packet delivery to NIC transmit queue.

Then forwarding logical core is processing the packet (step 2). Forwarding CPU is in charge to do :

* flow lookup,
* flow enforcement (switching, routing, NAT, packet transformation)
* encapsulation,
* packet delivery to physical NIC TX queue

For VM incoming traffic a hash is calculated in order to rebalance received traffic on a given polling core to all other forwarding cores :

![egress traffic coming from VM](data:image/png;base64;base64,)

egress traffic coming from VM

It can be easily shown using a traffic generator to send a "single UDP" flow onto a virtual instance.

When single UDP flow is reaching the vrouter, RX port and RX packets counters on vif 0/N have the same values for distinct lcores.

Here the VM incoming traffic is polled by core 13 and processed by core 11:

![egress flow: polling CPU is different as forwarding CPU](data:image/png;base64;base64,)

egress flow: polling CPU is different as forwarding CPU

Table above has been made using real single flow traffic seen on each vif 0/0 and vif 0/3 interface (vNIC) with vif --get command (cf appendixes)

regarding RX port and RX packet, see [Packet flow from a VM NIC to compute node Physical NIC - counters placement](#X06539e05c84c796f4744216df850f7445a35cd7)

this is different than ingress traffic received from pNIC - only MPLSoGRE traffic will use a different forwarding thread than polling thread.

Yes, and this is something that will change in next releases. To be discussed with Kiran and Premecz. It seems we will provide the ability to disable this hash calculation done at vrouter level to rebalance polled packets onto different CPU to be processed.

## Packet Flow Summary (Based on R1910)

|  |  |  |
| --- | --- | --- |
| **Packet Origination** | **Packet Type** | **Action** |
| pNIC | IPv4 MPLSoUDP or VXLAN | Processed by polling core |
|  | IPv4 MPLSoGRE - Inner packet is IPv4 or IPv6 | Distributed to a different processing core based on hash of inner packet. |
|  | IPv4 MPLSoGRE - Inner packet not IPv4 or IPV6 | Processed by polling core. |
| vNIC | IPv4 MPLSoGRE - Inner packet is iPv4 or IPV6 | Distributed to a different processing core based on hash of inner packet. |
|  | IPv4 MPLSoGRE - Inner packet not IPv4 or IPv6 | Processed by polling core |
|  | All other IPv4 packets | Distributed to a different processing core based on hash of packet. |
|  | All IPv6 packets | Distributed to a different processing core based on hash of packet. |
|  | All non-IPv4/IPv6 packets (i.e. L2 packets) | Processed by polling core |

whenever the polling core performs a hash to distribute the packet to a processing core, the polling core will never select itself to process the packet.

why diff between vNIC and pNIC? when pNIC got MPLSoUDP (just a UDP packet anyway), it do RSS hashing and put in differnet pNIC queue → diff polling core, so polling core does not need to hash again and just processed it. why vNIC do it differently? vNIC got UDP packet from VM, it should again do hash and place it into different queue, so different polling core will just poll and process it. why distribute to other cores here?

First, I think this provided matrix has to be discussed and revised. Personally I do not understand this concept of “IPv4 MPLSoGRE” when packet is originated onto a vNIC.

My understanding is this situation :

Incoming packets from Physical NIC

|  |  |  |
| --- | --- | --- |
| Outer packet Type | Inner packet type | Action |
| IPv4 MPLSoUDP or VXLAN | any | Polling = Processing core (single hash) |
| IPv4 MPLSoGRE | IP (v4 or v6) | Polling != Processing core (two hash calc.) |
|  | Not IP (Ethernet Frame for instance) | Polling = Processing core (single hash) |
| IPv4 | Not encapsulated (like XMPP messages) | ?? |

Incoming packets from Virtual NIC

|  |  |
| --- | --- |
| Packet type | Action |
| IP (v4 or v6) | Polling != Processing core (two hash calc.) |
| Not IP (Ethernet Frame for instance) | Polling = Processing core (single hash) |

Second: Why all this complex stuff ?

This is (it was) required by poor entropy situations:

* MPLS GRE encapsulation (incoming traffic from other baremetal computes)
* SingleQ VM (incoming traffic from virtual instances)

In both situations only 1 polling core is selected. So it is useless to allocate lots of CPU onto your vrouter if due to poor entropy / or single Q VM, you are using only one core.

This is why Contrail has created a mechanism to spread the load on all CPU. This mechanism consist in different hash calculation in order to select another CPU for processing.

This was a nice solution till, GRE was the main encapsulation protocol supported and most of DPDK VM were single Q.

But now, as most of our customers are using UDP encapsulation protocols and MultiQ VNF, this old nice mechanism is really a drawback. It brings an additional calculation and an additional queuing steps that is badly impacting vrouter performances.

This is why in next release the idea is to propose a setup in which all packets are polled and processed by the same CPU. It will be worth to use this new setup when your VNF are MultiQ and when using UDP encapsulations.

The selection of available processing cores for each polling core can be seen in the /var/log/containers/contrail/contrail-vrouter-dpdk.log file.

2020-01-07 13:08:01,403 VROUTER: Lcore 10: distributing MPLSoGRE packets to [11,12,13,14,15]  
2020-01-07 13:08:01,403 VROUTER: Lcore 12: distributing MPLSoGRE packets to [10,11,13,14,15]  
2020-01-07 13:08:01,403 VROUTER: Lcore 14: distributing MPLSoGRE packets to [10,11,12,13,15]  
2020-01-07 13:08:01,403 VROUTER: Lcore 11: distributing MPLSoGRE packets to [10,12,13,14,15]  
2020-01-07 13:08:01,404 VROUTER: Lcore 13: distributing MPLSoGRE packets to [10,11,12,14,15]  
2020-01-07 13:08:01,404 VROUTER: Lcore 15: distributing MPLSoGRE packets to [10,11,12,13,14]

It mentions MPLSoGRE, but this applies to all packets that are distributed via hashing by the polling core:

## **Non DPDK VM** on DPDK vrouter

* When sending packets from NIC to non-DPDK VM, DPDK vRouter raises an interrupt in the guest.
* This is an additional step after copying the packet to that VM.
* The interrupt is only needed because the VM is not polling for packets.
* The vRouter writes to a file descriptor, which tells the kernel to raise an interrupt to non-DPDK VM.
* The file descriptor is sent by Qemu to vrouter when the VM is spawned.
* Also note that an Interrupt is raised for a burst of packets, not for every packet.

To avoid interrupts raised by DPDK vRouter (required to raise packet processing by QEMU/KVM) that influence packets processing Juniper recommends to only connect DPDK VMs and DPDK interfaces to DPDK vRouter.

Putting non-DPDK VMs on a DPDK node is affecting performance of both VM and vRouter:

* VM performance is impacted because each interrupt raised would cause a "VMExit" (it has a very bad impact on performance)
* vRouter performance is also impacted since it needs to do additional work of "raising an interrupt" after it enqueues the packet to the vNIC Ring.

**As a result of these, the performance numbers would be the similar as that of kernel vRouter.**

1. When the VM is spawned, QEMU registers an fd (file descriptor) for the guest (irqfd) and passes to the backend (vRouter). The guest listens to this fd for changes to process the packets.
2. registration mechanism for this fd is provided by KVM kernel module. This is KVM module that actually provides a wait-notify mechanism between the guest and the backend (vRouter)
3. virtual machine is setting a flag VRING\_AVAIL\_F\_NO\_INTERRUPT into VirtIO ring by which vRouter will be aware it needs to notify the Guest VM that a packet has been delivered (this flag is not set when VM is using DPDK).
4. once the vRouter gets hold of this fd, all it needs to do is to enqueue the packets to the virtio ring and write to that fd.
5. KVM injects this event to the VM as an interrupt. In this process, the VM needs a 'VMExit'
6. VMExit latency is very high (around 10K clock cycles). This is further compounded by the NAPI latency. It has a very bad impact on VM performance. vRouter performance is also impacted due to the extra work of writing to the fd (which interrupts the guest).

## **vNIC queues**

In the case of DPDK vrouter, the support for multiqueue virtio is available from Contrail 3.1 onwards.

![vNIC single queue vs multiqueue](data:image/png;base64;base64,)

vNIC single queue vs multiqueue

### Single queue virtIO

The network performance does not scale as the number of vCPUs increases.

Guest cannot transmit or retrieve packets in parallel as virtio-net have only one TX and RX. virtio-net drivers must be synchronized before sending and receiving packets.

It is useless to assign more CPU to vrouter in order to increase packet processing rate, as only one vrouter CPU is used to poll the single vNIC queue.

Moreover, all vrouter CPU could have a packet to transmit to the vNIC single queue which is becoming a congestion point.

If we add more CPU, we increase the pressure on the vNIC single queue and it could lead to jitter and even packet drop (buffer overflow).

### Multiqueue virtIO

**CPU assigned for Multiqueue and virtIO.**

When multiqueue is used on a Guest VM, In the ideal scenario, each multiqueue vNIC is configured with the same number of queue than the number of CPU allocated to vrouter for packet processing, because the vrouter will only be able to sustain guest vNIC configured with a number of queue below or equal to the number for processing core allocated to the vrouter. The difference with non-DPDK is that vRouter runs in the user space instead of host kernel.

Also there is a vhost userspace process wherein the vRouter copies packets to/from the VM.

Every queue inside the VM maps to a virtio ring on the host user space.

![vNIC multiqueue](data:image/png;base64;base64,)

vNIC multiqueue

Some of the offload capabilities, e.g. GRO (Generic Receive Offload), is not supported with multiqueue virtio on DPDK vrouter in Contrail 3.2.

**DPDK Multiqueue packet walk-through.**

In this case vRouter runs as a multi-core process that exists on all assigned cores.

There is also a scale-out approach to packet processing using multiple cores so the performance of one VM is NOT limited by the performance of 1 core.

**traffic to VM.**

A vRouter might have more cores than there are queues in the VM. Queues can only be shared when the vRouter cores send to the VM queue.

**traffic from VM.**

When receiving from the queue, exactly one vRouter core will read from a queue (***i.e. receive queues are not shared, in order to prevent packet reordering***).

**3.2 lab.**

root@bcomp79:~# ps aux | grep vhost-  
root 1737 0.0 0.0 0 0 ? S 15:20 0:00 [vhost-1734]  
root 1738 0.0 0.0 0 0 ? S 15:20 0:00 [vhost-1734]  
root 1739 0.0 0.0 0 0 ? S 15:20 0:00 [vhost-1734]

**ping? this "vhost userspace process" is kernel vrouter only?.**

A (LD):

In my opinion we have to explain:

* DPDK vrouter is running in user space (this is the goal of DPDK)
* Kernel vouter dataplane is running in Kernel space (vrouter.ko module)

But afer, this kernel/user space has not only to be considered at vrouter level. You aslo have to consider the virtualization layer:

* what about virtio (QEMU capaability) ?
* what about the VM itself (using DPDK or not) ?

QEMU, few years ago was not able to run in userspace. So, it was creating performance issue when used with DPDK applications.

VNF, were also running Kernel packet processing stack

Drawback is interupt mechanisms it required that is slowering packet processing and Kernel to User context swap (which is CPU intensive) is requires.

Nowaday, lots of VNF are DPDK and QEMU is supporting lots of scenarios.

Ideal situation is to get everything running at userspace level:

* DPDK vrouter
* DPDK VNF (multiQ - same number of Q than vrouter)
* virtio also running in user space (vhost-user)

All these situations are described in this diagram:

![image](data:image/png;base64;base64,)

The last drawing at right is the best situation and the one that is providing the best performance.

The worst is the first diagram at left. Both diagrams in the middle are providing drawbacks:

* When DPDK VM is used onto a Kernel vRouter, vrouter will will slow down packet processing
* When Kernel VM is used onto a DPDK vrouter, Kernel VM will slow down packet processing

So, this is a pity situation to mix DPDK and not-DPDK element (but sometimes it can’t be avoided)

So, we have to explain that vrouter can’t solve everything. Part of the job has to be done at VNF layer.

**In my opinion, the main goal of this book is to explain the (nowadays) optimal situation:**

* DPDK vrouter
* UDP overlay protocol (MPLSoUDP or VxLAN)
* 200X release: with 2 hash mechanism disabled (discuss with Kiran and Premecz about X)
* DPDK VNF (multiQ – with same number of Q than vrouter)

### vNIC queues "queue size" configuration (RedHat OpenStack)

vNIC queues are not configured by Contrail vRouter, they are managed by OpenStack. Rqueue Size are defined at OpenStack level (using libvirt) : /etc/nova/nova.conf

# Configure virtio rx queue size.  
# This option is only usable for virtio-net device with vhost and  
# vhost-user backend. Available only with QEMU/KVM. Requires libvirt  
# v2.3 QEMU v2.7. (integer value)  
# Possible values:  
# 256 - <No description provided>  
# 512 - <No description provided>  
# 1024 - <No description provided>  
#rx\_queue\_size=<None>  
  
# Configure virtio tx queue size.  
# This option is only usable for virtio-net device with vhost-user  
# backend. Available only with QEMU/KVM. Requires libvirt v3.7 QEMU  
# v2.10. (integer value)  
# Possible values:  
# 256 - <No description provided>  
# 512 - <No description provided>  
# 1024 - <No description provided>  
#tx\_queue\_size=<None>

Nova configuration file values are provisioned with TripleO.

vNIC queues size can be defined using NovaLibvirtRxQueueSize and NovaLibvirtRxQueueSize environment parameters. By default they are configured with a 512 value.

Nova configuration file is configured with <tripleo-templates-root-dir>/puppet/services/nova-compute.yaml file:

NovaLibvirtRxQueueSize:  
 description: >  
 virtio-net RX queue size. Valid values are 256, 512, 1024  
 default: 512  
 type: number  
 constraints:  
 - allowed\_values: [ 256, 512, 1024 ]  
 tags:  
 - role\_specific  
 NovaLibvirtTxQueueSize:  
 description: >  
 virtio-net TX queue size. Valid values are 256, 512, 1024  
 default: 512  
 type: number  
 constraints:  
 - allowed\_values: [ 256, 512, 1024 ]

### vNIC queues "queue number" configuration (RedHat OpenStack)

**Enable Multiqueue on OpenStack instances.**

To enable multiqueue with DPDK in a Glance image, we add metadata hw\_vif\_multiqueue\_enabled="true":

openstack image set --property hw\_vif\_multiqueue\_enabled="true" [image name or ID]

**number of vNIC queues.**

Number of queues to be created can’t be specified with Glance metadata. Currently, the number of queues will match the number of vCPUs, defined for the instance.

**Nova is configuring automatically the number of queues of each vNIC. There is no way to manually define the number of queues to be created for each vNIC.** We can only change the number of queues of a given vNIC after the virtual instance has been started, using some Linux commande into the virtual machine whose vNIC configuration has to be modified (cf next section).

Nova is using vif.py script to create instance virtual interfaces (<https://github.com/openstack/nova/blob/master/nova/virt/libvirt/vif.py>)

Number of configured queues for a vif is depending on:

* Compute node kernel release
* Number of vCPU configured onto the virtual instance

**kernel 3.x.**

When a Linux Kernel 3.x is used (RHOSP 13), a maximum of 8 queues are configured by Nova for each vif.

* when an instance is configured with 8 or less vCPUs: the number of queues configured on its multiqueues vif is equal to the number of vCPU.
* when an instance is configured with more than 8 vCPUs: the number of queues configured on its multiqueues vif is equal 8

**kernel 4.x.**

When a Linux Kernel 4.x is used (RHOSP 16), the same algorithm is used but using 256 instead of 8 as a maximum of queues to be configured by each vif.

$ vi /usr/lib/python2.7/site-packages/nova/virt/libvirt/vif.py  
...  
 def \_get\_max\_tap\_queues(self):  
 # NOTE(kengo.sakai): In kernels prior to 3.0,  
 # multiple queues on a tap interface is not supported.  
 # In kernels 3.x, the number of queues on a tap interface  
 # is limited to 8. From 4.0, the number is 256.  
 # See: https://bugs.launchpad.net/nova/+bug/1570631  
 kernel\_version = int(os.uname()[2].split(".")[0])  
 if kernel\_version <= 2:  
 return 1  
 elif kernel\_version == 3:  
 return 8  
 elif kernel\_version == 4:  
 return 256  
 else:  
 return None  
...

### vNIC queues "queue number" changing

Inside an guest instantiated guest with multiqueues enabled, the NIC channel setup can be checked and changed as needed with the commands below, **inside each virtual machine**.

In order to see the current number of queues we have to use :

ethtool -l [nic name]

In order to change the number of queues we have to use :

ethtool -L [nic name] combined [number of queues]

For instance, below we are configuring 4 logical queues on eth0 vNIC :

ethtool -L eth0 combined 4

This should be done during interface initialization, for example in a "pre-up" action in /etc/network/interfaces. But it seems to be possible to change this configuration on a running interface without disruption.

**ping: lab.**

[root@perf-test1-swap ~]# ethtool -l eth1  
Channel parameters for eth1:  
Pre-set maximums:  
RX: 0  
TX: 0  
Other: 0  
Combined: 7 #<---  
Current hardware settings:  
RX: 0  
TX: 0  
Other: 0  
Combined: 7 #<---

### vNIC queues verfication

Using virsh dumpxml command, we can verify queue size configured by Nova with libvirt :

virsh dumpxml [vm id]  
...  
<interface type='ethernet'>  
 <model type='virtio'/>  
 <driver name='vhost' queues='5' rx\_queue\_size='1024' tx\_queue\_size='1024'/>  
</interface>  
...

Here, 5 queues have been allocated to the vNIC, rx/tx\_queue\_size is configured as 1024.

ping? interface type should be vhostuser?

A (LD): This is something that is not fully clear for me. When is use OVS DPDK I clearly see that VM interfaces are vhost user. To be clarified with Kiran and Premecz.

**ping: 3.2 lab: no queue configured.**

<interface type='vhostuser'>  
 <mac address='02:0c:e2:8e:2d:c1'/>  
 <source type='unix' path='/var/run/vrouter/uvh\_vif\_tap0ce28e2d-c1' mode='client'/>  
 <model type='virtio'/>  
 <address type='pci' domain='0x0000' bus='0x00' slot='0x03' function='0x0'/>  
</interface>

**ping: 1908 lab.**

[root@overcloudmz5-compdpdk-3 ~]# virsh edit 1  
Domain instance-000005ed XML configuration not changed.  
  
<interface type='vhostuser'>  
 <mac address='02:0a:8d:a2:c1:db'/>  
 <source type='unix' path='/var/run/vrouter/uvh\_vif\_tap0a8da2c1-db' mode='server'/>  
 <model type='virtio'/>  
 <driver queues='7' rx\_queue\_size='512' tx\_queue\_size='512'/>  
 <address type='pci' domain='0x0000' bus='0x00' slot='0x03' function='0x0'/>  
</interface>  
<interface type='vhostuser'>  
 <mac address='02:78:77:5a:56:43'/>  
 <source type='unix' path='/var/run/vrouter/uvh\_vif\_tap78775a56-43' mode='server'/>  
 <model type='virtio'/>  
 <driver queues='7' rx\_queue\_size='512' tx\_queue\_size='512'/>  
 <address type='pci' domain='0x0000' bus='0x00' slot='0x04' function='0x0'/>  
</interface>

### Multiqueue known limitations

#### Number of queues on VM instances

Number of queues configured on virtual instances collected by the vrouter **must be below or equal to the number of queues configured on the vrouter** (aka number of CPU assigned to vrouter for packet processing).

If more queues are configured on the instance side than on the vrouter side, following messages will be seen into the vrouter dpdk logs :

2019-09-24 16:36:50,011 VROUTER: Adding vif 8 (gen. 37) virtual device tap66e68bc1-a9  
2019-09-24 16:36:50,012 VROUTER: lcore 12 TX to HW queue 0  
2019-09-24 16:36:50,012 VROUTER: lcore 13 TX to HW queue 1  
2019-09-24 16:36:50,012 VROUTER: lcore 8 TX to HW queue 2  
2019-09-24 16:36:50,012 VROUTER: lcore 9 TX to HW queue 3  
2019-09-24 16:36:50,012 VROUTER: lcore 10 TX to HW queue 4  
2019-09-24 16:36:50,012 VROUTER: lcore 11 TX to HW queue 5  
2019-09-24 16:36:50,012 VROUTER: lcore 12 RX from HW queue 0  
2019-09-24 16:36:50,012 VROUTER: lcore 13 RX from HW queue 1  
2019-09-24 16:36:50,012 VROUTER: lcore 10 RX from HW queue 2  
2019-09-24 16:36:50,012 VROUTER: lcore 11 RX from HW queue 3  
2019-09-24 16:36:50,012 UVHOST: Adding vif 8 virtual device tap66e68bc1-a9  
2019-09-24 16:36:50,012 UVHOST: vif (server) 8 socket tap66e68bc1-a9 FD is 173  
......  
2019-09-24 16:37:46,692 UVHOST: Client \_tap66e68bc1-a9: handling message 18  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: setting vring 0 ready state 1  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: handling message 18  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: setting vring 1 ready state 1  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: handling message 18  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: setting vring 2 ready state 0  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: handling message 18  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: setting vring 3 ready state 0  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: handling message 18  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: setting vring 4 ready state 0  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: handling message 18  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: setting vring 5 ready state 0  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: handling message 18  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: setting vring 6 ready state 0  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: handling message 18  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: setting vring 7 ready state 0  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: handling message 18  
2019-09-24 16:37:46,693 UVHOST: vr\_uvhm\_set\_vring\_enable: Can not disable TX queue 4 (only 4 queues)  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: handling message 18  
2019-09-24 16:37:46,693 UVHOST: vr\_uvhm\_set\_vring\_enable: Can not disable RX queue 4 (only 4 queues)  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: handling message 18  
2019-09-24 16:37:46,693 UVHOST: vr\_uvhm\_set\_vring\_enable: Can not disable TX queue 5 (only 4 queues)  
2019-09-24 16:37:46,693 UVHOST: Client \_tap66e68bc1-a9: handling message 18  
2019-09-24 16:37:46,693 UVHOST: vr\_uvhm\_set\_vring\_enable: Can not disable RX queue 5 (only 4 queues)  
......  
019-09-24 16:40:58,250 UVHOST: vr\_uvhm\_set\_vring\_enable: Can not enable TX queue 7 (only 4 queues)  
2019-09-24 16:40:58,250 UVHOST: Client \_tap3c0c41f1-66: handling message 18  
2019-09-24 16:40:58,250 UVHOST: vr\_uvhm\_set\_vring\_enable: Can not enable RX queue 7 (only 4 queues)

Here we have a vrouter configured with 4 forwarding cores (= 4 queues) but the collected VM is configured with 8 queues. Queues 4 to 7 won’t be processed by the vrouter.

#### Indirect descriptors are not supported

Contrail does not support indirect buffer descriptors (VIRTIO\_RING\_F\_INDIRECT\_DESC). Cf: <https://spp-tmp.readthedocs.io/en/stable/rel_notes/release_16_11.html>

So, indirect\_desc field is set to false in QEMU interface setup :

[heat-admin@xxxx ~]$ sudo docker exec -it c149193e4a14 virsh qemu-monitor-command 1 --hmp info qtree  
bus: main-system-bus  
 type System  
 dev: kvm-ioapic, id ""  
 gpio-in "" 24  
 gsi\_base = 0 (0x0)  
 mmio 00000000fec00000/0000000000001000  
 dev: i440FX-pcihost, id ""  
 pci-hole64-size = 2147483648 (2 GiB)  
 short\_root\_bus = 0 (0x0)  
 x-pci-hole64-fix = true  
 bus: pci.0  
 type PCI  
 ...  
 dev: virtio-net-pci, id "net1"  
 ioeventfd = true  
 vectors = 18 (0x12)  
 virtio-pci-bus-master-bug-migration = false  
 ...  
 bar 1: mem at 0xfebd2000 [0xfebd2fff]  
 bar 6: mem at 0xffffffffffffffff [0x3fffe]  
 bus: virtio-bus  
 type virtio-pci-bus  
 dev: virtio-net-device, id ""  
 csum = true  
 rx\_queue\_size = 1024 (0x400)  
 tx\_queue\_size = 1024 (0x400)  
 host\_mtu = 0 (0x0)  
 x-mtu-bypass-backend = true  
 speed = -1 (0xffffffffffffffff)  
 duplex = ""  
 indirect\_desc = false  
 event\_idx = false  
 notify\_on\_empty = false  
 any\_layout = false  
 iommu\_platform = false  
 \_\_com.redhat\_rhel6\_ctrl\_guest\_workaround = false  
 ...

# **huge pages**

## Huge pages configuration

* DPDK vrouter is using hugepages. Huge pages need to be configured before it can be used.
* Only smaller (2MB) pages can be configured using sysctl, but 1GB pages are strongly recommended, so the only consistent way of configuration is to add parameters to linux kernel.
* Allocating huge pages should be done based on the prediction of how many VMs (their amount of memory) will be used on a hypervisor + 2GB for vRouter for default configuration.
* Of course some memory need to be left for operating system and other processes.

When using 2MB hugepages, the amount configured cannot be bigger than 32768. If more pages are configured, vrouter-dpdk will not start. This is a limitation of DPDK library.

In RHEL environment, to make vrouter-dpdk work with 1G hugepages, a small amount of 2MB hugepages needs to be declared too (128 pages is enough).

**configure huge pages.**

The following kernel parameters configure huge pages:

default\_hugepagesz=1GB hugepagesz=1G hugepages=40 hugepagesz=2M hugepages=40

default\_hugepagesz

defines default huge page size (this size will appear in /proc/meminfo, and this size will be mounted by default when pagesize mounting option will not be used)

hugepagesz

followed by hugepages defines size and amount respectively, the pair can be repeated to configure different sizes of huge pages.

To finish configuration of hugepages, hugetlbfs pseudo filesystem needs to be mounted. The following line needs to be added to /etc/fstab:

hugetlbfs on /dev/hugepages type hugetlbfs (rw,relatime,seclabel)

**checking huge pages.**

After adding the configuration to a kernel and rebooting server, the number of allocated huge pages can be checked from command line. There are multiple ways of doing this, The most common way of doing it is to print /proc/meminfo. This is not a good way, because it shows only one (default) huge page size. Since it is possible to configure multiple sizes of hugepages, the only source of information is /sys filesystem (for each numa node and each size - total/free):

# more /sys/devices/system/node/node0/hugepages/hugepages-\*/\* | cat

**3.2 lab.**

$ cat /proc/meminfo | grep -i page  
AnonPages: 23169520 kB  
PageTables: 60296 kB  
AnonHugePages: 22657024 kB  
HugePages\_Total: 48300  
HugePages\_Free: 43397  
HugePages\_Rsvd: 0  
HugePages\_Surp: 0  
Hugepagesize: 2048 kB #<---

**1908 lab.**

[root@overcloudmz5-compdpdk-3 ~]# cat /proc/meminfo | grep -i huge  
AnonHugePages: 8192 kB  
HugePages\_Total: 64  
HugePages\_Free: 44  
HugePages\_Rsvd: 0  
HugePages\_Surp: 0  
Hugepagesize: 1048576 kB

**3.2 lab.**

$ more /sys/devices/system/node/node0/hugepages/hugepages-\*/\* | cat  
::::::::::::::  
/sys/devices/system/node/node0/hugepages/hugepages-2048kB/free\_hugepages  
::::::::::::::  
19759  
::::::::::::::  
/sys/devices/system/node/node0/hugepages/hugepages-2048kB/nr\_hugepages  
::::::::::::::  
24150  
::::::::::::::  
/sys/devices/system/node/node0/hugepages/hugepages-2048kB/surplus\_hugepages  
::::::::::::::  
0

**1908 lab.**

[root@overcloudmz5-compdpdk-3 contrail]# more /sys/devices/system/node/node0/hugepages/hugepages-\*/\* | cat  
::::::::::::::  
/sys/devices/system/node/node0/hugepages/hugepages-1048576kB/free\_hugepages  
::::::::::::::  
13  
::::::::::::::  
/sys/devices/system/node/node0/hugepages/hugepages-1048576kB/nr\_hugepages  
::::::::::::::  
32  
::::::::::::::  
/sys/devices/system/node/node0/hugepages/hugepages-1048576kB/surplus\_hugepages  
::::::::::::::  
0  
::::::::::::::  
/sys/devices/system/node/node0/hugepages/hugepages-2048kB/free\_hugepages  
::::::::::::::  
4096  
::::::::::::::  
/sys/devices/system/node/node0/hugepages/hugepages-2048kB/nr\_hugepages  
::::::::::::::  
4096  
::::::::::::::  
/sys/devices/system/node/node0/hugepages/hugepages-2048kB/surplus\_hugepages  
::::::::::::::  
0

**3.2 lab.**

$ cat /etc/fstab  
# /etc/fstab: static file system information.  
#  
# Use 'blkid' to print the universally unique identifier for a  
# device; this may be used with UUID= as a more robust way to name devices  
# that works even if disks are added and removed. See fstab(5).  
#  
#<file system> <mount point> <type> <options> <dump> <pass>  
/dev/mapper/VG--bcomp78-root / ext4 errors=remount-ro 0 1  
#/dev/mapper/VG--bcomp78-home /home ext4 defaults 0 2  
/dev/mapper/VG--bcomp78-home /mnt ext4 defaults 0 2  
/dev/mapper/VG--bcomp78-swap none swap sw 0 0  
hugetlbfs /hugepages hugetlbfs defaults 0 0

**1908 lab.**

[root@overcloudmz5-compdpdk-3 ~]# cat /etc/fstab  
#<file system> <mount point> <type> <options> <dump> <pass>  
LABEL=img-rootfs / xfs defaults 0 1  
none /dev/hugepages1G hugetlbfs pagesize=1G 0 0  
none /dev/hugepages2M hugetlbfs pagesize=2M 0 0

## hugepages for vrouter: --socket-mem

As mentioned before, DPDK vRouter needs its own hugepages. The DPDK library auto-detects the huge pages from the hugetlbfs mount point.

2GB for vRouter are based on setup provided in configuration file.

In order to allocate memory on the first NUMA socket, we are using option with only one parameter:

--socket-mem <value>

In order to allocate memory on the NUMA0 and NUMA1 socket, we are using option with only two parameters:

--socket-mem <value>,<value>

/etc/contrail/supervisord\_vrouter\_files/contrail-vrouter-dpdk.ini  
[program:contrail-vrouter-dpdk]  
command=/usr/bin/taskset 0x154000000154 /usr/bin/contrail-vrouter-dpdk --no-daemon --vr\_flow\_entries=2000000 --vdev "eth\_bond\_bond0,mode=4,xmit\_policy=l34,socket\_id=0,mac=90:e2:ba:c5:79:90,slave=0000:01:00.0,slave=0000:01:00.1,slave=0000:02:00.0,slave=0000:02:00.1" --socket-mem 1024,1024

--socket-mem 1024,1024

means allocate 1GB memory (in huge pages) per NUMA node for vRouter (here we assume 2 NUMA nodes).

On a 2 NUMA nodes we have to allocate memory on each of them even if vRouter is only pinned on a single one. Indeed Virtual machines are pinned on both and require memory on each. It is important to allocate hugepage memory to all NUMA nodes that will have DPDK interfaces associated with them. If memory is not allocated on a NUMA node associated with a physical NIC or VM, they cannot be used.

If you are using 2 or more ports from different NICs, it is best to ensure that these NICs are on the same CPU socket.

![Hugepage memory and NUMA sockets](data:image/png;base64;base64,)

Hugepage memory and NUMA sockets

We can get all PCI Ethernet devices installed on the host using the following command :

# lspci -nn | grep Eth  
18:00.0 Ethernet controller [0200]: Intel Corporation 82599 10 Gigabit Dual Port Backplane Connection [8086:10f8] (rev 01)  
18:00.1 Ethernet controller [0200]: Intel Corporation 82599 10 Gigabit Dual Port Backplane Connection [8086:10f8] (rev 01)  
5e:00.0 Ethernet controller [0200]: Intel Corporation 82599 10 Gigabit Dual Port Backplane Connection [8086:10f8] (rev 01)  
5e:00.1 Ethernet controller [0200]: Intel Corporation 82599 10 Gigabit Dual Port Backplane Connection [8086:10f8] (rev 01)

We can check the PCI device related numa node id using one of following commands:

$ lspci -vmms 18:00.0 | grep NUMANode  
NUMANode: 0  
  
$ cat /sys/bus/pci/devices/\*0000\:18\:00.0\*/numa\_node  
0

Using numactl we can get CPU IDs on each NUMA socket:

# numactl -H  
available: 2 nodes (0-1)  
node 0 cpus: 0 2 4 6 8 10 12 14 16 18 20 22 24 26 28 30 32 34 36 38 40 42 44 46 48 50 52 54 56 58 60 62 64 66 68 70  
node 0 size: 96965 MB  
node 0 free: 10842 MB  
node 1 cpus: 1 3 5 7 9 11 13 15 17 19 21 23 25 27 29 31 33 35 37 39 41 43 45 47 49 51 53 55 57 59 61 63 65 67 69 71  
node 1 size: 98304 MB  
node 1 free: 12845 MB  
node distances:  
node 0 1  
0: 10 21  
1: 21 10

When DPDK vrouter is used, OpenStack flavors must have hw:mem\_page\_size property (cf OpenStack configuration section).

$ lspci -nn | grep -i ether  
06:00.0 Ethernet controller [0200]: Intel Corporation 82599 10 Gigabit Dual Port Backplane Connection [8086:10f8] (rev 01)  
06:00.1 Ethernet controller [0200]: Intel Corporation 82599 10 Gigabit Dual Port Backplane Connection [8086:10f8] (rev 01)  
08:00.0 Ethernet controller [0200]: Intel Corporation 82599 10 Gigabit Dual Port Backplane Connection [8086:10f8] (rev 01)  
08:00.1 Ethernet controller [0200]: Intel Corporation 82599 10 Gigabit Dual Port Backplane Connection [8086:10f8] (rev 01)  
87:00.0 Ethernet controller [0200]: Intel Corporation 82599 10 Gigabit Dual Port Backplane Connection [8086:10f8] (rev 01)  
87:00.1 Ethernet controller [0200]: Intel Corporation 82599 10 Gigabit Dual Port Backplane Connection [8086:10f8] (rev 01)  
  
[root@overcloudmz5-compdpdk-3 ~]# lspci -nn | grep -i ether  
02:00.0 Ethernet controller [0200]: Intel Corporation 82599ES 10-Gigabit SFI/SFP+ Network Connection [8086:10fb] (rev 01)  
02:00.1 Ethernet controller [0200]: Intel Corporation 82599ES 10-Gigabit SFI/SFP+ Network Connection [8086:10fb] (rev 01)  
04:00.0 Ethernet controller [0200]: Intel Corporation I350 Gigabit Network Connection [8086:1521] (rev 01)  
04:00.1 Ethernet controller [0200]: Intel Corporation I350 Gigabit Network Connection [8086:1521] (rev 01)

$ lspci -vmms "06:00.0"  
Slot: 06:00.0  
Class: Ethernet controller  
Vendor: Intel Corporation  
Device: 82599 10 Gigabit Dual Port Backplane Connection  
SVendor: Hewlett-Packard Company  
SDevice: Ethernet 10Gb 2-port 560FLB Adapter  
Rev: 01  
  
[root@overcloudmz5-compdpdk-3 ~]# lspci -vmms 02:00.0  
Slot: 02:00.0  
Class: Ethernet controller  
Vendor: Intel Corporation  
Device: 82599ES 10-Gigabit SFI/SFP+ Network Connection  
SVendor: Super Micro Computer Inc  
SDevice: Device 0611  
PhySlot: 7  
Rev: 01  
NUMANode: 0 #<---

$ numactl -H  
available: 2 nodes (0-1)  
node 0 cpus: 0 1 2 3 4 5 6 7 8 9 10 11 24 25 26 27 28 29 30 31 32 33 34 35  
node 0 size: 96307 MB  
node 0 free: 33996 MB  
node 1 cpus: 12 13 14 15 16 17 18 19 20 21 22 23 36 37 38 39 40 41 42 43 44 45 46 47  
node 1 size: 96764 MB  
node 1 free: 32347 MB  
node distances:  
node 0 1  
 0: 10 21  
 1: 21 10  
  
[root@overcloudmz5-compdpdk-3 ~]# numactl -H  
available: 2 nodes (0-1)  
node 0 cpus: 0 1 2 3 4 5 6 7 8 9 20 21 22 23 24 25 26 27 28 29  
node 0 size: 65425 MB  
node 0 free: 12794 MB  
node 1 cpus: 10 11 12 13 14 15 16 17 18 19 30 31 32 33 34 35 36 37 38 39  
node 1 size: 65536 MB  
node 1 free: 21645 MB  
node distances:  
node 0 1  
 0: 10 21  
 1: 21 10

Question: isn’t --socket-mem to allocate hugepage for vrouter (not to VM) only? or this is actually a same "global" system-wise parameter just as the kernel hugepagesz=1G hugepages=40 parameter?

Answer: This is also something we have to explain clearly. Hugepages use in DPDK are really badly explained. And, once again this is not so complex as it seems.

You just have to keep in mind that :

* Packet are put into memory at one place and **never copied** (only descriptors are moving from one Q to another)
* Consequently “memory” area where the packet are put must be shared between DPDK vrouter and all instances (what ever the instance is – DPDK or not DPDK)

Then, you have DPDK setup :

* At system level : to allocate a given amount of Memory as “hugepage type”
* At vrouter level: to use an amount of system hugepages to store packets (in mbufs)
* vRouter is using CPU on a same NUMA (at least this is the recommended setup if you want to avoid performance issues).
* Virtual instances are using CPU on both NUMA (and most probably on the other NUMA which is not used by vrouter – because you have lots of CPU on this second one available for your VMs)

So, in short, you have instances running on both NUMA. They have to be able access packets that are referenced by descriptors (that vrouter as put in vNIC RX queue).

This is why, by default we spread hugepage memory allocation on both NUMA.

![image](data:image/png;base64;base64,)

this diagram shows how huge pages are used.

So, first you are allocating HugePage at system level (at startup for 1G huge pages):

default\_hugepagesz=1GB hugepagesz=1G hugepages=40 hugepagesz=2M hugepages=40

I guess, that Huge pages are equally balanced on both NUMA (to be checked)

Then you are requesting at vrtouter level a part of them for vrouter DPDK application need (to store both underlay and VM packets):

--socket-mem <value>,<value>

## Kubernetes: vrouter and Single Hugepage size (skip)

* Currently Kubernetes in not supported to be run on compute nodes configured with multiple huge page size. If a worker node is configured with both 2M and 1GB hugepage size, Kubelet will fail to start.
* Contrail DPDK vrouter is able to run with a single Hugepage size and does not required to get both 2M and 1G pages allocated.
* by default, Contrail vrouter assumes that provided hugepages are 2Mb.

If only 1G huge pages are configured on the compute node, pagesize parameter must be specified into huge page table mount point in order for the vrouter to be aware that only 1G huge pages are available on the compute node:

Cf: <https://github.com/Juniper/contrail-vrouter/blob/R1908/dpdk/vr_dpdk_table_mem.c#L80-L84>

If this parameter is not present in the mountpoint, Contrail vrouter is assuming that 2MB hugepages are available, and will requests 2M huge pages.

If only 1GB huge pages are available onto the compute node, vrouter will fail to start.

**Hugepage size not specified in mount point.**

When huge pages mount point is configured without pagesize parameter, vrouter will request 2M hugepages allocation.

#/etc/fstab:  
hugetlbfs on /dev/hugepages type hugetlbfs (rw,relatime,seclabel)  
  
# cat /proc/mounts | grep hugepage  
hugetlbfs /dev/hugepages hugetlbfs rw,seclabel,relatime 0 0

**hugepage size (1G) specified in mount point.**

Here we have specified huge pages mount with pagesize=1G parameter. vrouter will request 1G hugepages allocation at startup.

/etc/fstab:  
hugetlbfs on /dev/hugepages type hugetlbfs (rw,relatime,seclabel,pagesize=1G)  
  
# cat /proc/mounts | grep hugepage  
hugetlbfs /dev/hugepages hugetlbfs rw,seclabel,relatime,pagesize=1G 0 0

summary of this section

* k8s setup support one pagesize only, fail if multiple configured
* by default vrouter assumes 2M
* for 1G, pagesize=1G has to be explicitly configured in fstab

feature limit, should avoid this topic

## IRQ setup (skip)

ping: talk about IRQ?

Disabling IRQ Balance is not recommended as it has no impact on performance. In RHEL, tuned’s cpu-partitioning profile leverages IRQ CPU affinity (isolated\_cores).

**Disable IRQ Balance.**

stop irqbalance daemon and remove irqbalance from system startup:

$ systemctl stop irqbalance  
$ systemctl disable irqbalance

**Exclude CPUs from IRQ Balancing.**

The /etc/sysconfig/irqbalance configuration file contains a parameter named IRQBALANCE\_BANNED\_CPUS that allows to define CPUs to be excluded from consideration by the IRQ balancing service.

The following mask excludes CPUs 8 to 15 as well as CPU 33 from IRQ balancing:

IRQBALANCE\_BANNED\_CPUS=00000001,0000ff00

If you are running a system with up to 64 CPU cores, separate each group of eight hexadecimal digits with a comma.

* QoS is not supported (Marking is supported with DPDK vrouter. Hardware queueing is not).
* Jumbo frames for DPDK VMs in 3.2.8 and 4.0.1 (\*).
* Jumbo frames for non-DPDK VMs on DPDK nodes in 3.2.8 and 4.0.1 (\*)

(\*) these features are requiring "mergeable buffers" to be supported.

ping? talk about mergeable buffers?

# **CPU pinning**

## Physical CPU cores allocation planning

When planning physical CPU cores allocation, the following aspects need to be taken into account:

* hyperthreading enabled or not
* numa topology
* number of cores assigned to vrouter for 2 kinds of tasks:
  + forwarding threads (packet processing purpose)
  + control and service threads (vrouter management purpose)
* number of cores left for system processes
* number of cores allocated to VMs

A proper definition and configuration of CPU partitioning is key for optimal performance. A bogus implementation is indeed the main source of transient packet drops even at moderate throughput.

## Hyper Threading

If HT (Hyper Threading) is enabled, the first half of each numa node core are physical cores, and the second half their HT sibling.

The best way to utilize all cores in the system, especially when using hw:cpu\_policy=dedicated (see [CPU isolation mechanisms](#X2b8b4c3b1456d2d7ce234bea43bb55c3cf3adc0)) is to **use both siblings when calculating mask for vrouter (and other resources line systemd)**. In that case, both siblings for each core used for VM pinning can be utilized.

With OpenStack, Having a core without its sibling listed in vcpu\_pin\_set variable in nova.conf file and hw:cpu\_policy=dedicated set in flavor properties used to spawn an instance leads to a scheduling error (variable sibling\_set referenced before assignment).

Question: shouldn’t disabling HT archive max perf?

Answer: HT matter is not a yes or no answer. It depends …

First, things to consider … HT has been created to improve hardware use efficiency. Idea is, we are creating “two virtual CPU” on a single Hardware CPU. It improve Physical CPU usage as the the second virtual CPU can use the physical resource when the first one is sleeping (like VM usage is improving Physical BM utilization). As the main DPDK principle is to never let a CPU to sleep … we should answer no !!!

But, from the customer perspective which is using Bare Metal Compute to run VM, his answer is YES, I want it !!!

So, in general every customer is enabling HT on his servers. So, the question is: for vrouter needs, will we recommend to use only one “logical CPU” per physical CPU ?

Or do we recommend to use both (aka siblings) on physical CPU ?

Here, again the answer is not so clear, and can’t be Yes or No.

Refer to this section: ***Last step: sibling consideration***

*Two (simplified) situations*:

1. highest throughput is expected and number VM per compute is no the first criteria, do not use siblings
2. VM per compute is the first criteria. An average DPDK vrouter performance is largely enough, let’s use siblings

## CPU isolation mechanisms

* Tasks to be run by an operating system must be spread across available CPUs.
* These tasks into a multi-threading environment are often made of several processes which are also made of several threads.
* In order to run all these processes and threads on the CPU offered by the node, the Operating System is using a scheduler to place each single one onto a given CPU.
* There are two styles of scheduling, cooperative and preemptive.
* By default, RedHat Linux is using a cooperative mode <https://medium.com/traveloka-engineering/cooperative-vs-preemptive-a-quest-to-maximize-concurrency-power-3b10c5a920fe>

In order to get a CPU booked for a subset of tasks, we have to inform the Operating System scheduler not to use these CPUs for all the tasks it has to run.

These CPUs are told: "isolated" because they are no more used to process all tasks. In order to get a CPU isolated several mechanisms can be used:

* remove this CPU from the "common" CPU list used to process all tasks
* change the scheduling algorithm (cooperative to preemptive)
* participate or not to interrupt processing

RedHat Linux is currently supporting 2 different CPU isolation methods. They are isolcpus and tuned CPU partitioning, They can be used either independently or simultaneously.

**isolcpus.**

A first method, **isolcpus** kernel parameter, has been proposed to keep CPUs away from linux scheduler. This isolation mechanism will:

* remove isolated CPUs from the "common" CPU list used to process all tasks
* change the scheduling algorithm from cooperative to preemptive
* perform CPU isolation at the **system boot**

The main drawbacks of using isolcpus are :

* it requires manual placement of processes on isolated cpus.
* it is not possible to re-arrange the CPU isolation rules after the system startup
* it is not possible to move process from one isolated cpu to another.

**tuned CPU partitioning.**

A second method, **tuned CPU partitioning**, has been proposed more recently. since almost all processes are started by systemd, physical CPU cores assignment can be configured in a different way:

* CPUAffinity parameter in /etc/systemd/system.conf; it will restrict all processes spawned by systemd to the list of cores.
* isolated\_cores: is removing a set of CPU from the "common" CPU list used to process all tasks

from RHEL 7.5, CPUAffinity is natively integrated in **tuned’s cpu-partitioning profile**.

This isolation mechanism will:

* remove isolated CPUs from the "common" CPU list used to process all tasks
* perform CPU isolation after the system boot using systemd.

The main drawbacks of using tuned partitioning are :

* Some processes are started at the system boot before systemd is started. These processes are run before isolation rules are enforced and could break expected isolation rules.
* Scheduling Algorithm is kept to cooperative mode which provides a lower isolation.

In few words, tuned partitioning is more flexible and featureful than isolcpus, but is providing a lower CPU isolation. This is why both mechanisms are often used altogether to enforce CPU isolation.

if both tuned CPU partitioning profiles and isolcpus mechanisms are used, **be careful to be consistent** in the defined setup.

Question: talk about both algorithm.

Answer:

First, we have to override this is RedHat specific. Ubuntu is using only one mechanism.

Second (not for the book), but this is not so clear on RedHat side. First idea was that new tuned partitioning will replace isolcpus historical mechanism.

But today this is not so clear on Redhat side, and they recommend to use both !!!.

Mainly because isolcpus is changing the scheduling algorithm from cooperative to preemptive, so it is more efficient for isolation.

This is why in my opinion we have to explain that:

* two mechanisms are proposed by redhat
* describe each one (how to configure it, what it does)
* explain we are recommending to use both of them to have the better CPU isolation as possible

### isolcpus mechanism configuration

before Contrail 20.03 release, it is not recommended to use such an isolation method. If used some packet drops could randomly occur and vrouter performances are not stable.

ping? explain why?

A (LD): For a lot of complex reason hard to explain. One of them (easiest to understand) is:

because before 20.03 we were not offering an ability to pin correctly service threads.

when we were enforcing a too strict CPU isolation service threads were sometime using vrouter allocated polling and processing CPUs.

Since 20.03 we are proposing a setup in which:

* vrouter processing CPUs are assigned to well defined CPU list
* vrouter control and service CPUs are assigned to another well defined CPU list

OpenStack is providing a mechanism to assign a well defined CPU list to Virtual Instances

Consequently at system level we can enforce a strict isolation to remove vrouter and openstack assigned CPU to the "common" pool.

A small common pool is kept for Operating System usage (in a shart Hypervisor needs)

**To be supplemented by Kiran and Premecz.**

***isolcpus*** is a kernel parameter. It has to be provisioned at the system startup. GRUB configuration has to be modified in order to take into consideration a new set of isolated CPU, and then, the system has to be restarted.

$ vi /etc/default/grub  
GRUB\_CMDLINE\_LINUX="console=tty0 console=ttyS0,115200n8 crashkernel=auto rhgb quiet default\_hugepagesz=1GB hugepagesz=1G hugepages=28 iommu=pt intel\_iommu=on isolcpus=7,9-35,43,45-71"  
$ grub2-mkconfig -o /etc/grub2.cfg

When TripleO is used for Contrail and OpenStack installation, this grub configuration update is automatically done, using TRIPLEO\_HEAT\_TEMPLATE\_KERNEL\_ARGS environment variable to define isolcpus value.

For instance :

TRIPLEO\_HEAT\_TEMPLATE\_KERNEL\_ARGS: "isolcpus=7,9-35,43,45-71"

ping? should be = instead of :?

TRIPLEO\_HEAT\_TEMPLATE\_KERNEL\_ARGS: "isolcpus=7,9-35,43,45-71"

Because, this variable content will be added to GRUB “command line” which is using shell like syntax.

**ping: lab (3.2 no isolcpus).**

[2020-05-12 12:47:43]root@bcomp78:~  
$ cat /etc/default/grub | grep iso

[root@overcloudmz5-compdpdk-3 ~]# cat /etc/default/grub | grep iso  
TRIPLEO\_HEAT\_TEMPLATE\_KERNEL\_ARGS=" default\_hugepagesz=1GB hugepagesz=1G hugepages=64 hugepagesz=2M hugepages=8192 isolcpus=1-9,11-19,21-29,31-39"  
#TRIPLEO\_HEAT\_TEMPLATE\_KERNEL\_ARGS=" default\_hugepagesz=1GB hugepagesz=1G hugepages=64 hugepagesz=2M hugepages=8192 isolcpus=5-9,11-19,25-29,31-39"  
#TRIPLEO\_HEAT\_TEMPLATE\_KERNEL\_ARGS=" default\_hugepagesz=1GB hugepagesz=1G hugepages=64 hugepagesz=2M hugepages=8192 isolcpus=5,8-9,11-19,25,28-29,31-39"

### Tuned CPU partitioning configuration

Tuned cpu partitioning has to be installed onto the system:

yum install tuned-profiles-cpu-partitioning

Tuned is using CPU isolation information defined into cpu-partitioning-variables.conf and into system.conf:

/etc/tuned/cpu-partitioning-variables.conf  
isolated\_cores=7,9-35,43,45-71  
  
/systemd/system.conf  
CPUAffinity=0-6,8,36-42,44

Tuned is not setting isolcpus Kernel value, but tuned.non\_isolcpus.

**ping: lab.**

[root@overcloudmz5-compdpdk-3 ~]# cat /etc/systemd/system.conf | grep CPU  
#CPUAffinity=1 2  
#DefaultCPUAccounting=no  
#DefaultLimitCPU=  
CPUAffinity=0 10 20 30 #<---systemd processes will use these CPUs only  
  
[root@overcloudmz5-compdpdk-3 ~]# cat /etc/tuned/cpu-partitioning-variables.conf  
# Examples:  
# isolated\_cores=2,4-7  
isolated\_cores=1-9,11-19,21-29,31-39 #<---  
#  
# To disable the kernel load balancing in certain isolated CPUs:  
# no\_balance\_cores=5-10

## CPU assignment for DPDK vRouter

In order to get DPDK vrouter threads pinned to a subset of CPUs on each compute node we have to define:

* vrouter dpdk cores used for packet processing (polling and forwarding threads) in CPU\_LIST (or coremask) within following file in:
  + /etc/contrail/supervisord\_vrouter\_files/contrail-vrouter-dpdk.ini (up to 4.1)
  + /etc/sysconfig/network-scripts/ifcfg-vhost0 (from 5.0 to higher)
* vrouter dpdk cores used for vrouter management (services threads) in SERVICE\_CORE\_MASK within file /etc/sysconfig/network-scripts/ifcfg-vhost0 (from 20.03 to higher)
* vrouter dpdk cores used for vrouter management (DPDK control threads) in DPDK\_CTRL\_THREAD\_MASK within file /etc/sysconfig/network-scripts/ifcfg-vhost0 (from 20.03 to higher)

These values: CPU\_LIST, DPDK\_CTRL\_THREAD\_MASK and SERVICE\_CORE\_MASK are CPU masks used for CPU pinning with taskset command.

### packet processing threads

vRouter CPU\_LIST (also named coremask in some configuration files) variable is allowing to define which core CPU will be allocated for router forwarding and polling processing threads.

vrouter forwarding and polling processings are CPU intensive. vrouter logical threads named logica core ID 10 to logical core 10 + N - 1 (with N = Number of allocated polling and forwarding cores) are used for forwarding and polling processing. These threads have to be pinned to some well defined CPU in order to avoid the vrouter to starve the full node CPU capacity. A maximum of 54 forwarding CPU can be allocated to a vrouter (logical core ID: 10 to 63).

Below is an example of a configuration of a 2 socket system, each processor with 2\*18 physical cores, with HT enabled. The network adapter in PCI-E bus is attached to NUMA 0. 4 physical cores are dedicated for vRouter (i.e. 8 logical cores thanks to Hyper Threading).

NUMA node0 CPU(s):  
PHY cores: \*0 2 4 6 8 10 12 14 16 18 20 22 24 26 28 30 32 34\*  
HT cores : \*36 38 40 42 44 46 48 50 52 54 56 58 60 62 64 66 68 70\*  
NUMA node1 CPU(s):  
PHY cores: \*1 3 5 7 9 11 13 15 17 19 21 23 25 27 29 31 33 35\*  
HT cores : \*37 39 41 43 45 47 49 51 53 55 57 59 61 63 65 67 69 71\*

We are planning CPU assignment as follows:

* 4 cores for Operating System processes and vrouter agent/dpdk lightweight threads: **red** **0, 1, 3, 5, 36, 37, 39, 41**
* 4 physical cores for vRouter DPDK forwarding threads (in same NUMA 0), **blue**: **2, 4, 6, 8** with HT siblings **38, 40, 42, 44**. Do not allocate physical Core 0 (e.g. here 0 and 36) for Vrouter DPDK forwarding threads.
* The rest of the cores are for Nova vcpu\_pin\_set, **black**: 7,9-35, 43,45-71.

For optimal performance it is recommended that a single VMs is executed on a same NUMA (unless it can efficiently leverage kvm/pinning information)

vRouter **CPU\_LIST** (aka coremask) calculation based on the assumption above: vCPUs 2, 4, 6, 8, 38, 40, 42, 44 are allocated for vRouter, which maps to b0001 0101 0100 0000 0000 0000 0000 0000 0000 0001 0101 0100 in binary.

This translates to a hex mask 0x154000000154 that must be configured in the /etc/contrail/supervisord\_vrouter\_files/contrail-vrouter-dpdk.ini file (see below example for Contrail 4.1 release).

[root@overcloud-contraildpdk-16 ~]# cat /etc/contrail/supervisord\_vrouter\_files/contrail-vrouter-dpdk.ini  
[program:contrail-vrouter-dpdk]  
command=/bin/taskset \*0x154000000154\* /usr/bin/contrail-vrouter-dpdk --no-daemon --vdev "eth\_bond\_bond1,mode=4,xmit\_policy=\*\*l34\*\*,socket\_id=0,mac=a0:36:9f:d1:c8:78,slave=0000:04:00.0,slave=0000:04:00.1" --vlan\_tci "201" --vlan\_fwd\_intf\_name "bond1" --socket-mem 1024,1024  
priority=410  
autostart=true  
killasgroup=true  
stdout\_capture\_maxbytes=1MB  
redirect\_stderr=true  
stdout\_logfile=/var/log/contrail/contrail-vrouter-dpdk-stdout.log  
stderr\_logfile=/var/log/contrail/contrail-vrouter-dpdk-stderr.log  
exitcodes=0 ; 'expected' exit codes for process (default 0,2)

After modifying this file, the vrouter must be restarted to take changes into account:

systemctl restart supervisor-vrouter

Some processors have different layout of cores in each numa node. The most popular is the first half being a part of numa 0 and the second half a part of numa 1. But there are processors, where even cores are a part of numa 0 and odd cores a part of numa

When using 5.0 and later version of contrail vrouter, hex mask 0x154000000154, must be configured into CPU\_LIST variable in /etc/sysconfig/network-scripts/ifcfg-vhost0 file: CPU\_LIST=0x154000000154

After modifying this file, the vrouter vhost0 interface must be restarted to take changes into account:

$ ifdown vhost0  
$ ifup vhost0

### service and control threads ⇐ 19.12

For contrail release 19.12 and earlier, Control and Service threads are not assigned to any CPU. Consequently, these threads can use any available CPU.

We can get all contrail-vrouter-dpdk assignments using taskset with -a option :

\*# taskset -cap `pidof contrail-vrouter-dpdk`\*  
\*pid 21666's current affinity list : 0-71\*  
\*pid 21740's current affinity list : 3-7,18-71\*  
\*pid 21741's current affinity list : 3-7,18-71\*  
\*pid 21790's current affinity list : 3-7,18-71\*  
\*pid 21791's current affinity list : 0-71\*  
\*pid 21792's current affinity list : 0-71\*  
\*pid 21793's current affinity list : 0-71\*  
\*pid 21794's current affinity list : 0-71\*  
\*pid 21795's current affinity list : 2\*  
\*pid 21796's current affinity list : 4\*  
\*pid 21797's current affinity list : 6\*  
\*pid 21798's current affinity list : 8\*  
\*pid 21799's current affinity list : 38\*  
\*pid 21800's current affinity list : 40\*  
\*pid 21801's current affinity list : 42\*  
\*pid 21802's current affinity list : 44\*  
\*pid 29401's current affinity list : 0-71\*

**ping: lab.**

[heat-admin@jnprctdpdk01 ~]$ taskset -cap `pidof contrail-vrouter-dpdk`  
pid 46058's current affinity list: 4  
pid 46070's current affinity list: 4  
pid 46071's current affinity list: 4  
pid 46073's current affinity list: 4  
pid 46074's current affinity list: 4  
pid 46075's current affinity list: 4  
pid 46076's current affinity list: 4  
pid 46077's current affinity list: 4  
pid 46078's current affinity list: 1  
pid 46079's current affinity list: 2  
pid 46080's current affinity list: 3  
pid 46536's current affinity list: 4

In the previous example, we can notice that threads are assigned to a given CPU set according following rules :

* **processing threads** have a CPU affinity restricted to a single one CPU (these are 2,4,6,8,38,40,42 and 44). Consequently each is placed on a single CPU.
* **service threads** have a CPU affinity with all available CPUs. They can use any CPU..
* **control threads** have CPU affinity with almost all available CPUs. This is the default DPDK library behavior (DPDK is keeping only CPU that are not booked for vrouter DPDK processing threads - previous example these are 3-7,18-71).

It’s possible for a Contrail release R1912 (and earlier) to apply a patch in order to be able to use a specific SERVICE\_CORE\_LIST parameter. This parameter allows to pin both service and control threads onto a specific CPU list. In order to get the new parameter available, we have to apply the following procedure on all the DPDK compute node :

# mkdir -p /tmp/vrouter\_patch  
# cd /tmp/vrouter\_patch  
# curl -o patched-r1912-archive.tar.gz \  
'https://review.opencontrail.org/changes/Juniper%2Fcontrail-container-builder~55730/revisions/1/archive?format=tgz'  
# tar xvzf ./patched-r1912-archive.tar.gz containers/vrouter/base/network-functions-vrouter-dpdk containers/vrouter/agent-dpdk/entrypoint.sh --strip 3  
# mv ./network-functions-vrouter-dpdk /etc/sysconfig/network-scripts/network-functions-vrouter-dpdk  
# X=$(docker images --format "\{\{.Repository}}:\{\{.Tag}}" | grep contrail-vrouter-agent-dpdk)  
# cat <<EOF > Dockerfile  
# FROM $\{X}  
# COPY ./entrypoint.sh /entrypoint.sh  
# EOF  
# docker build . -t $\{X}

SERVICE\_CORE\_LIST has been split into two variables into Contrail 20.03 and later releases:

* DPDK\_CTRL\_THREAD\_MASK
* SERVICE\_CORE\_MASK

In order to be used, you’ll have to follow explanation in next section given for SERVICE\_CORE\_MASK (just replace in you configuration SERVICE\_CORE\_MASK with SERVICE\_CORE\_LIST when using this patch)

### service and control threads pinning >= 20.03

Since Contrail 20.03 release it is possible to assign Control and Service threads to a given CPU list. vRouter ***SERVICE\_CORE\_MASK*** variable is allowing to define which core CPU will be allocated for vrouter service threads. ***DPDK\_CTRL\_THREAD\_MASK*** variable is allowing to define which core CPU will be allocated for vrouter control threads.

Below is an example of a configuration of a 2 socket system, each processor with 2\*18 physical cores, with HT enabled.

The network adapter in PCI-E bus is attached to NUMA 0. 4 physical cores are dedicated for vRouter (i.e. 8 logical cores thanks to Hyper Threading).

NUMA node0 CPU(s):  
PHY cores: \*0 2 4 6 8 10 12 14 16 18 20 22 24 26 28 30 32 34\*  
HT cores : \*36 38 40 42 44 46 48 50 52 54 56 58 60 62 64 66 68 70\*  
NUMA node1 CPU(s):  
PHY cores: \*1 3 5 7 9 11 13 15 17 19 21 23 25 27 29 31 33 35\*  
HT cores : \*37 39 41 43 45 47 49 51 53 55 57 59 61 63 65 67 69 71\*

We are planning CPU assignment as follows:

* 4 cores for Operating System processes and vrouter agent/dpdk lightweight threads: **red** **0, 1, 3, 5, 36, 37, 39, 41.** DPDK control threads will also be pinned on these CPUs.
* 4 physical cores for vRouter DPDK vrouter forwarding threads (in same NUMA 0), **blue**: **2, 4, 6, 8** with HT siblings **38, 40, 42, 44**. Do not allocate physical Core 0 (e.g. here 0 and 36) for Vrouter DPDK threads.
* 1 physical core for vRouter DPDK vrouter service threads (in same NUMA 0), **green**: **10** with HT sibling **46**.
* The rest of the cores are for Nova vcpu\_pin\_set, **black**: 7,9,11-35, 43,45,47-71.

For optimal performance it is recommended that each VM be executed on a same NUMA (unless it can efficiently leverage kvm/pinning information).

vRouter service cores mask calculation based on the assumption above: vCPUs 10, 46 are allocated for vRouter, which maps to b0100 0000 0000 0000 0000 0000 0000 0000 0000 0100 0000 0000 in binary.

This translates to a hex mask 0x400000000400 that must be configured into **SERVICE\_CORE\_MASK** variable in /etc/sysconfig/network-scripts/ifcfg-vhost0 file:

SERVICE\_CORE\_MASK=\*\*0x400000000400\*\*

vRouter DPDK control threads mask calculation based on the assumption above: vCPUs 0,1,3,5,36,37,39,41 are allocated for vRouter, which maps to binary:

b0000 0010 1011 0000 0000 0000 0000 0000 0000 0000 0010 1011

This translates to a hex mask 0x2B00000002B that must be configured into **DPDK\_CTRL\_TREAD\_MASK** variable in /etc/sysconfig/network-scripts/ifcfg-vhost0 file: DPDK\_CTRL\_THREAD\_MASK=**0x2B00000002B**

After file has been updated, the vrouter vhost0 interface must be restarted to take changes into account:

$ ifdown vhost0  
$ ifup vhost0

We can get all contrail-vrouter-dpdk assignments using taskset with -a option :

\*# taskset -cap `pidof contrail-vrouter-dpdk`\*  
\*pid 21666's current affinity list : 0-71\*  
\*pid 21740's current affinity list : 0,1,3,5,36,37,39,41\*  
\*pid 21741's current affinity list : 0,1,3,5,36,37,39,41\*  
\*pid 21790's current affinity list : 0,1,3,5,36,37,39,41\*  
\*pid 21791's current affinity list : 10,46\*  
\*pid 21792's current affinity list : 10,46\*  
\*pid 21793's current affinity list : 10,46\*  
\*pid 21794's current affinity list : 10,46\*  
\*pid 21795's current affinity list : 2\*  
\*pid 21796's current affinity list : 4\*  
\*pid 21797's current affinity list : 6\*  
\*pid 21798's current affinity list : 8\*  
\*pid 21799's current affinity list : 38\*  
\*pid 21800's current affinity list : 40\*  
\*pid 21801's current affinity list : 42\*  
\*pid 21802's current affinity list : 44\*  
\*pid 29401's current affinity list : 10,46\*

In the previous example, we can notice that threads are assigned to a given CPU set according following rules :

* **processing threads** have a CPU affinity restricted to a single one CPU (these are 2,4,6,8,38,40,42 and 44). Consequently each is placed on a single CPU.
* **service threads** have CPU affinity restricted to only 2 CPUs (they are 10,46).
* **control threads** have a CPU affinity restricted to the same CPUs assigned for Operation System (they are 0,1,3,5,36,37,39,41).

## Provisioning concerns

Currently **only CPU assigned to packet processing threads** (**CPU\_LIST / COREMASK**) can be managed with provisioning tools.

Since version 20.03, we can also manage CPU assigned to control and service threads (**DPDK\_CTRL\_THREAD\_MASK** and **SERVICE\_CORE\_MASK**) with provisioning tools.

Contrail can be installed through different tools: Contrail Cloud, Contrail Networking integrated with RHOSP and TripleO deployer or Juniper Contrail Ansible Deployer to name some.

### control and service threads >= 20.03

When setting up the environment we will have to specify the CPU assignment for service threads. For RSHOP and Ansible deployer installation be sure to include the service mask within quotes within configuration files.

When deploying via **Ansible deployer**, file instances.yaml has to include SERVICE\_CORE\_MASK and DPDK\_CTRL\_THREAD\_MASK variables with quotes in order to avoid the given value to be converted into a decimal number leading to wrong core assignment.

So, we have to use SERVICE\_CORE\_MASK=”0x400000000400” instead of SERVICE\_CORE\_MASK=0x400000000400 and DPDK\_CTRL\_THREAD\_MASK=”0x2B00000002B” instead of SERVICE\_CORE\_MASK=0x2B00000002B

compute\_dpdk\_1:  
provider: bms  
ip: 172.30.200.46  
roles:  
vrouter:  
PHYSICAL\_INTERFACE: vlan0200  
AGENT\_MODE: dpdk  
CPU\_CORE\_MASK: ”0x154000000154”  
\*SERVICE\_CORE\_MASK\*: ”0x400000000400”  
\*DPDK\_CTRL\_THREAD\_MASK\*: ”0x2B00000002B”  
DPDK\_UIO\_DRIVER: uio\_pci\_generic  
HUGE\_PAGES: 60000

When **TripleO** is used, SERVICE\_CORE\_MASK and DPDK\_CTRL\_THREAD\_MASK variables have to be included into Contrail Service configuration file (*<tripleo-root-dir>*/environments/contrail/contrail-services.yaml). Quotes have also to be used into TripleO Yaml files in order to avoid the value to be converted into decimal.

In TripleO SERVICE\_CORE\_MASK: ”0x400000000400” has to be used to get vrouter service threads assigned onto 10 and 46 CPU cores, and DPDK\_CTRL\_THREAD\_MASK=”0x2B00000002B” has to be used to get vrouter control threads assigned onto 0,1,3,5,36,37,39 and 41 CPU cores.

SERVICE\_CORE\_MASK and DPDK\_CTRL\_THREAD\_MASK have to be defined into ContrailSettings. ContrailSettings variable can be set at role level :

parameter\_defaults:

<Role Name>Parameters:  
TunedProfileName: "cpu-partitioning"  
IsolCpusList: "2-35,38-71"  
NovaVcpuPinSet: "12-35,48-71"  
NovaComputeCpuSharedSet: "5-7"  
KernelArgs: " isolcpus=2-35,38-71"  
ContrailSettings:  
SERVICE\_CORE\_MASK: ”0x400000000400”  
DPDK\_CTRL\_THREAD\_MASK: ”0x2B00000002B”

By default, ContrailDpdk is the role name used for DPDK compute.

Or, globally for all roles:

parameter\_defaults:  
ContrailSettings:  
SERVICE\_CORE\_MASK: ”0x400000000400”  
DPDK\_CTRL\_THREAD\_MASK: ”0x2B00000002B”

If ContrailSettings is defined at role level, it will hide all ContrailSettings values defined globally. Each ContrailSettings parameters expected at role level have to be redefined even if defined at the global level.

### packet processing threads (forwarding cores)

When setting up the environment we will have to specify the CPU assignment for packet processing threads. For RSHOP and Ansible deployer installation be sure to include the core mask within quotes within configuration files.

When deploying via **Ansible deployer**, file instances.yaml has to include CPU\_CORE\_MASK variable with quotes in order to avoid the given value to be converted into a decimal number leading to wrong core assignment.

So, we have to use CPU\_CORE\_MASK=”0x154000000154” instead of CPU\_CORE\_MASK=0x154000000154.

Here is an example when installing Contrail via Ansible deployer:

compute\_dpdk\_1:  
provider: bms  
ip: 172.30.200.46  
roles:  
vrouter:  
PHYSICAL\_INTERFACE: vlan0200  
AGENT\_MODE: dpdk  
\*CPU\_CORE\_MASK\*: ”0x154000000154”  
SERVICE\_CORE\_MASK: ”0x400000000400”  
DPDK\_UIO\_DRIVER: uio\_pci\_generic  
HUGE\_PAGES: 60000

You can connect onto a DPDK compute node and read the vrouter environment file (which is on the host OS, not inside a container) in order to check that the correct value has been configured by the deployer.

If you see something like this, things are correct:

[root@server-5b ~]# cat /etc/contrail/common\_vrouter.env | grep CORE  
CPU\_CORE\_MASK=0x154000000154

Otherwise, if you see this configuration will not be correct:

[root@server-5b ~]# cat /etc/contrail/common\_vrouter.env | grep CORE  
CPU\_CORE\_MASK=23364622090580

Value 23364622090580 is 0x154000000154 in decimal format.

If you find yourself in the wrong scenario then you can simply edit the common\_vrouter file so to include the right core mask syntax. Next, "re-create" containers by running:

cd to /etc/contrail/vrouter  
docker-compose down  
docker-compose up -d

This time DPDK will be pinned as desired.

When **TripleO** is used, CPU\_LIST has to be included into the Contrail NIC template configuration file (*<tripleo-root-dir>*/network/config/contrail/contrail-dpdk-nic-config.yaml}. Quotes have also to be used into TripleO Yaml files in order to avoid the value to be converted into decimal.

In TripleO CPU\_LIST=”0x154000000154” have to be used to get vrouter processing threads assigned onto 2.4.6,8,38,40,42 and 44 CPU cores.

Here is a Contrail NIC template configuration example when installing Contrail via TripleO deployer:

resources:  
OsNetConfigImpl:  
type: OS::Heat::SoftwareConfig  
properties:  
…  
params:  
$network\_config:  
network\_config:  
- type: contrail\_vrouter\_dpdk  
name: vhost0  
use\_dhcp: false  
cpu\_list: ”0x154000000154”  
…

If more that 54 forwarding cores are selected with CPU\_CORE\_MASK (or cpu\_list), vrouter startup will fail with following message into contrail-vrouter-dpdk.log file: "Error configuring lcores: number of forwarding cores exceeds maximum of 54" .

## CPU pinning and isolation

### tuned and isolcpus - RedHat

First we are enforcing CPU isolation rules in order to keep CPUs assigned to vRouter and Nova out of the system scheduler :

1. Tuned: Prevent CPUs for Nova and vRouter in /etc/tuned/cpu-partitioning-variables.conf

* cat /etc/tuned/cpu-partitioning-variables.conf  
  isolated\_cores=2-35,38-71

1. Isolcpus: Edit grub configuration in order to add isolcpus (and edit grub to hugepages)

* cat /etc/default/grub  
  GRUB\_CMDLINE\_LINUX="console=tty0 console=ttyS0,115200n8 crashkernel=auto rhgb quiet default\_hugepagesz=1GB hugepagesz=1G hugepages=128 hugepagesz=2M hugepages=40 \*isolcpus=2-35,38-71\*

1. apply isolation changes :

* $ systemctl restart tuned  
  $ grub2-mkconfig -o /boot/grub2/grub.cfg  
  $ reboot

### isolcpus - Ubuntu

On Ubuntu OS, isolcpus mechanism is used in order to keep CPUs assigned to vRouter and Nova out of the system scheduler :

Kernel parameter isolcpus=2-35,38-71 in /etc/default/grub,  
run update-grub and restart the node.

### Operating system scheduler CPU assignment (CPUAffinity) - RedHat

1. CPUs assigned to the system scheduler are defined using tuned partitioning mechanism :

* vi /systemd/system.conf  
  ...  
  CPUAffinity=0-1,36-37

1. then we apply tuned configuration changes :

* # systemctl restart tuned

### Nova CPU assignment (vcpu\_pin\_set)

Cores to be used by Nova to run VMs is defined into *vcpu\_pin\_set* variable (in DEFAULT section in /etc/nova/nova.conf file).

1. We are enforcing Nova CPU assignment :

* # openstack-config --set /etc/nova/nova.conf DEFAULT vcpu\_pin\_set 4-47  
  # cat /etc/nova/nova.conf | grep vcpu\_pin\_set  
  vcpu\_pin\_set=3,5,7,9,11-35,39,41,43,45,47-71

1. In order to get these changes taken into consideration, nova compute service has to be restarted:

* When OpenStack Kolla is used:
* # docker restart nova\_compute
* When OpenStack Kolla is not used:
* # service nova-compute restart (Ununtu) +  
  # service openstack-nova-compute restart (RHEL)

Optionally, property *hw:cpu\_policy=dedicated* can be set in any openstack flavor definition to disable VCPUs migration from one physical core to another.

The advantage of this approach is that for flavors without the ***hw:cpu\_policy=dedicated*** property (the default value will be set ***hw:cpu\_policy=prefered***), VMs will be balanced between cpus.

With isolcpus set, all VMs without the above property will end up executing on the first cpu from the list.

### vRouter CPU assignment (CPU\_LIST, SERVICE\_CORE\_MASK and DPDK\_CTRL\_THREAD\_MASK)

1. Configure vrouter CPU\_LIST (only CPU 2,4,6,8 are used: mask=0x154):

* vi /etc/sysconfig/network-scripts/ifcfg-vhost0  
  [...] CPU\_LIST=0x154
* PS: CPU 38,40,42 and 44 are not selected and won’t receive any task to process.

1. Configure vrouter SERVICE\_CORE\_MASK:

* vi /etc/sysconfig/network-scripts/ifcfg-vhost0  
  [...] SERVICE\_CORE\_MASK=0x400000000400

1. Configure vrouter DPDK\_CTRL\_THREAD\_MASK:

* vi /etc/sysconfig/network-scripts/ifcfg-vhost0  
  [...] DPDK\_CTRL\_THREAD\_MASK=0x2B00000002B

1. We apply vrouter configuration changes :

* # ifdown vhost0  
  # ifup vhost0

### Check CPU pinning on all processes

In order to check actual CPU used to run a process and the CPU pinning rule bound to each process, following command can be used :

$ ps -eT -o psr,tid,comm,pid,ppid,cmd,pcpu,stat | awk '$3 != "ps" \{ cmd="taskset -cp " $2 "| sed \"s/^pid .\*s current affinity list://\" | tr -d \" \" | tr -d \"\\n\" "; cmd | getline affin; printf( "%6s %s \n", affin, $0) }' 2> /dev/null | more  
PSR TID COMMAND PID PPID CMD %CPU STAT  
0-47 0 1 systemd 1 0 /usr/lib/systemd/systemd -- 0.0 Ss  
0-47 0 2 kthreadd 2 0 [kthreadd] 0.0 S  
0 0 4 kworker/0:0H 4 2 [kworker/0:0H] 0.0 S<  
0 0 6 ksoftirqd/0 6 2 [ksoftirqd/0] 0.0 S  
0 0 7 migration/0 7 2 [migration/0] 0.0 S  
0-47 8 8 rcu\_bh 8 2 [rcu\_bh] 0.0 S

In the first column we can read the ***CPU pinning*** put onto the process with taskset command, in the second one (PSR), we can see the ***actual CPU*** used by the process.

**ping: from lab.**

[heat-admin@jnprctdpdk01 ~]$ ps -eT -o psr,tid,comm,pid,ppid,cmd,pcpu,stat | awk '$3 != "ps" { cmd="taskset -cp " $2 "| sed \"s/^pid .\*s current affinity list://\" | tr -d \" \" | tr -d \"\\n\" "; cmd | getline affin; printf( "%6s %s \n", affin, $0) }' 2> /dev/null  
 PSR TID COMMAND PID PPID CMD %CPU STAT  
 0,15 15 1 systemd 1 0 /usr/lib/systemd/systemd -- 0.1 Ss  
 0,15 15 2 kthreadd 2 0 [kthreadd] 0.0 S  
 0 0 4 kworker/0:0H 4 2 [kworker/0:0H] 0.0 S<  
 0-15 15 5 kworker/u32:0 5 2 [kworker/u32:0] 0.0 S  
 0 0 6 ksoftirqd/0 6 2 [ksoftirqd/0] 0.0 S  
 0 0 7 migration/0 7 2 [migration/0] 0.0 S  
 0,15 15 8 rcu\_bh 8 2 [rcu\_bh] 0.0 S  
 0,15 15 9 rcu\_sched 9 2 [rcu\_sched] 0.1 S  
 15 15 10 lru-add-drain 10 2 [lru-add-drain] 0.0 S<  
 1 1 11 migration/1 11 2 [migration/1] 0.0 S  
 1 1 12 ksoftirqd/1 12 2 [ksoftirqd/1] 0.0 S  
 1 1 13 kworker/1:0 13 2 [kworker/1:0] 0.0 S  
 1 1 14 kworker/1:0H 14 2 [kworker/1:0H] 0.0 S<  
 0,15 0 15 rcuob/1 15 2 [rcuob/1] 0.0 S

# **DPDK vrouter Performance fine tuning**

## Performance tuning essentials

Juniper Networks recommends to tune performance in the following four areas:

* Enable multiqueue on VNF as described in section [???](#Enable Multiqueue on OpenStack instances)
* Proper CPU allocation as described in section [service and control threads pinning >= 20.03](#X667c6f0ed5a227b0b54ba9e69c668c8bb6686aa)
* Not disable Irqbalance as described in section [???](#Irqbalance)
* When router is working in Flow based mode, optimize flow setup rate as described in section [Flow setup rate optimisation](#X312a4a1815a90963812df0f2c2ec97918a420c4) or consider usage of Packed based mode.

The following performance optimization actions are details below:

* Enable CPU performance mode
* Manage a high flow environment
* Bond setting
* Change default encapsulation
* DPDK buffer size adjustment (mbuf)
* Jumbo frame support
* Control the number of CPU cores for vRouter

## Enable CPU performance mode

* CPU frequency scaling enables the operating system to scale the CPU frequency up or down in order to save power.
* CPU frequencies can be scaled automatically depending on the system load, in response to ACPI events, or manually by userspace programs.
* To run the CPU at the maximum frequency set scaling\_governor to performance.
* for f in /sys/devices/system/cpu/cpu\*/cpufreq/scaling\_governor ; do echo performance > $f ; cat $f; done

Disable all power saving options such as: Power performance tuning, CPU P-State, CPU C3 Report and CPU C6 Report. Select Performance as the CPU Power and Performance policy.

![BIOS/Platform Configuration(RBSU)](data:image/png;base64;base64,)

BIOS/Platform Configuration(RBSU)

Disable Turbo Boost to ensure the performance scaling increases with the number of cores.

![Disable Turbo Boost](data:image/png;base64;base64,)

Disable Turbo Boost

Set memory frequency to the highest available number, NOT auto.

![Set memory frequency](data:image/png;base64;base64,)

Set memory frequency

## vrouter physical bond setting

For optimal performance, bond mode must be set to 4, and hash set to layer 3/4 in contrail-vrouter-dpdk.ini on the physical interface (Since Contrail 5.0 release and later, Contrail is now containerized and DPDK parameters are no more defined into contrail-vrouter-dpdk.ini file but are installed by /bin/bash /entrypoint.sh into contrail-vrouter-agent-dpdk container - cf appendix section).

/etc/contrail/supervisord\_vrouter\_files/contrail-vrouter-dpdk.ini  
[program:contrail-vrouter-dpdk]  
command=/usr/bin/taskset 0xff /usr/bin/contrail-vrouter-dpdk --no-daemon --vr\_flow\_entries=2000000 --vdev "eth\_bond\_bond0,\*mode=4\*,\*xmit\_policy=l34\*,socket\_id=0,mac=90:e2:ba:c5:79:90,slave=0000:01:00.0,slave=0000:01:00.1,slave=0000:02:00.0,slave=0000:02:00.1" --socket-mem 1024,1024  
priority=410  
autostart=true  
killasgroup=true  
stdout\_capture\_maxbytes=1MB  
redirect\_stderr=true  
stdout\_logfile=/var/log/contrail/contrail-vrouter-dpdk-stdout.log  
stderr\_logfile=/var/log/contrail/contrail-vrouter-dpdk-stderr.log  
exitcodes=0 ; 'expected' exit codes for process (default 0,2)

Then run service supervisor-vrouter restart for the changes to take effect.

Bond linux setup "lacp bond mode=4,xmit\_policy=l23" is performing load-balancing on **layer2+layer3 outer header**. In other words, outgoing packets are spread onto both interface according underlay destination IP (as source IP is the same for all encapsulated packets sent by a given compute).

Every packet sent by a compute node to a given remote compute node will use the same outgoing Ethernet interface for a given encapsulation protocol (VxLAN, MPLSoUDP or MPLSoGRE).

Using Bond linux setup "lacp bond mode=4,xmit\_policy=l34” is performing load-balancing on **layer3+layer4 outer header.** With this setup when a UDP encapsulation protocol is used (MPLSoUDP or VxLAN), outgoing packets to be sent to a given compute node are spread onto both outgoing Ethernet interfaces according to UDP source port that is used to create traffic “entropy" (diversity) between different flows.

## Manage a high flow environment

### Increase flow table size

The default flow table size is 512K and can be increased by setting the -– vr\_flow\_entries in /etc/contrail/supervisor-vrouter\_files/contrail-vrouter-dpdk.ini

(Since Contrail 5.0 release and later, Contrail is now containerized and DPDK parameters are no more defined into contrail-vrouter-dpdk.ini file but are installed by /bin/bash /entrypoint.sh into contrail-vrouter-agent-dpdk container - cf appendix section)

To increase the flow table to 2M flows set the –vr\_flow\_entries as below:

command=taskset 0xff /usr/bin/contrail-vrouter-dpdk --no-daemon \*--vr\_flow\_entries=2000000\* –vdev "eth\_bond\_bond0,mode=4,xmit\_policy=l34,socket\_id=0,mac=90:e2:ba:b8:70:c4,slave=0000:03:00.0,slave=0000:83:00.0,slave=0000:83:00.1,slave=0000:03:00.1" --socket-mem 1024,1024

Then reload kernel module and restart vrouter

### Flow setup rate optimisation

For optimal flow setup rate, the agent flow thread count can be increased to 4 (default 2 threads).

/etc/contrail/contrail-vrouter-agent.conf  
[FLOWS]  
thread\_count = 4

Then run service supervisor-vrouter restart for the changes to take effect.

This setting is also available at orchestration level through the following variable in TripleO template:

ContrailSettings:  
 VROUTER\_GATEWAY: 172.30.254.1  
 BGP\_ASN: 64512  
 BGP\_AUTO\_MESH: true  
 LACP\_RATE: 1  
 \*VROUTER\_AGENT\_\_FLOWS\_\_thread\_count: '4'\*

To set about the total amount of threads assigned to the agent (not only for flows), the number of threads for agent should be higher than for the flow thread number.

/etc/contrail/supervisord\_vrouter.conf  
environment=TBB\_THREAD\_COUNT=6

Then run service supervisor-vrouter restart for the changes to take effect.

### Configuration of packet based processing

By default Contrail works in flow-based processing providing a vast feature portfolio. Alternatively, packet based mode can be enabled in Contrail on per interface basis, in order to increase the packet processing rate for traffic that may not need a processing per flow.

Packet-based processing is configurable at port level by selecting the "Disable Policy" checkbox: this will stop the creation of new flows for this interface only.

![Picture1.png](data:image/png;base64;base64,)

Despite disabling policy the following features will continue to be available:

* Virtualisation and routing with ECMP
* Metadata service
* Link local
* BGPaaS
* Port Mirroring
* Service Chaining with network policy with rule any any and a single-step chain (no chaining of several SIs).

## MPLSoUDP encapsulation Configuration

### Contrail Configuration

During provisioning of Contrail sometimes provisioning tool not set an encapsulation priority by this for communication to gateways and among vrouters is using default MPLSoGRE. MPLSoGRE is less efficient and not support 5 tuple entropy. To change it encapsulation priority need to be set as follow:

* MPLSoUDP
* MPLSoGRE
* VxLAN

The encapsulation can be set by WebUI.

![image](data:image/png;base64;base64,)

### SDN Gateway configuration: MPLSoUDP and Load Balancing

***MPLSoUDP configuration*.**

In parallel, for optimal load balancing capabilities and resource usage optimisation the SDN gateway must also be configured with the MPLSoUDP encapsulation.

The below configuration applies for JUNOS devices (MX). Note that Junos MPLSoUDP support starts with 16.2 onwards.

1. Configure Tunnels with MPLSoUDP encapsulation

* [edit routing-options]  
  autonomous-system 65100;  
  dynamic-tunnels {  
   contrail {  
   source-address 10.0.0.100;  
   udp; # <===== configuration MPLSoUDP encapsulation (data plane)  
   destination-networks {  
   10.0.0.0/24;  
   }  
   }  
  }

1. Configuration of Control Plane signalling (BGP) to advertise the MPLSoUDP encapsulation community (RFC 5512). This overrides the Contrail default GRE forwarding mode.

* # Define a policy and an encapsulation community (RFC 5512) to advertise  
  # that prefixes must be reached via an MPLSoUDP Tunnelling encapsulation.  
  [edit policy-options]  
  community com-encaps-udp members 0x030c:65100:13; #last digit MUST be 13 (Type = MPLSoUDP)  
  policy-statement pol-set-udp-encaps { # define a policy  
   then {  
   community add com-encaps-udp;  
   }  
  }
* # Apply this policy toward the MP-BGP peering toward the Contrail Control Nodes.  
  [edit protocols bgp]  
  group to-Cluster1 {  
   export pol-set-udp-encaps; # apply policy adding UDP encap community  
   vpn-apply-export; # if routes exported from a local VRF is defined on PE  
   ...  
   neighbor 10.0.0.6;  
  }

***Virtual Network Load Balancing Configuration*.**

In parallel, some VNF design can also require the activation of Load Balancing (a.ka. multipath) at VRF level.

# Control Plane ECMP activation  
routing-instances {  
 VRF\_XXXXX {  
 routing-options {  
 multipath;  
 }  
 }  
}  
# Data Plane ECMP activation  
routing-options {  
 forwarding-table {  
 export load-balance-per-flow;  
 }  
}  
policy-options {  
 policy-statement load-balance-per-flow {  
 term 1 {  
 then {  
 load-balance per-packet;  
 accept;  
 }  
 }  
 }  
}  
# Optional GTP TEID hashing activation for mobile use cases  
forwarding-options {  
 enhanced-hash-key {  
 family inet {  
 gtp-tunnel-endpoint-identifier;  
 }  
 }  
}

## DPDK buffer size adjustment (mbuf)

Received packets in Fortville NICs are processed differently to Niantic. Contrail vRouter adjusts to Intel recommendations and increases the number of TX and RX buffer descriptors from 128 to 2048 and the mbuf pool from 16K to 32K bytes.

Starting from the Contrail 3.2.10 release it will be possible to configure the number of TX / RX descriptors in contrail-vrouter-dpdk.ini file <https://bugs.launchpad.net/juniperopenstack/+bug/1743391>

LP 1743391:

During testings, we hit problem with packet loss between switch port (TX) and vrouter vif 0 (RX). The error counters on DPDK vRouter was 0 during all the test (1Mpps, 4Gbps). After testing it turned out the problem is with lack of available RX descriptors. Engineering prepared a build that uses 2K TX and RX descriptors/buffers (instead of 128) and a mbuf pool of size 32K (instead of 16K). The mbuf pool size is actually configurable at runtime by adding this to the vrouter-dpdk ini file (--vr\_mempool\_sz=any power of 2). It should be also possible to configure number of TX / RX descriptors there.

Configuration of the settings through this LP fixed the drop issue and allowed to achieve higher thorughput (link saturation).

--dpdk\_txd\_sz=2048 --dpdk\_rxd\_sz=2048 --vr\_mempool\_sz=131072

Since Contrail 5.0 release and later, Contrail is now containerized and DPDK parameters are no more defined into contrail-vrouter-dpdk.ini file but are installed by /bin/bash /entrypoint.sh into contrail-vrouter-agent-dpdk container - cf appendix section.

**Caveat: The Intel NIC may silently drop packets in case of a shortage of RX descriptors. The DPDK vRouter polls NIC for these statistics.**

### Intel recommendation

Intel recommendation to reduce or avoid packet loss

When using Niantic (PF), the packets can be either buffered in the RX descriptors (or, more correctly speaking, in the memory addressed by the RX descriptors), or in the RX packet buffer in the NIC.

RX packet buffer size is 512KB when flow director is disabled, hence it can hold > 8000 packets of 64 Bytes ⇒ handle an interrupt longer than 500 microseconds - <https://etherealmind.com/wp-content/uploads/2017/01/X520_to_XL710_Tuning_The_Buffers.pdf> )

When using Fortville, packets are by default dropped when RX descriptors are not available. Hence, by default, the only buffers available to store packets when a core is interrupted are the buffers pointed to by the RX descriptors.

A similar behavior (packets dropped when no descriptors available) is obtained on Niantic when using Virtual functions: to avoid "head of line" blocking, packets are dropped if no descriptor is available and virtual functions are used.

So, to avoid packet losses due to CPU core being interrupted when using Fortville (*or when using Niantic and \*SR-IOV\**), the number of RX descriptors should be configured high enough, for instance to 2048.

Setup number of rx descriptors through rte\_eth\_rx\_queue\_setup (see <http://www.dpdk.org/browse/dpdk/tree/examples/l3fwd/main.c#n990>

ret = rte\_eth\_rx\_queue\_setup(portid, queueid, nb\_rxd, socketid, NULL, pktmbuf\_pool[socketid]);

The number of TX descriptors should also be considered and depends on the application. Imagine the CPU core is interrupted and up to 2048 packets are now buffered through the RX descriptors. Once the interrupt is dealt with, up to 2048 packets can be received very fast by the application: as the packets are already in memory, they might arrive much faster than 10Gbps. Hence, when the application tries to forward those packets, the application might try to send those packets faster than 10Gbps. Some of those packets must be buffered before being sent to the 10 Gb/s link. Either the application takes care of this by buffering those packets, or those packets must be buffered in the TX descriptors. In that case, the number of TX descriptors should also be increased (e.g. up to 2048).

Increasing the number of RX and/or TX descriptors implies that you might have to increase the number of pre-allocated mbufs. This can have a small impact on performance (throughput), as more memory is being used.

Setup number of mbufs through rte\_pktmbuf\_pool\_create: (see <http://www.dpdk.org/browse/dpdk/tree/examples/l3fwd/main.c#n724>)

rte\_pktmbuf\_pool\_create(s, nb\_mbuf, MEMPOOL\_CACHE\_SIZE, 0, RTE\_MBUF\_DEFAULT\_BUF\_SIZE, socketid);

### Problem

A problem with reassigning kernel driver back to interface when DPDK vRouter is stopped.

On Compute node In file /opt/contrail/bin/vrouter-functions.sh (line 532) in s/\x1([0-9:.]+)[\x1]+/ \1/g there are missing letters from a to f. This should be corrected and that could impact on not binding interface back to interface kernel driver from UIO kernel driver when vRouter is stopped.

## Look for slave PCI addresses of vRouter --vdev argument  
DPDK\_BOND\_PCIS=`sed -nr \  
 -e '/^ \*command \*=/ {  
 s/slave=/\x1/g  
 s/[^\x1]+//  
 s/\x1([0-9:\.]+)[^\x1]+/ \1/g  
 p  
 }' \  
 ${VROUTER\_DPDK\_INI}`

The correct sed should have letters s/\x1([0-9a-f:\.]+)[^\x1]+/ \1/g.

This issue will be solved in release 5.0.1 <https://bugs.launchpad.net/juniperopenstack/+bug/1774403>

## vRouter CPU numbers and single queue VM

In non-multiqueue VNF with one DPDK interface, increasing the number of CPU cores for vRouter can actually decrease performance because of One to Many CPU cores queues are sending packets one by one what takes time and can produce microbursts.

![vrouter core numbers and single-queue VNF](data:image/png;base64;base64,)

vrouter core numbers and single-queue VNF

On the diagram cores one by one are sending traffic to VM and when last finish data processing potentially first will have no time (buffers) to send VM (virtio queue).

During this case microbursts affecting VNF will be observed on vRouter as TX errors.

# **Deployment considerations**

## Define number of resources required for vRouter DPDK

DPDK vrouter dimensioning is depending on following parameters:

* Cores for vrouter forwarding
* Cores for vrouter services threads and DPDK control threads
* Hugepages for vrouter

## Compute Node CPU capacity planning

When we are designing an OpenStack Contrail infrastructure we have to define how many CPU will be used for vRouter needs, how many for virtual instances and how many will remain to be used by the Operating system.

![Compute Node CPU capacity planning](data:image/png;base64;base64,)

Compute Node CPU capacity planning

## vrouter forwarding cores capacity planning

### First step: expected network throughput

Expected network throughput is the first thing to take into consideration.

We can take following assumption for vRouter dimensioning (this is the best scenario with an optimal setup) :

|  |  |  |  |
| --- | --- | --- | --- |
|  | 64 bytes packets | 512 bytes packets | 1500 bytes packets |
| lcore (sibling enabled) | 1 MPPS | 0.9 MPPS | 0.6 MPPS |
| physical CPU | 2 MPPS | 1.8 MPPS | 1.2 MPPS |

these values are depending on the actual customer environment. Real figures could be different.

**Scenario 1:.**

Let’s assume we want to be able to process 10 Gb/s of 512 bytes packet size in full duplex, we need 5 MPPS throughput at the vrouter level (2 x 10 x 1000 / 512 / 8).

So, we need at least 6 forwarding cores to be configured onto the vRouter (5 / 0.9).

**Scenario 2:.**

We need to be able to process 12 MPPS of 64 bytes packets onto our vRouter (in full duplex mode: 6 MPPS RX + 6 MPPS TX). So we need at least 12 forwarding cores (12 / 1).

### Second step: VM DPDK support and multi queues capability

considerations:

* whether the virtual instances are using DPDK or not.
* if DPDK is supported, the virtual instances support multiQ vNIC or not?

**not DPDK capable or not supporting DPDK multiQ vNIC.**

It is preferable not to use more than 4 forwarding cores onto the vRouter. If more than 4 forwarding cores are used onto the vrouter, some drop can occur at virtIO queue level due to the traffic burst that will be generated by the usage of several forwarding cores to deliver packet into a single Q.

**DPDK capable multiQ vNIC.**

The number of vRouter forwarding cores to be used will depend on:

* Linux Kernel release used onto the OpenStack compute node
* Maximum number of vCPU configured on DPDK virtual instance

The table below is providing the vRouter allocation rule to follow:

|  |  |  |
| --- | --- | --- |
|  | Number of Forwarding cores to use |  |
| Max Number of vCPU | Linux Kernel 3.X | Linux Kernel 4.X |
| N < 8 | >= N | >= N |
| N >= 8 | >= 8 | >= N |

**Scenario 1 and 2.**

Let’s assume we are using MultiQ vNIC virtual instances on RedHat OpenStack 13 platform. So, Linux Kernel 3.X will be used on compute nodes. These virtual instances will be configured with 12 vCPU. As Linux Kernel 3.X is used onto our compute nodes, each multiQ vNIC will be configured with 8 queues at maximum. So we need to use at least 8 forwarding cores to be configured onto the vRouter.

### Last step: sibling consideration

Then we have to take into consideration the purpose of the OpenStack Contrail platform.

1. high network throughput per vNIC

* If the customer is intending to use its OpenStack computes to host virtual instances requiring **very high network throughput per vNIC**, It is sometimes preferable **not to use** siblings on forwarding cores, and we could expect a 50% performance improvement per processing core.

|  |  |  |  |
| --- | --- | --- | --- |
|  | * 64 bytes packets | * 512 bytes packets | * 1500 bytes packets |
| * lcore (sibling enabled) | * 1.5 MPPS | * 1.3 MPPS | * 0.9 MPPS |
| * physical CPU | * 1.5 MPPS | * 1.3 MPPS | * 0.9 MPPS |

* these values are depending on the actual customer environment. Real figures could be different.

1. as many as possible virtual instances per compute node

* If the customer is willing to keep a **better capacity** on its compute nodes in order to start as many virtual instances as possible, it is preferable to **use CPU siblings** on forwarding cores.
* We are using 2 x 12 physical CPU computes.
* We need 5 Gb/s full duplex traffic throughput to be processed by Contrail vRouter (at least 6 forwarding core required). As we are using MultiQ Virtual instances with more than 8 vCPU onto Compute nodes running Linux 3.x Kernel, we have to allocate at least 8 forwarding cores onto Contrail vRouter.
* We do not foresee a higher network throughput expectation than the hypothesis taken for our current vRouter dimensioning.
* So we are preferring to keep more CPU for VM usage instead of Network performance improvement.
* We will use our CPU siblings for our forwarding cores.

So, we will use a vRouter configuration with 8 forwarding cores configured onto 4 Physical CPUs on NUMA0. Our compute nodes are fitted with 12 Physical CPUs per NUMA. So, 8 Physical CPUs - 16 logical cores - will remain available for other purposes (7 allocated - 14 logical cores - to VM instances and 1 allocated - 2 logical cores to Linux Operating System for Hypervisor needs).

**max throughput.**

We are using 2 x 12 physical CPU computes. We need 12 MPPS throughput on our vRouter (64 bytes packets) . At least 12 logical cores are required to get such a performance. As we are using MultiQ Virtual instances with more than 8 vCPU onto Compute nodes running Linux 3.x Kernel, we have to allocate at least 8 forwarding cores onto Contrail vRouter.

* If sibling is used we need to use 12 logical cores on our vRouter (6 Physical CPUs)
* If sibling is not used we need 8 physical cores on our vRouter (8 physical CPUs)

If we are using siblings we are saving 2 Physical CPUs. But, we probably won’t be able to reach the expected throughput. Indeed, our multiQ vNIC are configured with 8 queues. If 8 physical cores are used, we will be able to process each vNIC queue at 1.5 MPPS. So 12 MPPS for the eight queues (6 MPPS RX + 6 MPPS TX). But, if we are using siblings, we will only be able to process 1 MPPS each vNIC queue at 1 MPPS. So only 8 MPPS for the eight queues (4 MPPS RX + 4 MPPS TX).

* If we need 12 MPPS on vRouter distributed on several vNIC, we could use only 6 physical cores with their siblings (12 logical cores in total).
* If we need 12 MPPS for a single vNIC, it is preferable to use only 8 physical cores. We have a virtual instance which has **high network throughput requirements per vNIC**.

## vrouter services cores capacity planning

Service threads are used into the communication between vRouter dataplane (DPDK vrouter process) and the control plane (vrouter agent). They are involved in vNIC plugin to the vRouter, flow creation/deletion onto the vrouter. So we have two scenarios to consider :

**Packet Mode only.**

One single CPU will be enough for Service Threads. If hyperthreading is enabled, a single logical core would be enough. This CPU could be chosen on any NUMA node, e.g. NUMA#1

**Flow Mode only.**

We are allocating a single **Physical CPU** to services threads. If hyperthreading is enabled, **both logical cores** will be allocated to Service Threads. If lots of flows are required at a high rate, an additional CPU could be needed. These CPUs could be chosen on any NUMA node (but on the same NUMA).

**both packet and flow mode.**

We are running most of our vNIC in packet mode. Only a few of them will be using flow mode. We will allocate a Physical CPU on NUMA1 for vrouter Service Threads (as our forwarding cores have been allocated on NUMA0). We will use both logical cores on this physical CPU for our Service Threads.

## typical CPU assignment

Onto a Contrail OpenStack platform we have following kind of processes that will use CPUs:

* Operating system processes
* Nova compute etc processes
* vRouter DPDK service lightweight processes
  + packet processing threads
  + control and service threads **(20.03 and later release)**
* vRouter Agent (default is 2, this can be upgraded to 4 in high flow environment)
* vrouter DPDK forwarding thread

![CPU assignment typical setups](data:image/png;base64;base64,)

CPU assignment typical setups

ping? this is great diagram showing overall allocations. the numbering seems not correct. see [hwloc-ls GUI](#hwloc-ls) and lscpu

A (LD): the problem is that we are mixing platforms …​

All examples I’ve added in this document are comming from Orange which is using to kinds of plaforms (72 lcores or 48 lcores).

So, I’m trying to be consistent in perf guide. But some examples are provided from other platforms. So, it can lead to confusion.

CPU numbering is not always following same rules:

* some suppliers are using odd and even numbers to differentiate Numa0 from Numa1 CPUs
* others are using first half and second half numbers to differentiate Numa0 from Numa1 CPUs

This is bringing confusion …​

Here an example - 48 lcores:

# lscpu | grep NUMA  
NUMA node(s): 2  
NUMA node0 CPU(s): 0-11,24-35  
NUMA node1 CPU(s): 12-23,36-47  
Physical Cores are ID 0 to 23  
First half = Numa0  
Second half = Numa1  
Siblings are ID 24 to 27  
Here is another example 72 lcores (like Orange Model):  
Physical Cores are ID 0 to 35  
Even = Numa0  
Odd number = Numa1  
Siblings are ID 36 to 71  
NUMA node0 CPU(s):  
PHY cores: \*0 2 4 6 8 10 12 14 16 18 20 22 24 26 28 30 32 34\*  
HT cores : \*36 38 40 42 44 46 48 50 52 54 56 58 60 62 64 66 68 70\*  
NUMA node1 CPU(s):  
PHY cores: \*1 3 5 7 9 11 13 15 17 19 21 23 25 27 29 31 33 35\*  
HT cores : \*37 39 41 43 45 47 49 51 53 55 57 59 61 63 65 67 69 71\*  
Updated situation with 48 CPUs:  
NUMA node0 CPU(s):  
PHY cores: \*0 2 4 6 8 10 12 14 16 18 20 22\*  
HT cores : \*24 … 46\*  
NUMA node1 CPU(s):  
PHY cores: \*1 3 5 7 9 11 13 15 17 19 21 23\*  
HT cores : \*25 …. 47\*

And the diagram I’ve provided in the book:

![image](data:image/png;base64;base64,)

I can provide an updated diagram. But pay attention all netmask I’ve provided are following this numbering rule:

**0x154 …. Has to be changed everywhere if we are changing CPU model**

We are defining 4 CPU groups:

* vRouter
  + packet processing threads
  + service threads
* VNF (managed by Nova)
* OS, control threads (DPDK vRouter initial setup), etc

We are applying these allocation rules to get the best performance as possible:

* When Hyper Threading is used, we will book both physical CPUs and their sibling ones for DPDK vRouter packet processing threads.
* vRouter packet processing threads will be assigned with **physical CPUs** in same NUMA. **Sibling CPUs are unused**
* vRouter assigned CPUs and Nova assigned CPU will be isolated in order to prevent them from being used by any other application (or any OS task). Both isolcpu and tuned partitioning mechanisms will be used to get the best isolation as possible.

**ping? statement #1 and #2 above is conflicting.**

A (LD): yes, your right.

To be updated (last part of second sentence to be removed):

vRouter packet processing threads will be assigned with physical CPUs in same NUMA.

In the following example, we will describe a performance tuning configuration using a node with 36 physical cores split on 2 NUMA and Hyperthreading enabled (72 logical cores).

On this system we are applying the following typical CPU allocation:

* vRouter packet processing: 2,4,6,8,38,40,42,44 (NUMA 0)
  + 4 of them will be assigned to vrouter: 2,4,6,8
  + remaining ones are kept unassigned: 38,40,42,44
* vRouter service threads: 10,46 (NUMA 0)
* VNF (aka Nova CPU): 3,5,7,9,11-35,39,41,43,45,47-71 (NUMA 0 and 1)
* OS, vrouter control thread, other task: 0,1,36,37 (NUMA 0 and 1)

Configuration described below is really relevant when a Contrail 20.03 and later release is used. CPUs 2-35,38-71 will be allocated to Contrail DPDK vRouter and to Nova. They will be isolated using both tuned partitioning and isolcpus mechanisms. The diagram below is describing the target situation:

![CPU assignment example](data:image/png;base64;base64,)

CPU assignment example

When using a Contrail release 19.12 and earlier, this is not recommended to enforce any CPU isolation rule (for both vrouter and nova assigned CPU). As these release are not supporting control and service threads CPU pinning, any isolation rule could generate some instabilities and random packet drop period)

## Performance tests figures (DPDK vrouter)

In best case scenarios the vRouter can achieve 1,5Mpps per physical core.

The actual performance of the system depends on several parameters:

* VNF capabilities,
* traffic patterns,
* CPU, RAM speed,
* NICs capabilities,
* drivers,
* firmware,
* etc.

Juniper Networks recommends performing tests using a lab representative of the target production environment.

For standard deployments, 4 up to 8 physical cores are allocated. When HT siblings are not assigned for vRouter they **MUST NOT** be assigned for Nova or operating system because this can cause CPU steals.

![Juniper QA tests - 2018](data:image/png;base64;base64,)

*Juniper QA tests - 2018*

* vr - vRouter allocate on NUMA 0 or 1
* vm - VM allocated on NUMA 0 or 1
* [X]p[Y]ht - number of allocated physical cores with HT siblings

In this diagram we can see that:

* 1 lcore: with a single lcore allocated to the vrouter, we’ve got around 1.8 MPPS performance.
* 2 lcores: When 2 lcores are allocated to the vrouter, performance is falling to 0.5 MPPS per core (this is the impact of internal load balancing which is very inefficient for only 2 lcores).
* When 4 or more lcores are allocated to the vrouter, we can see a performance of 0.8 MPPS per lcore when siblings are used (1.6 MPPS per physical CPUl) and a performance of 1.2 MPPS per lecore when siblings are not used (1.2 MPPS at per physical CPU).

**ping? confusing. text makes sense, but not corelating to the diagram. 2p2ht means 2 pcores, both enabled ht⇒4lcores in use?**

A (LD):

It is consistent. Let see the situation with 4 lcores usage:

2 situations:

2p + 2h → diagram = 3 MPPS

4p + 0h → diagram = 5.2 MPPS

3 / 4 = 0.75 (almost 0.8) =⇒ 1,6 MPPS per Physical CPU

5.2 / 4 = 1.3 =⇒ 1,3 MPPS per Physical CPU (near to 1,25)

We can summarize this diagram performance result into following table:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **With Siblings** | **Without Siblings** |  |  |
|  | per lcore | per Phys. CPU | per lcore | per Phys. CPU |
| **1 lcore** | 1.8 MPPS | 1.8 MPPS | 1.8 MPPS | 1.8 MPPS |
| **2 lcores** | 0.5 MPPS | 1.0 MPPS | 1.0 MPPS | 1.0 MPPS |
| **>= 4 lcores** | 0.75 MPPS | 1.5 MPPS | 1.25 MPPS | 1.25 MPPS |

These tests have been done without DPDK control threads and vrouter service threads pinning.

before release 20.03 - release 19.12 and earlier (without the patch) some erratic drops can be seen when CPU isolation rules are enforced either on vrouter and or nova allocated CPUs. For these versions it is preferable not to enforce any CPU isolation rules to get the best performance as it has an impact on packet drops. the bests results are reached when no isolation mechanisms are enforced.

In 2020, new tests have been proceeded (in Juniper and customer labs) with DPDK control threads vrouter service threads pinning. In these tests (done on RedHat OpeStack platform + contrail 19.12 + patch for DPDK control threads and vrouter service threads pinning) we’ve enforced CPU isolation (with isolcpus and tuned).

![Juniper and customer tests summary - 2020 (19.12 + patch) - siblings used](data:image/png;base64;base64,)

*Juniper and customer tests summary - 2020 (19.12 + patch) - siblings used*

These tests have been done with 8 lcores and CPU siblings were used. vRouter physical interface was a bond of 2x10 Gb/s NIC (Intel Niantic cards).

MPPS per lcore is the number of packet per second that are processed at vrouter level. Given values are the performance seen at user level for a half duplex flow (outgoing only). For a full duplex flows (both outgoing and incoming direction) these values have to be divided by two.

On such a platform when packet size is more than 512 bytes we were reaching the physical interface maximum throughput. This is why performance per lcore seems to decrease at a very low rate for higher packet size.

We can use the results we’ve got for packet size below 512 bytes to extrapolate values for a higher packet size when we have more than 20 Gb/s available on vrouter physical interface.

In the diagram below, the MPPS per lcore values for 1024, 1280 and 1500 packet have been extrapolated using 64, 128, 256 and 512 packet size values :

![image](data:image/png;base64;base64,)

This diagram could help our customers to evaluate the number of lcores needed to get a given performance at vrouter level.

Of course these values are dependent on the customer’s actual setup and have to be revalidated on field. Real results can differ from what we’ve got in Juniper labs.

The best results will be achieved when:

* vRouter, VNF and NICs will be on the same NUMA.
  + It does not mean that other configurations are not allowed but some performance degradation can be observed (depends on traffic characteristic and NUMA allocation).
* Contrail vrouter threads are correctly pinned (available since 20.03 version) :
  + using CPU\_LIST for packet processing threads
  + using SERVICE\_CORE\_MASK and DPDK\_CTRL\_THREAD\_MASK for control and service threads (only available since 20.03 version)
  + core siblings are **not used** for physical core allocated to packet processing threads (see [Compute Node CPU capacity planning](#X7ba0f917e4f59d835a36e96cd9b2fba177ca55f) section)
* CPU allocated to DPDK vrouter and Nova are properly isolated with both tuned  
  partitioning and isolcpus mechanisms (contrail 20.03 and later version).

## Jumbo frame support

**Host.**

To enable Jumbo frames on tap and physical interfaces assign Jumbo on vhost0 interface.

# ifconfig vhost0 mtu 9000

On DPDK node the mtu needs to be set on vhost0 and it will update the pmd.

**Guest.**

Before Contrail 3.2.8 and 4.0.1 on DPDK Compute:

1. If it is a DPDK application then jumbo on the Guest interface(s) works (except i40e NICs)
2. If it is a Kernel application (Linux Socket Application) then jumbo on the guest interface(s) works from Contrail 3.2.8 / 4.0 (mergeable buffers). For more information, this code enhancement is tracked under <https://bugs.launchpad.net/juniperopenstack/+bug/1592935>

LP 1592935: DPDK: GRO and GSO support

Vrouter performs Tx and Rx TCP segmentation offload only in the kernel mode currently. It largely leverages kernel APIs for achieving this. However, in case of DPDK, the library lacks segmentation support due to which DPDK based vrouter could not do the offloads.

This commit overcomes the above limitation and adds receive offload and send offload support to DPDK. As a pre-requisite to this, it also adds mbuf chaining support and virtio mergeable buffer support.

There are limitations with jumbo frame support for Contrail Versions below 4.0.1 and 3.2.8:

DPDK Compute:

* if it is a DPDK application then jumbo on the Guest interface(s) WORKS.
* if it is a Kernel application (Linux Socket Application) then jumbo on the guest interface(s) DO NOT WORK.

Kernel Compute:

* if it is a Kernel application (Linux Socket Application) then jumbo on the Guest interface(s) works.

This issue is tracked under <https://bugs.launchpad.net/juniperopenstack/+bug/1731174> We do not support these offloads yet inside vrouter-dpdk.

LP 1731174: This is needed to support jumbo MTU in non-DPDK VM. Request from Orange vEPC - Ericsson

Starting from Contrail 4.0.1 and 3.2.8, jumbo frames are supported in all scenarios.

## Configure driver and network settings

Add parameters to configuration file /etc/contrail/contrail-vrouter-agent.conf

DEFAULT]  
platform = dpdk  
physical\_uio\_driver = $dpdk\_nic\_driver  
physical\_interface\_address = $dpdk\_dev\_pci;  
physical\_interface\_mac = $dpdk\_dev\_mac;

* **$dpdk\_dev\_pci** is an interface pci address (in case of bond it is 0000:00:00.0)
* **$dpdk\_dev\_mac** is a mac address assigned to interface (in case of bond the lower slaves mac)
* **$dpdk\_nic\_driver** as described in the section "UIO / VFIO" choose linux driver (default is igb\_uio)

## Configure nova scheduler and flavor

**nova scheduler.**

On every controller, add values AggregateInstanceExtraSpecFilter and NUMATopologyFilter to the scheduler\_default\_filters parameter in /etc/nova/nova.conf. Restart nova-scheduler.

Configure host aggregates:

openstack aggregate create dpdk  
openstack aggregate add host dpdk [hypervisor 1]  
openstack aggregate add host dpdk [hypervisor 2]  
openstack aggregate set --property dpdk=true dpdk

**Define flavors for VNFs.**

openstack flavor create --ram 8192 --disk 20 --vcpus 4 --public my-flavor  
openstack flavor set --property aggregate\_instance\_extra\_specs:dpdk=true my-flavor  
openstack flavor set --property hw:mem\_page\_size=large my-flavor  
openstack flavor set --property hw:cpu\_policy=dedicated my-flavor  
openstack flavor set --property hw:cpu\_thread\_policy=require my-flavor

that mem\_page\_size can have 1GB or 2048 values depending on hugepage size requirements of the VNF. Multiple flavors could be created in order to provide for both options.

* hw:cpu\_policy=dedicated - means that Nova will allocate physical cores and their sibling HT
* hw:cpu\_policy=isolated - means that Nova will allocate physical cores only
* hw:cpu\_policy=prefered - allocate range for VM and then system range will allocate cores dynamically. **DO NOT use this option with isolated CPUs!**

**Large pages are required** for each instance **(even any non-DPDK instance) running on hosts with DPDK vrouter**. If large pages are not present in the guest, the **interface will appear but will not function**. This is why, on a compute node running DPDK vrouter, openstack instances must use flavors having hw:mem\_page\_size=large property.

ping? didn’t say why..

A (LD): Indeed. See earlier explanations. Second sentence is explaining why.

*You just have to keep in mind that :*

*- Packet are put into memory at one place and never copied (only descriptors are moving from one Q to another)*

*- Consequently “memory” area where the packets are put must be shared between DPDK vrouter and all instances (whatever the instance is – DPDK or not DPDK)*

**Spawn a VM.**

openstack server create --image dpdk\_image --flavor my-flavor --nic net-id=276c706c-cf78-44ba-ba97-d9b9dbe36707 vm-dpdk-1

# **DPDK vrouter troubleshooting**

## vrouter fine tuning parameters (kernel and DPDK mode)

### Generic vrouter dimensioning parameters

ping? since 4.0?

A (LD): I do not know I do not have any 4.0 lab. I guess there is no difference (as we are telling “is still using”). But, it is not so important in my opinion. Let’s focus now on 19.X for this book. We can look for this information for the current (and internal only) perf guide document.

Since Contrail 5.0 release and later, Contrail is containerized. Kernel vrouter module is still using /etc/modprobe.d/vrouter.conf file to get specific dimensioning values. These parameters are**:**

* **vr\_flow\_entries** :maximum flow entries (default is 512K)
* **vr\_oflow\_entries** :maximum overflow entries (default is 8K)
* **vr\_bridge\_entries** :maximum bridge entries (default is 256K)
* **vr\_bridge\_oentries**:maximum bridge overflow entries
* **vr\_mpls\_labels** :maximum MPLS labels used in the node (default is 5K)
* **vr\_nexthops** :maximum next hops in the node (defaut is 512K since contrail 19.11 - 65K before)
* **vr\_vrfs** :maximum VRFs supported in the node
* **vr\_interfaces** :maximum interfaces that can be created (default is 4352); this can be modified from release 3.1.1.0 & 3.2
* **vrouter\_dbg** :1 to dump packets, 0 to disable (disabled by default)

***kernel vrouter*.**

On a containerized **Kernel mode vrouter**, in order to be able to define a specific value for these parameters we have to **create** or edit /etc/modprobe.d/vrouter.conf configuration file onto the compute host. Once done the vrouter interface and the vrouter agent container has also to be started:

$ ifdown vhost0  
$ ifup vhost0  
$ docker start contrail\_vrouter\_agent

vRouter parameters can be checked with :

$ docker exec contrail\_vrouter\_agent vrouter --info

It’s also possible to define vrouter option values via VROUTER\_MODULE\_OPTIONS environment variable in /etc/sysconfig/network-scripts/ifcfg-vhost0 file.

For instance, we can add the following line to this file to decrease the Next Hop limit:

VROUTER\_MODULE\_OPTIONS="vr\_nexthops=32768"

Then we are restarting vhost0 interface and vrouter agent container in order to get it applied.

***DPDK vrouter*.**

On a containerized **DPDK mode vrouter**, in order to be able to define a specific value for these parameters we have to use DPDK\_COMMAND\_ADDITIONAL\_ARGS variable into /etc/sysconfig/network-scripts/ifcfg-vhost0.

the syntax to be used is slightly different as for the Kernel mode vrouter. All parameters have to be prefixed with "--". eg:

DPDK\_COMMAND\_ADDITIONAL\_ARGS=”--vr\_nexthops=32768”

Once done the vrouter interface has to be restarted.

$ ifdown vhost0  
$ ifup vhost0

No need to start the vrouter agent container with the DPDK vrouter:

***Example*:.**

We will decrease the flow table size from 512 kB to 400 kB onto a **Kernel Mode** vrouter. Before the change we can display the flow table size using vrouter --info command:

$ sudo docker exec vrouter\_vrouter-agent\_1 vrouter --info | grep -i "flow table"  
Flow Table limit 524288  
Flow Table overflow limit 105472

vr\_flow\_entries parameter is set to 400000 in the vrouter.conf configuration file onto the host compute:

$ vi /etc/modprobe.d/vrouter.conf  
options vrouter vr\_flow\_entries=400000

Then we are restarting vhost0 interface :

$ ifdown vhost0  
$ ifup vhost0  
$ docker start contrail\_vrouter\_agent

After the change we can notice the new value:

$ sudo docker exec vrouter\_vrouter-agent\_1 vrouter --info | grep -i "flow table"  
Flow Table limit 400000  
Flow Table overflow limit 80896

If you are facing an issue with the router agent container which is not succeeding to go up, it’s probably due to a lack of memory.

You can try to free unused blocks using the following procedure :

$ sudo -i  
# ifdown vhost0  
# rmmod vrouter  
# free && sync && echo 3 > /proc/sys/vm/drop\_caches && free  
# modprobe vrouter  
# ifup vhost0

Cf: <https://github.com/Juniper/contrail-controller/wiki/Vrouter-Module-Parameters>

### Increase vrouter default value of dimensioning parameters (especially flow table)

Default parameters of vrouter have to be changed carefully. Some side effects could happen when changing this parameters, especially on system memory consumption.

For instance, in the previous section it has been described how to change vrouter setup and how to increase default size value for many table used by the vrouter. In some situations it could be needed to increase the number of hugepages allocated to the system.

For instance, we can sustain around 12000 flows per 2M hugepage. When not enough huge pages are available, vhost0 interface can’t be created at the vrouter startup:

[root@overcloud-contraildpdk-0 ~]# ifup vhost0  
b3a25600ece1637e82e017b01357826e2c0abd29e64e8464c67fc5ff61512732  
INFO: wait DPDK agent to run... 1  
INFO: wait DPDK agent to run... 2  
INFO: wait DPDK agent to run... 3  
INFO: wait DPDK agent to run... 4

We can see the following error messages into vrouter dpdk log file :

2019-06-19 14:59:02,619 VROUTER: Error mapping file /dev/hugepages2M/flow: Cannot allocate memory (12)  
2019-06-19 14:59:02,619 VROUTER: Error initializing flow table: Cannot allocate memory (12)

Number of allocated huge pages, and free huge pages, can be checked with following commands:

# cat /sys/devices/system/node/node0/hugepages/hugepages-2048kB/nr\_hugepages  
# cat /sys/devices/system/node/node0/hugepages/hugepages-2048kB/free\_hugepages

When the number of available hugepages fall to 0 (or is below to the needed value by the vrouter), we have to increase the number of hugepages allocated at the system startup.

In order to do so, we have to change GRUB config. Here we are setting 64 x 2M hugepages on the system:

# vi /etc/default/grub  
....  
TRIPLEO\_HEAT\_TEMPLATE\_KERNEL\_ARGS=" default\_hugepagesz=1GB hugepagesz=1G hugepages=10 hugepagesz=2M hugepages=64"  
GRUB\_CMDLINE\_LINUX="$\{GRUB\_CMDLINE\_LINUX:+$GRUB\_CMDLINE\_LINUX }$\{TRIPLEO\_HEAT\_TEMPLATE\_KERNEL\_ARGS}"

Once this file has been changed, we have to rebuild the grub config using this command (RedHat):

grub2-mkconfig -o /boot/grub2/grub.cfg

Once done, we are rebooting the node. After reboot, the number of hugepages can be checked with following commands:

# cat /proc/cmdline  
BOOT\_IMAGE=/boot/vmlinuz-3.10.0-957.10.1.el7.x86\_64 root=UUID=334f450f-1946-4577-a4eb-822bd33b8db2 ro console=tty0 console=ttyS0,115200n8 crashkernel=auto rhgb quiet default\_hugepagesz=1GB hugepagesz=1G hugepages=10 hugepagesz=2M hugepages=64  
# cat /sys/devices/system/node/node0/hugepages/hugepages-2048kB/nr\_hugepages  
64

If we want to be able to sustain 2 000 000 flows, we need to have around 164 pages (2,000,000/12,000). With the procedure seen earlier we are changing the number of hugepages allocated to the system:

[root@overcloud-contraildpdk-0 ~]# cat /sys/devices/system/node/node0/hugepages/hugepages-2048kB/nr\_hugepages  
164

Then, *vr\_flow\_entries* parameter is set to 2 000 000 into the vrouter.conf configuration file inside the vrouter agent container :

$ sudo docker exec -it vrouter\_vrouter-agent\_1 vi /etc/modprobe.d/vrouter.conf  
options vrouter vr\_flow\_entries=2000000

Then we are restarting vhost0 interface :

$ ifdown vhost0  
$ ifup vhost0

This last command should be successful:

[root@overcloud-contraildpdk-0 ~]# ifup vhost0  
72acf9590f7bbb76cf737c535e20665ace495c9cc5783d2014f8778363fef221  
INFO: wait DPDK agent to run... 1  
INFO: wait DPDK agent to run... 2  
INFO: wait vhost0 to be initilaized... 0/60  
INFO: wait vhost0 to be initilaized... 1/60  
INFO: vhost0 is ready.

Once done we can see that the number of available hugepages has fallen near to 0:

[root@overcloud-contraildpdk-0 ~]# cat /sys/devices/system/node/node0/hugepages/hugepages-2048kB/free\_hugepages  
7

And we can see the flow table size has been set to 2 000 000 :

[root@overcloud-contraildpdk-0 ~]# sudo docker exec -it contrail-vrouter-agent-dpdk vrouter --info | grep -i flow\ table  
Flow Table limit 2000000  
Flow Table overflow limit 400384

### 32 bits vrouter nexthop limit parameter (contrail release 19.11 and later)

In release 19.10 and earlier next hop id in contrail virtual router was 16 bits. Default value for next hop limit was set to 65536. In high-scaled environment next hop limit would often exceed leading to traffic drops. After reaching next hop limit contrail vrouter agent still sent new next hop adds to vrouter, on receiving new config. Failure in creating next hop did not raise any alarm. There was no accounting for usage of vrouter parameters like next hop, mpls label, vrf (cf <https://github.com/Juniper/contrail-controller/wiki/Vrouter-Module-Parameters> ).

Since 19.11 release next hop id in contrail virtual router is increased to 32 bits. New default value of next hop limit is set to 512k (512\*1024). Now, contrail vrouter can support up to 1M next hops. New specific alarms are raised once next hop limit exceeds and or once mpls label limit exceeds.

A watermark can be configured in agent configuration file (percentage of vr limits - values: [50-95]).

High Watermark is defined in /etc/contrail/contrail-vrouter-agent.conf. Low watermark in agent is high watermark – 5.

**Example:.**

{empty}[DEFAULT] vr\_object\_high\_watermark = 80

Nexthop and mpls label alarm is raised when count for these objects reaches one of these limits:

* watermark\*vr\_nexthops
* watermark\*vr\_mpls\_labels

Since 19.11 release, two new alarms have been created :

* **system-defined-vrouter-limit-exceeded alarm** (severity major)
  + This alarm is raised when nexthop or mpls labels count crosses high watermark.
  + This alarm is cleared when nexthop and mpls labels count becomes lower than the low watermark.
* **system-defined-vrouter-table-limit-exceeded** (severity critical)
  + This alarm is raised when nexthop or mpls labels count reaches nexthop or mpls labels count configured in vrouter.
  + This alarm is cleared once nexthop or mpls labels count goes below 95% of nexthop and mpls labels count configured in vrouter.
  + These alarms are raised when either nexthop or mpls labels or both have exceeded the limits.
  + The type of resource/table is available in the alarm

### vrouter networking parameters (MTU)

Some other parameters (like MTU) are directly set into /etc/sysconfig/network-scripts/ifcfg-vhost0.

$ sudo vi /etc/sysconfig/network-scripts/ifcfg-vhost0  
MTU=1400

Then vhost0 interface has to be restarted:

$ ifdown vhost0  
$ ifup vhost0

/etc/sysconfig/network-scripts/network-functions-vrouter-kernel-env can also be used.

## vrouter DPDK fine tuning parameters

### DPDK vrouter parameters

Main parameters that should be customized onto DPDK vrouters in order to get better performances are :

* mempool size (default 16384 Bytes)
* Physical NIC (PMD) TX and RX descriptors size (default 128)
* socket memory size

Since 20.03 release, some new parameters have been added in order to be able to configure :

* vrouter forwarding lcores TX and RX descriptors size
* yield deactivation on forwarding cores
* --dpdk\_ctrl\_thread\_mask : (20.03 and later version) CPUs to be used for vrouter control threads (CPU list or hexadecimal bitmask).
* --service\_core\_mask : (20.03 and later version) CPUs to be used for vrouter service threads (CPU list or hexadecimal bitmask).
* --yield\_option : (20.03 and later version) is used to enable or disable yield on forwarding cores (0 or 1 - enabled by default). In the case of --yield\_option 0, yield is disabled onto forwarding cores.
* --vr\_dpdk\_tx\_ring\_sz : (20.03 and later version) is used to define forwarding lcores TX Ring descriptor size (1024 by default). e.g., for --vr\_dpdk\_tx\_ring\_sz 2048, TX Ring descriptor size has been set to 2048.
* --vr\_dpdk\_rx\_ring\_sz : (20.03 and later version) is used to define forwarding lcores RX Ring descriptor size (1024 by default). e.g., --vr\_dpdk\_rx\_ring\_sz 2048 , RX Ring descriptor size has been set to 2048.
* --socket-mem : is used to define the amount of memory pre-allocated for contrail vrouter. In the case below, 1GB of huge-page memory is pre-allocated on NUMA node 0 and NUMA node 1. --socket-mem 1024,1024
* --vr\_mempool\_sz : is used to define mempool memory size. In the case below 128 MB mempool memory size is defined. --vr\_mempool\_sz 131072
* --dpdk\_txd\_sz : is used to define Physical NIC TX Ring descriptor size. In the case below 2048 bytes RX ring descriptor size is defined. --dpdk\_txd\_sz  
  2048
* --dpdk\_rxd\_sz : is used to define Physical NIC RX Ring descriptor size. In the case below 2048 bytes RX ring descriptor size is defined. --dpdk\_rxd\_sz  
  2048

These values have to be adjusted depending on:

* the inter NIC model used
* the number of NIC members of vhost0 bond
* the number of logical cores allocated to the vrouter

ping: great visualization! maybe worth a better quality image here

A (LD): as now we are using .doc word format, it will be easier for me to integrate better quality images. Let’s see how we will integrate images in the definitive document.

![vrouter parameters illustration](data:image/png;base64;base64,)

vrouter parameters illustration

### DPDK fine tuning rules (mainly for Intel NIC)

***MEMPOOL SIZE*.**

Following formula has to be used to define the mempool size (set of mbufs) to be configured on vrouter :

*mempool size = MAX(16384, 2 \* (number\_of\_RX\_descriptors + number\_of\_TX\_descriptors) \* number\_of\_vrouter\_cores \* number\_of\_ports\_in\_dpdk\_bond)*

ping? how to interpret this?

mempool\_size = 2\*(rxd+txd)\*\*C\*P \* (size of ring?)

1 pNIC has N queues =>  
 N rings/descriptors in RAM?  
 N forwarding cores => N rings in cores?

Provided mempool (that are containing membufs) size value is suitable to use in most cases. This value has to be confirmed by tests or monitoring of live traffic. Indeed, memory needs are depending on a lot of factors like : packets size, traffic load, bursts, number of virtual NIC, MTU, …​

In some situations it could be needed to increase mempool size above this calculated size. We can detect such a need onto vif interface counters. When mempool size is too low, we can see "no mbuf" high counters values :

$ vif --list | grep -B4 “no mbuf”  
vif0/0 PCI: 0000:00:00.0 (Speed 10000, Duplex 1)  
Type:Physical HWaddr:b8:85:84:44:50:d1 IPaddr:0.0.0.0  
Vrf:0 Mcast Vrf:65535 Flags:TcL3L2VpEr QOS:-1 Ref:152  
RX device packets:24559028 bytes:4969135442 errors:0 no mbufs:231501288288  
  
vif0/1 PMD: vhost0  
Type:Host HWaddr:b8:85:84:44:50:d1 IPaddr:192.168.63.40  
Vrf:0 Mcast Vrf:65535 Flags:L3DEr QOS:-1 Ref:18  
RX device packets:596147 bytes:456776973 errors:0 no mbufs:170086

Increasing the mempool size gives lower performance and higher caches misses. So it is preferable not to oversize this value and to adjust it to the real needs.

***TX/RX DESCRIPTOR SIZE*.**

For Intel Niantic NIC family (without SR-IOV) used default value for TX and RX descriptor size has to be kept (128). For Intel Fortville NIC family (and Intel Niantic NIC family when SR-IOV is used), TX and RX descriptor size has to be increased to 2048.

|  |  |  |
| --- | --- | --- |
|  | **SR-IOV** **used** | **RX/TX descriptor size** |
| **Niantic** | No | 128 |
| Yes | 2048 |  |
| **Fortville** | No | 2048 |
| Yes | 2048 |  |

***SOCKET MEMORY SIZE*.**

Following formula has to be used to define the socket memory size to be configured on vrouter :

* if mempool size ⇐ 131072 then use **socketmem = 1024**
* if mempool size > 131072 then use **socketmem = 2048**

***CPU CORE\_MASK*.**

For DPDK CPU allocation (CPU affinity mask definition), it is preferable to follow rules hereafter :

* CPU 0 should always be left for the host process
* CPUs should be associated with NUMA node of the DPDK interface
* CPU siblings (in case of Hyper-threading) should be added together
* CPUs assigned to PMD should be excluded from nova scheduling using NovaVcpuPinset

Following command gives the siblings of a CPU:

cat /sys/devices/system/cpu/cpu<cpu no>/topology/thread\_siblings\_list

*Example of vrouter dpdk setup with Intel NIC cards (SR-IOV not used)*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **#LCORES** | **#BOND MEMBERS** | **TX/RX DESC SIZE** | **MEMPOOL SIZE** | **SOCKET MEM** |
| **Default Setup** | 4 | N/A | 128 | N/A | N/A |
| **Niantic Family (82599/X520)** **10G interface** | 4 | 2 | 128 | 16384 | 1024 |
| 8 | 2 | 128 | 16384 | 1024 |  |
| **Fortville Family (XL 710)** **40G interfaces** | 4 | 2 | 2048 | 65536 | 1024 |
| 8 | 2 | 2048 | 131072 | 1024 |  |

Hence, in /etc/contrail/supervisord\_vrouter\_files/contrail-vrouter-dpdk.ini we have to put above parameters:

* **4 or 8 logical cores on 2 Niantic bond members - 2 NUMA nodes**
* command=/bin/taskset \*<CPU 4 or 8 cores affinity>\* /usr/bin/contrail-vrouter-dpdk  
  --socket-mem 1024,1024 …
* **4 logical cores on 2 Fortville bond members - 2 NUMA nodes**
* command=/bin/taskset \*<CPU 4 cores affinity>\* /usr/bin/contrail-vrouter-dpdk  
  --dpdk\_rxd\_sz 2048 --dpdk\_txd\_sz 2048 --vr\_mempool\_sz 65536  
  --socket-mem 1024,1024 …
* **8 logical cores on 2 Fortville bond members - 2 NUMA nodes**
* command=/bin/taskset \*<CPU 8 cores affinity>\* /usr/bin/contrail-vrouter-dpdk  
  --dpdk\_rxd\_sz 2048 --dpdk\_txd\_sz 2048 --vr\_mempool\_sz 131072  
  --socket-mem 1024,1024 …

### DPDK vouter parameters provisioning

DPDK fine tuning setup has first to be defined before Contrail rollout into the used OpenStack Contrail deployment tools.

For instance, if TripleO is used, specific parameters have to be defined into ContrailDpdkOptions variable. This variable is used to fulfill *DPDK\_COMMAND\_ADDITIONAL\_ARGS* environment variable for DPDK vrouter container instance. If Ansible is used, *DPDK\_COMMAND\_ADDITIONAL\_ARGS* parameter can be used.

***For instance with TripleO* :.**

An environment file (<tripleO root dir>/environments/contrail/contrail-service.yaml) has to be used to declare ContrailDpdkOptions value. With TripleO there are two possibilities:

First : declare this parameter at global level (same value for any DPDK roles):

parameter\_defaults:  
 \*ContrailDpdkOptions: "--yield\_option 0 …"\*

Second : declare this parameter at role level (specific value for each DPDK roles):

# role specific variables:  
parameter\_defaults:  
 <Role Name>Parameters:  
 ContrailSettings:  
 # for service threads  
 SERVICE\_CORE\_MASK: ”0x400000000400”  
 # for ctrl threads  
 DPDK\_CTRL\_THREAD\_MASK: ”0x2B00000002B”  
 ContrailDpdkOptions: “--yield\_option 0 …”

For instance with Ansible:

instances:  
 bms1:  
 provider: bms  
 ip: 192.204.216.44  
 roles:  
 vrouter:  
 AGENT\_MODE: dpdk  
 SERVICE\_CORE\_MASK: ”0x400000000400”  
 DPDK\_CTRL\_THREAD\_MASK: ”0x2B00000002B”  
 CPU\_CORE\_MASK: ”0x154000000154”  
 DPDK\_COMMAND\_ADDITIONAL\_ARGS: “--yield\_option 0 …”

When contrail 5.0 or later release is used, dpecified valuers for these parameters will be put into /etc/sysconfig/network-scripts/ifcfg-vhost0 config file on each DPDK compute node..

### DPDK vouter parameters configuration (5.0 and later versions)

Since Contrail 5.0 release and later, Contrail is containerized and DPDK parameters are no more defined into contrail-vrouter-dpdk.ini file but are installed by /bin/bash /entrypoint.sh into contrail-vrouter-agent-dpdk container.

At the startup, DPDK vrouter container which will run /bin/bash /entrypoint.sh, which is applying specific DPDK configuration defined into DPDK\_COMMAND\_ADDITIONAL\_ARGS environment variable.

When a specific DPDK setup update is required after the initial rollout, it could be defined into /etc/sysconfig/network-scripts/network-functions-vrouter-dpdk-env file. In this file we can override DPDK\_COMMAND\_ADDITIONAL\_ARGS value defined into the deployment script.

**Example :.**

We are adding new specific TX and RX ring size (256 bytes instead of 128 bytes default value) and using a specific CPU mask into network-functions-vrouter-dpdk-env file :

$ vi /etc/sysconfig/network-scripts/network-functions-vrouter-dpdk-env  
#!/bin/bash  
DPDK\_COMMAND\_ADDITIONAL\_ARGS="--dpdk\_rxd\_sz 256 --dpdk\_txd\_sz 256"  
CPU\_LIST=0x154

Specific DPDK fine tuning could also be defined into /etc/sysconfig/network-scripts/ifcfg-vhost0 file.

$ vi /etc/sysconfig/network-scripts/ifcfg-vhost0  
...  
DPDK\_COMMAND\_ADDITIONAL\_ARGS="--dpdk\_rxd\_sz 256 --dpdk\_txd\_sz 256"  
CPU\_LIST=0x154  
MTU=9000

In order to get these new values taken into consideration we have to restart vhost0 interface, After vhost0 interface restart the new values have been applied.

$ sudo ifdown vhost0  
$ sudo ifup vhost0  
$ sudo ps -ef | grep vrouter-dpdk  
root 97244 97226 0 16:30 ? 00:00:00 /bin/bash /entrypoint.sh /usr/bin/contrail-vrouter-dpdk  
root 97476 97244 99 16:30 ? 00:01:13 /usr/bin/contrail-vrouter-dpdk --no-daemon --dpdk\_rxd\_sz 256 --dpdk\_txd\_sz 256 --socket-mem 1024 1024 --vlan\_tci 20 --vlan\_fwd\_intf\_name bond0 --vdev eth\_bond\_bond0,mode=4,xmit\_policy=l23,socket\_id=0,mac=3c:fd:fe:bc:f7:e8,lacp\_rate=0,slave=0000:03:00.0,slave=0000:03:00.1  
heat-ad+ 97795 92566 0 16:30 pts/9 00:00:00 grep --color=auto vrouter-dpdk

We can also see into contrail dpdk vrouter logs, the new values in use :

$ vi /var/log/containers/contrail/contrail-vrouter-dpdk.log  
...  
2019-04-19 16:30:41,411 VROUTER: vRouter version: \{"build-info": [\{"build-time": "2019-04-11 23:47:32.407280", "build-hostname": "rhel-7-builder-juniper-contrail-ci-c-0000225573.novalocal", "build-user": "zuul", "build-version": "5.1.0"}]}  
2019-04-19 16:30:41,411 VROUTER: DPDK version: DPDK 18.05.1  
2019-04-19 16:30:41,427 VROUTER: Log file : /var/log/contrail/contrail-vrouter-dpdk.log  
2019-04-19 16:30:41,427 VROUTER: Using VLAN TCI: 20  
2019-04-19 16:30:41,427 VROUTER: Bridge Table limit: 262144  
2019-04-19 16:30:41,427 VROUTER: Bridge Table overflow limit: 53248  
2019-04-19 16:30:41,427 VROUTER: Flow Table limit: 524288  
2019-04-19 16:30:41,427 VROUTER: Flow Table overflow limit: 105472  
2019-04-19 16:30:41,427 VROUTER: MPLS labels limit: 5120  
2019-04-19 16:30:41,427 VROUTER: Nexthops limit: 65536  
2019-04-19 16:30:41,427 VROUTER: VRF tables limit: 4096  
2019-04-19 16:30:41,427 VROUTER: Packet pool size: 16384  
2019-04-19 16:30:41,427 VROUTER: PMD Tx Descriptor size: 256  
2019-04-19 16:30:41,427 VROUTER: PMD Rx Descriptor size: 256  
2019-04-19 16:30:41,427 VROUTER: Maximum packet size: 9216  
2019-04-19 16:30:41,427 VROUTER: Maximum log buffer size: 200  
2019-04-19 16:30:41,427 VROUTER: EAL arguments:  
2019-04-19 16:30:41,427 VROUTER: -n "4"  
2019-04-19 16:30:41,427 VROUTER: --socket-mem "1024,1024"  
2019-04-19 16:30:41,427 VROUTER: --vdev "eth\_bond\_bond0,mode=4,xmit\_policy=l23,socket\_id=0,mac=3c:fd:fe:bc:f7:e8,lacp\_rate=0,slave=0000:03:00.0,slave=0000:03:00.1"  
2019-04-19 16:30:41,427 VROUTER: --lcores "(0-2)@(0-71),(8-9)@(0-71),10@2,11@4,12@6,13@8"  
2019-04-19 16:30:41,432 EAL: Detected 72 lcore(s)  
2019-04-19 16:30:41,432 EAL: Detected 2 NUMA nodes

**But, be careful, after this operation contrail\_vrouter\_agent is stopped, we have to start it :**

[heat-admin@oln-compute-dpdk-0 ~]$ sudo docker ps --all  
CONTAINER ID IMAGE COMMAND CREATED STATUS PORTS NAMES  
300c9d8b9987 10.19.2.1:8787/contrail-nightly/contrail-vrouter-agent-dpdk:5.1.0-0.655-rhel-queens "/entrypoint.sh /u..." 35 seconds ago Up 34 seconds contrail-vrouter-agent-dpdk  
b936827c6999 10.19.2.1:8787/contrail-nightly/contrail-vrouter-agent:5.1.0-0.538-rhel-queens "/entrypoint.sh /u..." 8 days ago Exited (0) 6 minutes ago contrail\_vrouter\_agent  
...

In order to start contrail\_vrouter\_agent container we have to issue the following command :

$ sudo docker start contrail\_vrouter\_agent

## Connectivity Troubleshooting

### How to check vrouter connectivity

Verify if VM was started on proper DPDK Compute node.

# openstack server list  
...get VM UUID...  
# nova show <VM\_UUID>

Verify if tap interface has vhostuser type.

# virsh list  
 Id Name State  
 ---------------------------------------------------  
 5 instance-000032d2 running  
  
# virsh dumpxml instance-000032d2 | grep -A 6 "interface type"  
 <interface type='vhostuser'>  
 <mac address='02:7f:8e:16:17:ae'/>  
 <source type='unix' path='/var/run/vrouter/uvh\_vif\_tap7f8e1617-ae' mode='client'/>  
 <model type='virtio'/>  
 <alias name='net0'/>  
 <address type='pci' domain='0x0000' bus='0x00' slot='0x03' function='0x0'/>  
 </interface>

Use vif --list to match the tap interface name to a vif identifier.

# vif --list  
vif0/0 OS: pkt0  
 Type:Agent HWaddr:00:00:5e:00:01:00 IPaddr:0  
 Vrf:65535 Flags:L3 MTU:1514 Ref:2  
 RX packets:6591 bytes:648577 errors:0  
 TX packets:12150 bytes:1974451 errors:0  
vif0/1 OS: vhost0  
 Type:Host HWaddr:00:25:90:c3:08:68 IPaddr:0  
 Vrf:0 Flags:L3 MTU:1514 Ref:3  
 RX packets:3446598 bytes:4478599344 errors:0  
 TX packets:851770 bytes:1337017154 errors:0  
vif0/2 OS: p1p0p0 (Speed 1000, Duplex 1)  
 Type:Physical HWaddr:00:25:90:c3:08:68 IPaddr:0  
 Vrf:0 Flags:L3 MTU:1514 Ref:22  
 RX packets:1643238 bytes:1391655366 errors:2812  
 TX packets:3523278 bytes:6806058059 errors:0  
vif0/4 OS: tap7f8e1617-ae  
 Type:Virtual HWaddr:00:00:5e:00:01:00 IPaddr:192.168.0.17  
 Vrf:1 Flags:PL3L2D MTU:9160 Ref:23  
 RX packets:60 bytes:4873 errors:0  
 TX packets:21 bytes:2158 errors:0

Use vif --get to check if tap interface is connected to correct RI and TX / RX counters are increasing.

# vif --get 4  
Vrouter Interface Table  
  
Flags: P=Policy, X=Cross Connect, S=Service Chain, Mr=Receive Mirror  
 Mt=Transmit Mirror, Tc=Transmit Checksum Offload, L3=Layer 3, L2=Layer 2  
 D=DHCP, Vp=Vhost Physical, Pr=Promiscuous, Vnt=Native Vlan Tagged  
 Mnp=No MAC Proxy, Dpdk=DPDK PMD Interface, Rfl=Receive Filtering Offload, Mon=Interface is Monitored  
 Uuf=Unknown Unicast Flood, Vof=VLAN insert/strip offload, Df=Drop New Flows, Proxy=MAC Requests Proxied Always  
  
vif0/4 PMD: tap7f8e1617-ae  
 Type:Virtual HWaddr:00:00:5e:00:01:00 IPaddr:192.168.0.17  
 Vrf:1 Flags:PL3L2D QOS:-1 Ref:23  
 RX queue errors to lcore 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0  
 RX packets:29 bytes:1218 errors:0  
 TX packets:29 bytes:1218 errors:0  
 TX port packets:0 errors:29  
 Drops:0

Use vifdump command to dump traffic on tap interface.

# vifdump -i 4  
vif0/4 PMD: tap7f8e1617-ae  
tcpdump: verbose output suppressed, use -v or -vv for full protocol decode  
listening on mon4, link-type EN10MB (Ethernet), capture size 262144 bytes  
15:01:17.004641 ARP, Request who-has 192.168.0.17 tell 192.168.0.2, length 28  
15:01:19.004610 ARP, Request who-has 192.168.0.17 tell 192.168.0.2, length 28

Check contrail-status.

# contrail-status -d

Use dpdk\_nic\_bind.py command to verify proper binding of NICs to proper Linux driver.

# /opt/contrail/bin/dpdk\_nic\_bind.py -s

### vRouter vif queues setup

When the router boots up, it displays a message about its logical cores numbering and pNIC and vNIC queues logical core pinning into contrail-vrouter-dpdk-stdout.log file.

First vif to be initialized, is physical NIC, vif 0/0 :

2019-02-06 10:15:40,516 VROUTER: Adding vif 0 (gen. 1) eth device 2 PCI 0000:00:00.0 MAC 00:00:00:00:00:00 (vif MAC b8:85:84:44:50:83)  
2019-02-06 10:15:40,516 VROUTER: Using 64 TX queues, 4 RX queues  
...  
2019-02-06 10:15:40,831 VROUTER: lcore 10 TX to HW queue 0  
2019-02-06 10:15:40,831 VROUTER: lcore 11 TX to HW queue 1  
2019-02-06 10:15:40,831 VROUTER: lcore 12 TX to HW queue 2  
2019-02-06 10:15:40,831 VROUTER: lcore 13 TX to HW queue 3  
2019-02-06 10:15:40,831 VROUTER: lcore 8 TX to HW queue 4  
2019-02-06 10:15:40,831 VROUTER: lcore 9 TX to HW queue 5  
2019-02-06 10:15:40,831 VROUTER: lcore 10 RX from HW queue 0  
2019-02-06 10:15:40,831 VROUTER: lcore 11 RX from HW queue 1  
2019-02-06 10:15:40,831 VROUTER: lcore 12 RX from HW queue 2  
2019-02-06 10:15:40,831 VROUTER: lcore 13 RX from HW queue 3

On vif 0/0, 4 queues are configured and pinned to one dedicated "packet processing core". They are queues 0 to 3, pinned to lcore 10 to 13.

Later on, vNIC vif 0/N are also initialized :

2019-02-13 14:37:16,250 VROUTER: Adding vif 3 (gen. 4) virtual device tapc02d2743-e3  
2019-02-13 14:37:16,250 VROUTER: lcore 11 TX to HW queue 0  
2019-02-13 14:37:16,250 VROUTER: lcore 12 TX to HW queue 1  
2019-02-13 14:37:16,250 VROUTER: lcore 13 TX to HW queue 2  
2019-02-13 14:37:16,250 VROUTER: lcore 8 TX to HW queue 3  
2019-02-13 14:37:16,250 VROUTER: lcore 9 TX to HW queue 4  
2019-02-13 14:37:16,250 VROUTER: lcore 10 TX to HW queue 5  
2019-02-13 14:37:16,250 VROUTER: lcore 11 RX from HW queue 0  
2019-02-13 14:37:16,250 VROUTER: lcore 12 RX from HW queue 1  
2019-02-13 14:37:16,250 VROUTER: lcore 13 RX from HW queue 2  
2019-02-13 14:37:16,250 VROUTER: lcore 10 RX from HW queue 3  
2019-02-13 14:37:16,251 UVHOST: Adding vif 3 virtual device tapc02d2743-e3  
2019-02-13 14:37:16,251 UVHOST: vif (server) 3 socket tapc02d2743-e3 FD is 76

On vif 0/0, 4 queues are configured and pinned to one dedicated "packet processing core". They are also queues 0 to 3, pinned to lcore 10 to 13. We can notice that cpu to queue mapping is not the same on all vif interfaces.

PS: When the vif is created. it’s important to check it has be done in server mode :

2019-09-16 12:32:34,069 UVHOST: Adding vif 3 virtual device tape6b3d698-95  
2019-09-16 12:32:34,069 VROUTER: Adding vif 4 (gen. 7) virtual device tap32da3a01-1e  
2019-09-16 12:32:34,069 UVHOST: vif (server) 3 socket tape6b3d698-95 FD is 65

In our latest release (5.1 and above), a message like:

2019-09-16 12:32:34,069 UVHOST: vif (client) 3 socket tape6b3d698-95 FD is 65

Means the vif interface has not been properly created by the vrouter.

### vRouter vif queues activation

First the a connected message is confirming the socket is well connected. Then, as soon as QEMU sending VHOST\_USER\_SET\_VRING\_ENABLE (message 18) message, ring is enabled from vrouter side:

2019-09-12 12:46:40,445 UVHOST: connected to /var/run/vrouter/uvh\_vif\_tapfe589e24-ae for uvhost socket FD 190  
2019-09-12 12:46:45,859 UVHOST: Client \_tapfe589e24-ae: handling message 1  
2019-09-12 12:46:45,859 UVHOST: Client \_tapfe589e24-ae: handling message 15  
2019-09-12 12:46:45,859 UVHOST: Client \_tapfe589e24-ae: handling message 16  
2019-09-12 12:46:45,859 UVHOST: Client \_tapfe589e24-ae: handling message 17  
2019-09-12 12:46:45,860 UVHOST: Client \_tapfe589e24-ae: no handler defined for message 3  
2019-09-12 12:46:45,860 UVHOST: Client \_tapfe589e24-ae: handling message 1  
2019-09-12 12:46:45,860 UVHOST: Client \_tapfe589e24-ae: handling message 13  
2019-09-12 12:46:45,860 UVHOST: Client \_tapfe589e24-ae: handling message 13  
2019-09-12 12:46:52,274 UVHOST: Client \_tapfe589e24-ae: handling message 18

As soon as this last message is received, the vrouter interface is active. If this last message is not received from QEMU by Contrail vrouter, the interface will be disabled :

2019-09-12 12:47:29,107 UVHOST: connected to /var/run/vrouter/uvh\_vif\_tape75222a7-31 for uvhost socket FD 212  
2019-09-12 12:47:35,733 UVHOST: Client \_tape75222a7-31: handling message 1  
2019-09-12 12:47:35,733 UVHOST: Client \_tape75222a7-31: handling message 15  
2019-09-12 12:47:35,733 UVHOST: Client \_tape75222a7-31: handling message 16  
2019-09-12 12:47:35,733 UVHOST: Client \_tape75222a7-31: handling message 17  
2019-09-12 12:47:35,733 UVHOST: Client \_tape75222a7-31: no handler defined for message 3  
2019-09-12 12:47:35,733 UVHOST: Client \_tape75222a7-31: handling message 1  
2019-09-12 12:47:35,734 UVHOST: Client \_tape75222a7-31: handling message 13  
2019-09-12 12:47:35,734 UVHOST: Client \_tape75222a7-31: handling message 13  
2019-09-12 12:53:04,854 UVHOST: Client \_tape75222a7-31: shutdown at message receiving  
2019-09-12 12:53:04,854 UVHOST: Client \_tape75222a7-31: unmapping 0 memory regions:  
2019-09-12 12:53:05,980 UVHOST: Client \_tape75222a7-31: unmapping 0 memory regions

Here, more than 5 minutes after being connected to the socket, the VHOST\_USER\_SET\_VRING\_ENABLE has still not been received by the vrouter. So, the interface is being shut.

Here are the User space VHOST message bound for each ID :

|  |  |
| --- | --- |
| **Message** | **ID** |
| VHOST\_USER\_NONE | 0 |
| VHOST\_USER\_GET\_FEATURES | 1 |
| VHOST\_USER\_SET\_FEATURES | 2 |
| VHOST\_USER\_SET\_OWNER | 3 |
| VHOST\_USER\_RESET\_OWNER | 4 |
| VHOST\_USER\_SET\_MEM\_TABLE | 5 |
| VHOST\_USER\_SET\_LOG\_BASE | 6 |
| VHOST\_USER\_SET\_LOG\_FD | 7 |
| VHOST\_USER\_SET\_VRING\_NUM | 8 |
| VHOST\_USER\_SET\_VRING\_ADDR | 9 |
| VHOST\_USER\_SET\_VRING\_BASE | 10 |
| VHOST\_USER\_GET\_VRING\_BASE | 11 |
| VHOST\_USER\_SET\_VRING\_KICK | 12 |
| VHOST\_USER\_SET\_VRING\_CALL | 13 |
| VHOST\_USER\_SET\_VRING\_ERR | 14 |
| VHOST\_USER\_GET\_PROTOCOL\_FEATURES | 15 |
| VHOST\_USER\_SET\_PROTOCOL\_FEATURES | 16 |
| VHOST\_USER\_GET\_QUEUE\_NUM | 17 |
| VHOST\_USER\_SET\_VRING\_ENABLE | 18 |
| VHOST\_USER\_MAX | 19 |

PS: Files into following directories have to be investigated in order to check a vif has been properly enabled :

* /var/run/vrouter/ : uvh\_tap file has to be present for each virtual instance virtual port
* /var/lib/vrouter/ports : files describing virtual instance port properties

## Packet drop troubleshooting

### Interface traffic counters

To verify packet and error statistics for all interfaces.

# vif --list --rate  
 Interface rate statistics  
 ------------------------  
 Interface name VIF ID RX TX  
 Errors Packets Errors Packets  
 Physical: bondB vif0/0 0 644 0 888  
 Host: vhost0 vif0/1 0 0 0 0  
 Agent: unix vif0/2 0 0 0 0  
 Virtual: tapf7d6196c-81 vif0/3 0 0 0 0  
 Virtual: tapbd746390-d8 vif0/4 0 0 0 0  
 Virtual: tap122e8e7b-33 vif0/5 0 0 0 0  
 Virtual: tap48f25122-9e vif0/6 0 20 0 98  
 Virtual: tap3d147039-e9 vif0/7 0 25 0 20

Identify vRouter statistics (per core). Use without --core to get total interface statistics.

# vif --get 0 --core 10 --rate  
  
 Interface rate statistics  
 -------------------------  
  
 Vrouter Interface Table  
  
 Flags: P=Policy, X=Cross Connect, S=Service Chain, Mr=Receive Mirror  
 Mt=Transmit Mirror, Tc=Transmit Checksum Offload, L3=Layer 3, L2=Layer 2  
 D=DHCP, Vp=Vhost Physical, Pr=Promiscuous, Vnt=Native Vlan Tagged  
 Mnp=No MAC Proxy, Dpdk=DPDK PMD Interface, Rfl=Receive Filtering Offload, Mon=Interface is Monitored  
 Uuf=Unknown Unicast Flood, Vof=VLAN insert/strip offload, Df=Drop New Flows, Proxy=MAC Requests Proxied Always  
  
 vif0/0 PCI: 0000:00:00.0 (Speed 10000, Duplex 1)  
 Type:Physical HWaddr:3c:fd:fe:9c:c2:c5 IPaddr:0.0.0.0  
 Vrf:0 Flags:TcL3L2Vp QOS:-1 Ref:46  
 Core 10 RX device packets:0 bytes:0 errors:0  
 Core 10 RX port packets:15 errors:0  
 Core 10 RX queue packets:15 errors:0  
 RX queue errors to lcore 0 0 0 0 0 0 0 0 0 0 0 0 0 0  
 Core 10 RX packets:0 bytes:0 errors:0  
 Core 10 TX packets:0 bytes:189 errors:0  
 Core 10 TX queue packets:0 errors:0  
 Core 10 TX port packets:0 errors:0  
 Core 10 TX device packets:0 bytes:0 errors:0  
 Drops:8772364

Each physical core is mapped to a virtual core starting from 10 to 10+N. (Don’t confuse these lcores with host CPU cores). In the case of MPLSoGRE one core will receive all the pkts and sprays to other cores.

Cycle through the lcores from 10 to 10+(N-1) where N is the no of cores assigned to vrouter.

**Counters description**

|  |  |
| --- | --- |
| **Counter** | **Description** |
| **RX device** | counter of received packets by physical interface (NIC card), used only for vif 0/0. **WARNING!** counters are from vif 0/0 not from physical NIC |
| **RX port** | counter of received packets by logical port (aka PMD statistics) |
| **RX queue** | counter of inter core communication queues usage |
| **RX queue errors** | error counter of lcores queues usage, physical cores used for packets pulling. lcores ID starting from position 10 |
| **RX packets** | counter of received packets by "processing" core. This is the packets received by vrouter (after passing through NIC, PMD and load-balancing core). |
| **TX device** | counter of sent packets by physical interface (NIC card), used only for vif 0/0. **Warning!** counters are from vif 0/0 not from physical NIC. |
| **TX port** | counter of sent packets by logical port (aka PMD statistics) |
| **TX queue** | counter of inter core communication queues usage |
| **TX queue errors** | error counter of lcores queues usage, physical cores used for packets pulling. lcores ID starting from position 10. |
| **TX packets** | counter of sent packets by "processing" core. |
| **Drops** | counter of drops, to get more info run command with option --get-drop-stats |
| **Syscalls** | number of interrupts raised in the guest using eventfd (wait/notify mechanism by user-space applications, and by the kernel to notify user-space applications of events). |

### Packet flow from a Compute Physical NIC to a VM NIC - counters placement

Compute physical vif is always defined as vif0/0 into the vrouter. vNIC vif are defined as vif0/N (with N above or equal 3).

From underlay to virtual instances, packets are processed into 3 differents steps :

* vif0 packet polling by a polling core
* vif0 packet processing by a forwarding core
* vif0/n packet delivery by a forwarding core

In order to check the 2 first steps, we have to use counters on vif0/0. For the last one, we have to use counters on vif0/n. In the following diagram is shown counters that we have to check on each interface to be able to follow packets processing from vif0/0 to vif0/n into the vrouter :

![Packet flow from a Compute Physical NIC to a VM NIC - counters placement](data:image/png;base64;base64,)

**Packet flow from a Compute Physical NIC to a VM NIC - counters placement**

comparing with:

![image](data:image/png;base64;base64,)

Here on vif 0/0, RX port and RX packets have the same value :

vif0/0 PCI: 0000:00:00.0 (Speed 10000, Duplex 1)  
 Type:Physical HWaddr:b8:85:84:44:50:83 IPaddr:0.0.0.0  
 Vrf:0 Mcast Vrf:65535 Flags:TcL3L2VpEr QOS:-1 Ref:147  
 RX device packets:11581241437 bytes:4298162385219 errors:0  
 RX port packets: 2067782 errors:0  
 RX queue packets:15 errors:0  
 RX queue errors to lcore 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0  
 RX packets: 2067782 bytes:511158595 errors:0  
 TX packets:2222204 bytes:654123820 errors:0  
 Drops:1037474  
 TX port packets:2228775 errors:20  
 TX device packets:4545746 bytes:920251684 errors:0

This is the expected situation. It means no packet has been dropped inside the vrouter.

On a receiving VM vif, TX port and TX packets should also have the same value :

vif0/10 PMD: tap14cebe1c-c5  
 Type:Virtual HWaddr:00:00:5e:00:01:00 IPaddr:172.20.10.20  
 Vrf:2 Mcast Vrf:2 Flags:L3L2DEr QOS:-1 Ref:19  
 RX queue errors to lcore 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0  
 RX packets:0 bytes:0 errors:0  
 TX packets: 4665 bytes:196158 errors:0  
 ISID: 0 Bmac: 02:14:ce:be:1c:c5  
 Drops:0  
 TX port packets: 1105 errors: 3560 syscalls: 1105

Here 4665 packets have been processed by the "forwarding core", but only 1105 have been sent to VM interface, 3560 where errored.

We can also take note that 1105 "syscalls" notifications have been raised (1 per packet sent to the VM) which shows this instance is not a DPDK one.

This is an **unexpected** situation. It shows the virtual instance was not able to process all incoming packets in its vif queues and some of them have been dropped.

### Packet flow from a VM NIC to compute node Physical NIC - counters placement

Compute physical vif is always defined as vif0/0 into the vrouter. vNIC vif are defined as vif0/N (with N above or equal 3).

From virtual instances to underlay, packets are processed into 3 differents steps :

* vif0/n packet polling by a polling core
* vif0/n packet processing by a forwarding core
* vif0/0 packet delivery by a forwarding core

![Packet flow from a VM NIC to compute node Physical NIC - counters placement](data:image/png;base64;base64,)

**Packet flow from a VM NIC to compute node Physical NIC - counters placement**

Here on a transmitting VM vif, RX port and RX packets have the same value :

vif0/11 PMD: tapb2767cbd-40  
 Type:Virtual HWaddr:00:00:5e:00:01:00 IPaddr:194.3.0.8  
 Vrf:5 Mcast Vrf:5 Flags:L2Er QOS:-1 Ref:17  
 RX port packets: [red]#1433409# errors:0 syscalls:2  
 RX queue packets:516225 errors:0  
 RX queue errors to lcore 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0  
 RX packets: [red]#1433409# bytes:191289533 errors:0  
 TX packets:1544574 bytes:374354192 errors:0  
 ISID: 0 Bmac: 02:00:00:01:fd:01  
 Drops:673575  
 TX port packets:1544236 errors:338 syscalls:1450386

This is the **expected** situation. It means no packet has been dropped inside the vrouter.

### Traffic Load balancing on forwarding cores

A tool for getting statistics per core pps, bw utilisation that can be used for monitoring or testing performance purpose:

<https://github.com/PrzemekGrygiel/DPDKstats>

This tool is using vif RX and TX packets counters (packet received and transmitted by forwarding cores).

In order to check traffic is well balanced on all forwarding cores for a given interface, we have to use following command:

./dpdkvifstats.py -v <N>

with **<N>**, interface number to be checked.

**For instance:**

$ ./dpdkvifstats.py -v 3

![image](data:image/png;base64;base64,)

Here we can see that the traffic is well balanced on all cores for vif 0/3. Whatever the direction (vrouter to vif 0/3 = TX pps or vif0/3 to vrouter = RX pps), whatever the core, each core is processing around 500KPPS.

### vrouter is dropping packets

When drops are occurring inside the vrouter, it can be checked into "RX queue errors” counter or “IF Drop" in drop statistics option.

$ vif --get 3 --get-drop-stats | grep "IF Drop“  
IF Drop 325686650  
  
$ vif --get 3 --get-drop-stats | grep "RX queue packets“  
RX queue packets:73891601519 errors: 325686650

This value also matches RX Ports packets – RX Packets value:

$ vif --get 3 --get-drop-stats | grep "RX packets"  
RX packets:73891746924 bytes:4433501752754 errors:0  
  
$ vif --get 3 --get-drop-stats | grep "RX port"  
RX port packets:74217433574 errors:0 syscalls:1

![vrouter is dropping packets](data:image/png;base64;base64,)

**vrouter is dropping packets**

This is a situation that is occuring when too many packets are sent onto one or more processing cores. It means :

* traffic is not equally load balanced on all forwarding cores
* or not enough all forwarding cores have been allocated to the vrouter to be able to process the incoming traffic.

We can check on which forwarding core the drops have been occured using following command:

$ vif --get <interface> --core <forwarding core> | grep "RX queue errors"

For instance:

$ vif --get 3 --core 11 | grep "RX queue errors"  
RX queue errors to lcore 0 0 0 0 0 0 0 0 0 0 27283689 0 7534963 9294274 6851459 5748667

* **xxx**: forwarding core which drops packets
* **xxx**: polling cores whose packets have been dropped

Currently (19.12 release with an optimal setup), a forwarding core is able to process around 500 KPPS in each direction (RX and TX), so 1 MPPS in total for 64 bytes packets.

### virtual instance is dropping packets

When drops are occurring because a virtual instance is not fast enough to process incoming packet, it can be detected using TX port errors counters :

$ vif --get 10 | grep "TX port \|TX packets"  
TX packets:4665 bytes:196158 errors:0  
TX port packets: [red]#1105# errors: [red]#3560# syscalls: [red]#1105#

Here we are detecting that 3560 packets have been dropped on TX port. It means VM was to slow to process incoming packets. Some of them have been dropped into the virtio queues.

### Packet Drop statistics

With dropstats command we can get details about drops performed by the vrouter.

We can get all parameters supported by this command using :

$ dropstats --help

When some packet loss issue is encountered, this is a good starting point to get an overview of all drops that have been performed on the vrouter.

dropstats command run without any arguments is returning drop statistics for all vrouter cores :

$ dropstats

In order to get statistics for a given vrouter core, we can use the --core option. Keep in mind that 10 is the first processing vrouter lcore:

$ dropstats --core 10

In order to clear stats counters on all cores we can use this command :

$ dropstats --clear

Example:

$ (vrouter-agent-dpdk)[root@overcloud-contraildpdk-1 /]$ dropstats  
Invalid IF 0  
Trap No IF 0  
IF TX Discard 0  
IF Drop 0  
IF RX Discard 0  
  
Flow Unusable 0  
Flow No Memory 0  
Flow Table Full 0  
Flow NAT no rflow 0  
Flow Action Drop 0  
Flow Action Invalid 0  
Flow Invalid Protocol 0  
Flow Queue Limit Exceeded 0  
New Flow Drops 0  
Flow Unusable (Eviction) 0  
  
Original Packet Trapped 0  
  
Discards 0  
TTL Exceeded 0  
Mcast Clone Fail 0  
Cloned Original 0  
  
Invalid NH 27  
Invalid Label 0  
Invalid Protocol 0  
Etree Leaf to Leaf 0  
Bmac/ISID Mismatch 0  
Rewrite Fail 0  
Invalid Mcast Source 0  
Packet Loop 0  
  
Push Fails 0  
Pull Fails 0  
Duplicated 0  
Head Alloc Fails 0  
PCOW fails 0  
Invalid Packets 0  
  
Misc 0  
Nowhere to go 0  
Checksum errors 0  
No Fmd 0  
Invalid VNID 0  
Fragment errors 0  
Invalid Source 0  
Jumbo Mcast Pkt with DF Bit 0  
No L2 Route 0  
Memory Failures 0  
Fragment Queueing Failures 0  
No Encrypt Path Failures 0  
  
VLAN fwd intf failed TX 0  
VLAN fwd intf failed enq 0

**dropstats ARP Block**

|  |  |
| --- | --- |
| **GARP** | GARP packets from VMs are dropped by vrouter.This is an expected behavior. This counter indicates how many GARP packets were dropped. |
| **ARP notme** | this counter is incremented when ARP requests that are not handled by vrouter are dropped. For example, requests for a system that is not a host. These drops are counted by counters. |
| **Invalid ARPs** | this counter is incremented when the Ethernet protocol is ARP, but the ARP operation was neither a request nor a response. |

**dropstats Interface Block**

|  |  |
| --- | --- |
| **Invalid IF** | this counter is incremented normally during transient conditions, and should not be a concern. |
| **Trap No IF** | this counter is incremented when vrouter is not able to find the interface to trap the packets to vrouter agent, and should not happen in a working system |
| **IF TX Discard and IF RX Discard** | these counters are incremented when vrouter is not in a state to transmit and receive packets, and typically happens when vrouter goes through a reset state or when the module is unloaded. |
| **IF Drop** | this counter indicates packets that are dropped in the interface layer. The increase can typically happen when interface settings are wrong or vrouter was not powerful enough to process all incoming packets. |

**dropstats Flow Block**

|  |  |
| --- | --- |
| **Flow unusable counter** | When packets go through flow processing, the first packet in a flow is cached and the vrouter agent is notified so it can take actions on the packet according to the policies configured. If more packets arrive after the first packet but before the agent makes a decision on the first packet, then those new packets are dropped. The dropped packets are tracked by this counter |
| **Flow No Memory** | this counter increments when the flow block doesn’t have enough memory to perform internal operations. The Flow Table Full counter increments when the vrouter cannot install a new flow due to lack of available slots. A particular flow can only go in certain slots, and if all those slots are occupied, packets are dropped. It is possible that the flow table is not full, but the counter might increment. |
| **Flow NAT no rflow** | this counter tracks packets that are dropped when there is no reverse flow associated with a forward flow that had action set as NAT. For NAT, the vrouter needs both forward and reverse flows to be set properly. If they are not set, packets are dropped. |
| **Flow Action Drop** | this counter tracks packets that are dropped due to policies that prohibit a flow. |
| **Flow Action Invalid counter** | this counter usually does not increment in the normal course of time, and can be ignored. |
| **Flow Invalid Protocol** | this counter usually does not increment in the normal course of time, and can be ignored. |
| **Flow Queue Limit Exceeded** | More than three packets received before flow processing is completed. This counter usually does not increment in the normal course of time, and can be ignored. |

**dropstats Miscellaneous Operational Block**

|  |  |
| --- | --- |
| **Discard** | this counter tracks packets that hit a discard next hop. For various reasons interpreted by the agent and during some transient conditions, a route can point to a discard next hop. When packets hit that route, they are dropped. |
| **TTL Exceeded** | this counter increments when the MPLS time-to-live goes to zero. |
| **Mcast Clone Fail** | it happens when the vrouter is not able to replicate a packet for flooding. |
| **Cloned Original** | Original packet is dropped, after action is taken on cloned packet. This is an internal tracking counter. **It is harmless and can be ignored.** |
| **Invalid NH** | this counter tracks the number of packets that hit a next hop that was not in a state to be used (usually in transient conditions) or a next hop that was not expected, or no next hops when there was a next hop expected. Such increments happen rarely, and **should not continuously increment.** |
| **Invalid Label** | this counter tracks packets with an MPLS label unusable by vrouter because the value is not in the expected range. |
| **Invalid Protocol** | typically increments when the IP header is corrupt. |
| **Rewrite Fail** | this counter tracks the number of times vrouter was not able to write next hop rewrite data to the packet. |
| **Invalid Mcast Source** | this counter tracks the multicast packets that came from an unknown or unexpected source and thus were dropped. |
| **Invalid Source** | this counter tracks the number of packets that came from an invalid or unexpected source and thus were dropped (RPF check on the packet failed). |

**Other counters (mainly intended for developers)**

|  |  |
| --- | --- |
| **Push Fails** | Increasing the length of buffer failed |
| **Pull Fails** | Decreasing the length of buffer failed |
| **Duplicated** | Trap packet to Agent has been truncated and original packet is dropped |
| **PCOW fails** | Cloning and copying of buffer failed |
| **Invalid Packets** | Format of the received packet is Invalid |
| **Misc** | Packet dropped for miscellaneous reasons |
| **Nowhere to go** | Packet dropped because intended L3 or L2 processing failed |
| **Checksum errors** | Packet dropped because of Checksum failure |
| **No Fmd** | No forwarding metadata to process the packet |
| **Invalid VNID** | Wrong VNI/Vxlan Id received in the packet |
| **Fragment errors** | Enqueueing to fragment queue failed |
| **Jumbo Mcast Pkt with DF Bit** | Multicast packet more than MTU size is received |
| **No L2 Route** | L2 route is missing |

### vif command: get-drop-stats option

In order to get drops statistics generated on a given vrouter interface we can use this command :

$ vif --get --get-drop-stats

Adding --core option we can get these statistics for a given vrouter lcore :

$ vif --get --get-drop-stats --core

As for dropstats command, let’s keep in mind that 10 is the first processing vrouter lcore:

Example:

$ vif --get 0 --get-drop-stats  
Vrouter Interface Table  
  
Flags: P=Policy, X=Cross Connect, S=Service Chain, Mr=Receive Mirror  
 Mt=Transmit Mirror, Tc=Transmit Checksum Offload, L3=Layer 3, L2=Layer 2  
 D=DHCP, Vp=Vhost Physical, Pr=Promiscuous, Vnt=Native Vlan Tagged  
 Mnp=No MAC Proxy, Dpdk=DPDK PMD Interface, Rfl=Receive Filtering Offload, Mon=Interface is Monitored  
 Uuf=Unknown Unicast Flood, Vof=VLAN insert/strip offload, Df=Drop New Flows, L=MAC Learning Enabled  
 Proxy=MAC Requests Proxied Always, Er=Etree Root, Mn=Mirror without Vlan Tag, Ig=Igmp Trap Enabled  
  
vif0/0 PCI: 0000:00:04.0 (Speed 1000, Duplex 1)  
 Type:Physical HWaddr:52:54:00:f2:9f:f6 IPaddr:0.0.0.0  
 Vrf:0 Mcast Vrf:65535 Flags:L3L2 QOS:0 Ref:20  
 RX device packets:1021114 bytes:0 errors:0  
 RX port packets:1021114 errors:0  
 RX queue errors to lcore 0 0 0 0 0 0 0 0 0 0 0  
 RX packets:1021114 bytes:157010437 errors:0  
 TX packets:1063497 bytes:690713560 errors:0  
 Drops:0  
 TX queue packets:104822 errors:0  
 TX port packets:1063497 errors:0  
 TX device packets:1063497 bytes:0 errors:0  
  
Invalid IF 0  
Trap No IF 0  
IF TX Discard 0  
IF Drop 0  
IF RX Discard 0  
...

### Dropstats and packet drop log utility

Packet Drop log utility is an extension of dropstats command (available since Contrail 5.0) which logs drop packet information like: timestamp, drop reason, vif\_index, nexthop id, packet type, source IP, destination IP, source port, destination port, packet length, packet data, filename and line number.

Packet drop log utility is enabled by default with minimum logging (log only timestamp, drop reason, file name and line number).

In further release, IP source and destination will be added to this minimum logging information.

**vrouter kernel version.**

Packet drop log can be enabled/disabled and its buffer size can be changed during load time by setting some options in /etc/modprobe.d/vrouter.conf:

options vrouter vr\_pkt\_droplog\_bufsz=<value>  
options vrouter vr\_pkt\_droplog\_buf\_en=1

Packet drop log and minimum logging feature during can be enabled/disabled during runtime using following command:

$ echo 1 > /proc/sys/net/vrouter/pkt\_drop\_log\_enable  
$ echo 1 > /proc/sys/net/vrouter/pkt\_drop\_log\_min\_enable

**vrouter DPDK version.**

Currently neither vrouter vr\_pkt\_droplog\_buf\_en nor vr\_pkt\_droplog\_bufsz parameters can be modified when using a DPDK vrouter version. This is also not possible to disable packet drop log nor minimum logging feature on a dpdk vrouter.

The defined buffer size is the number of entries available for each processing lcore. The default value is set to 200 entries. On a DPDK vrouter which is using 4 lcore, we can collect up to 4x200 = 800 dropped packets

**Command**:

5.1 release:

$ dropstat -log 0

display log packet drops for all cores.

$ dropstats -log <core number>

display log packet drops for the given core.

Full log table is displayed by this command, so empty lines have to be filtered out:

\_sl no: 0 Epoch Time: 0 Local Time: Thu Jan 1 00:00:00 1970\_  
\_Packet Type: 0 Drop reason: NULL Vif idx: 0 Nexthop id: 0 Src IP: NULL Dst IP: NULL Source port: 0 Dest port: 0 file: NULL line no: 0 Packet Length: 0 Packet Data:\_

It can be done using a filter onto the Drop reason :

(vrouter-agent-dpdk)[root@overcloud-contraildpdk-1 /]$ dropstats -l 0 | grep -C3 INVALID\_NH | head -n 8  
Pkt Drop Log for Core 11  
sl no: 0 Epoch Time: 1569247326 Local Time: Mon Sep 23 14:02:06 2019  
Packet Type: 0 Drop reason: VP\_DROP\_INVALID\_NH Vif idx: 0 Nexthop id: 0 Src IP: NULL Dst IP: NULL Source port: 0 Dest port: 0 file: VR\_NEXTHOP\_C line no: 2656 Packet Length: 0 Packet Data:  
sl no: 1 Epoch Time: 1569247326 Local Time: Mon Sep 23 14:02:06 2019  
Packet Type: 0 Drop reason: VP\_DROP\_INVALID\_NH Vif idx: 0 Nexthop id: 0 Src IP: NULL Dst IP: NULL Source port: 0 Dest port: 0 file: VR\_NEXTHOP\_C line no: 2656 Packet Length: 0 Packet Data:

**19.7 release and above:.**

$ dropstat --log 0

display log packet drops for all cores.

$ dropstats --log <core number>

display log packet drops for the given core.

with --log option, the lcore number to be given is the real coreID + 1.

**Workaround - How to disable minimum logging feature on Contrail DPDK vrouter** :

Currently there is no simple way to disable minimum logging feature onto a Contrail DPDK vrouter.

In this section we are describing a workaround that could be used onto some development environment in order to collect full packet drop logs onto Contrail DPDK vrouter. **This workaround must not be used onto a production environment**.

1. download contrail-debug container from the Juniper Docker Hub:

* $ sudo docker pull hub.juniper.net/contrail-debug:<tag>
* <tag> is depending on the release used, 5.1.0-0.38-rhel-queens for instance.

1. copy contrail-vrouter-dpdk.debug fileinside DPDK container at /usr/bin

* $ sudo -i  
  # cd /var/lib/docker/overlay2  
  # find . -name contrail-vrouter-agent.debug  
  # find . -name contrail-vrouter-dpdk.debug
* Keep note the path of the last command :
* # docker cp \_\_<contrail-vrouter-dpdk.debug path>/\_\_contrail-vrouter-dpdk.debug `<contrail-vrouter-dpdk name or ID>`:/usr/bin
* Here for instance, our dpdk vrouter agent container name is contrail-vrouter-agent-dpdk and its ID: 3920ca0aac69
* # docker ps | grep vrouter | grep dpdk  
  3920ca0aac69 192.168.24.1:8787/contrail/contrail-vrouter-agent-dpdk:1909.30-rhel-queens "/entrypoint.sh /u..." 7 hours ago Up 14 minutes contrail-vrouter-agent-dpdk

1. run gdb on to contrail vrouter dpdk binary

* # docker exec -it `<contrail-vrouter-dpdk name or ID>` bash  
  (container)# ps -eaf | grep contrail-vrouter-dpdk
* Keep note the process ID: <DPDK PID>
* (container)# gdb /usr/bin/contrail-vrouter-dpdk
* GDB will load both contrail-vrouter-dpdk and contrail-vrouter-dpdk.debug binary files.

1. attach to the current running dpdk process

* (gdb) attach <DPDK PID>

1. Print and update the variable vr\_pkt\_droplog\_min\_sysctl\_en

* (gdb) p vr\_pkt\_droplog\_min\_sysctl\_en  
  (gdb) set vr\_pkt\_droplog\_min\_sysctl\_en=0

## Faulty vrouter deployment troubleshooting

Some typical root cause of a faulty OpenStack contrail deployment failure is a network misconfiguration onto compute nodes. Openstack is using os-net-config to perform network configuration onto network hosts.

*os-net-config* CLI is using YAML or JSON file formats. By default os-net-config uses a YAML config file located at /etc/os-net-config/config.yaml. It can be customized via the --config-file CLI option.

Providers are used to apply the desired configuration on the host system. By default 3 providers are implemented:

* Ifcfg: persistent network config format stored in /etc/sysconfig/network-scripts
* ENI: persistent network config format stored in /etc/network/interfaces
* iproute2: non-persistent provider which implements the config using iproute2, vconfig, etc…​

When using bin/os-net-config the provider is automatically selected based on the host systems preferred persistent network type (ifcfg or ENI). This can be customized via the --provider CLI option.

When vrouter is failing to start onto a compute node we have first to check the configuration that has been tried to be applied by the deployment tool (Ansible, TripleO for instance). It can be checked using the following command :

$ cat /etc/os-net-config/config.json | jq.

vhost0 (vrouter main interface) activation failure can be checked with the following one:

$ sudo journalctl -u os-collect-config

os-net-config CLI tools can also be run manually in order to try to find the root cause of a faulty vrouter deployment. For instance following command can be launched onto a faulty compute node :

$ sudo os-net-config –c /etc/os-net-config/config.json

Contrail vrouter logs have also to be checked. For a DPDK vrouter it can be checked into /var/log/contrail/contrail-vrouter-dpdk.log (up to 4.1) or /var/log/containers/contrail/contrail-vrouter-dpdk.log (from 5.0 and above).

$ cat /var/log/containers/contrail/contrail-vrouter-dpdk.log

When DPDK is used, it’s also important to check that some DPDK interfaces are available to be used by the vrouter. It can be checked with :

$ sudo /opt/contrail/bin/dpdk\_nic\_bind.py -s

# misc/backup content/changes

## CPU assignment and isolation mechanisms

Isolation and assignment are two complementary mechanisms:

* CPU isolation restricts the set of CPUs that are available for Operating System Scheduler level. When a CPU is isolated, no task will be scheduled on it by the Operating System. An explicit task assignment must be done.
* CPU assignment is called processor affinity, or CPU pinning.It enables the binding and unbinding of process or a thread onto a CPU. It is an opposite mechanism that consists in defining a limited set of CPUs that are allowed to be used by: o the OS Scheduler. Operating System CPU affinity is managed through systemd. o a specific process: using CPU pinning rules (taskset command for instance)

RedHat operating systems Tasks to be run by an operating system must be spread across available CPUs. These tasks into a multi-threading environment are often made of several processes which are also made of several threads. In order to run all these processes and threads on the CPU offered by the node, the Operating System is using a scheduler to place each single one onto a given CPU. There are two styles of scheduling, cooperative and preemptive. By default, RedHat Linux is using a cooperative mode. Cf: <https://medium.com/traveloka-engineering/cooperative-vs-preemptive-a-quest-to-maximize-concurrency-power-3b10c5a920fe>

In order to get a CPU booked for a subset of tasks, we have to inform the Operating System scheduler not to use these CPUs for all the tasks it has to run. These CPUs are told: “isolated” because they are no more used to process all tasks. In order to get a CPU isolated several mechanisms can be used: • remove this CPU from the “common” CPU list used to process all tasks • change the scheduling algorithm (cooperative to preemptive) • participate or not to interrupt processing

RedHat Linux is currently supporting 2 different CPU isolation methods. They are isolcpus and tuned CPU partitioning, They can be used either independently or simultaneously.

A first method, isolcpus kernel parameter, has been proposed to keep CPUs away from linux scheduler. This isolation mechanism will: • remove isolated CPUs from the “common” CPU list used to process all tasks • change the scheduling algorithm from cooperative to preemptive • perform CPU isolation at the system boot The main drawbacks of using isolcpus are : • it requires manual placement of processes on isolated cpus. • it is not possible to rearrange the CPU isolation rules after the system startup • it is not possible to move process from one isolated cpu to another. A second method, tuned CPU partitioning, has been proposed more recently on RedHat Operating Systems. This program enables to manage both CPU isolations and assignment rules. It used systemd CPUAffinity proposed on Linux systems to manage OS CPU affinity and enriches the Kernel isolation method with a new mechanism managed by systemd.

Isolation and Affinity rules are configured in a different locations: • CPUAffinity parameter in /etc/systemd/system.conf; restricts all processes spawned by systemd to the list of cores. Note that from RHEL 7.5, CPUAffinity is natively integrated in tuned’s cpu-partitioning profile (more information on this topic is provided later in this section). • isolated\_cores parameter in /etc/tuned/cpu-partitioning-variables.conf, is removing a set of CPU from the “common” CPU list used to process all tasks

Following tasks can be managed with tuned program: • removes isolated CPUs from the “common” CPU list used to process all tasks • performs CPU isolation after the system boot using systemd. • All container processes follow systemd CPUAffinity configured with Tuned CPU partitioning.

Tuned program is also managed by systemd as a service. $ sudo systemctl status tuned ● tuned.service - Dynamic System Tuning Daemon Loaded: loaded (/usr/lib/systemd/system/tuned.service; enabled; vendor preset: enabled) Active: active (running) since Thu 2020-05-28 04:38:06 CEST; 10h ago

Tuned configuration is enforced at system startup by systemd. The main drawbacks of using tuned partitioning are : • Some processes are started at the system boot before systemd is started. These processes are run before isolation rules are enforced and could break expected isolation rules. • Scheduling Algorithm is kept to cooperative mode which provides a lower isolation. In few words, tuned partitioning is more flexible and featureful than isolcpus, but is providing a lower CPU isolation. This is why both mechanisms are often used altogether to enforce CPU isolation.

IMPORTANT NOTE: if both tuned CPU partitioning profiles and isolcpus mechanisms are used be careful to be consistent. in the defined setup.

Ubuntu operating systems Ubuntu operating systems are supporting isolcpus kernel parameters and systemd CPU Affinity mechanisms. CPU partitioning profile, which is RedHat specific, is not supported. When we are deploying Contrail on Ubuntu Operating Systems (that use OCI runc for container instantiation) we have also to isolate processes running in these Containers. This is because in Ubuntu Operating System architecture containerd-shim child processes do not have CPUAffinity set according to the host OS configuration (/etc/systemd/system.conf CPUAffinity or kernel isolcpus). So we need to isolate these processes too. It can be achieved natively with docker using the ‘cpuset’ configuration in the relevant docker-compose YAML file. If juju is used for deployment: ‘cpuset’ will be configured for the relevant containers according to ‘dpdk-ctrl-thread-coremask’ in the contrail-agent charm.

Best regards, Laurent DURAND

## References

* <https://developers.redhat.com/blog/2017/06/28/ovs-dpdk-parameters-dealing-with-multi-numa/>
* <https://doc.dpdk.org/guides/linux_gsg/nic_perf_intel_platform.html>
* <https://software.intel.com/en-us/articles/dpdk-performance-optimization-guidelines-white-paper>
* <https://doc.dpdk.org/guides/prog_guide/env_abstraction_layer.html>

**Some reference about the kernel args**:

* <https://access.redhat.com/articles/3720611>
* <https://access.redhat.com/documentation/en-us/red_hat_enterprise_linux_for_real_time/7/html-single/tuning_guide/index#Isolating_CPUs_Using_tuned-profiles-realtime>
* <https://codilime.com/how-can-dpdk-access-devices-from-user-space/> (great)